연구보고서

시설공사 내역서 표준화 및 간소화

방안에 관한 연구

2004.  9

연구수행기관 : (사)한국구매조달학회

연구책임자 : 충남대학교  유 성 연

조    달    청

제   출   문

본 보고서를 “시설공사 내역서 표준화 및 간소화 방안에 관한 연구” 용역의 최종보고서로 제출합니다.

20004. 9.

연구수행기관 : (사)한국구매조달학회

연구책임자 : 충남대학교  유 성 연

조    달    청

목 차
1. 1) 2) 3)	서 론 연구목적 연구방법 시설공사 내역서 관련 규정
2. 1) 2) 3) 4) 5)	국내․외 건설공사 내역서 작성 사례조사 및 비교 분석 국 내 미 국 유 럽 일 본 각국의 내역서 작성 사례 비교 분석
3. 1) 2) 3) 가) 나) 다) 라) 마) 4)	표준화 및 간소화 방안 연구 내역서 양식의 표준화 공종분류의 표준화 내역서 표준화 및 간소화 방안 부속자재를 주자재의 공사비 비율로 표기 일위대가화 단위 변경 중공종별 내역서 작성 기타 내역서 표준화 및 간소화 업무처리 절차
4.	표준화 내역서 작성 결과 분석
5.	기대효과
6.	문제점 및 대책
7.	결 론
	참고문헌
	부 록

표  목  차

표 2-1  2004년도 실적 단가집(7월 발표)

표 2-2  표준품셈(강관배관의 부자재 산정요율)

표 2-3  부속자재 비율

표 2-4  전선관 부속품률

표 2-5  Pipe Works 내역서

표 2-6  Steel Works 내역서

표 2-7  Pipe and Pipe Fittings 내역서

표 2-8  콘크리트공사 내역서

표 2-9  각 국의 내역서 작성방법 비교

표 3-1  표준화 내역서 양식

표 3-2  건축공사 표준시방서에 의한 공종 분류

표 3-3  건축기계설비 공사 표준시방서에 의한 공종 분류

표 3-4 기계설비․플랜트설비공사 수량산출기준지침서에 의한 공종 분류

표 3-5-1  배관재의 경우(변경 전)

표 3-5-2  배관재의 경우(변경 후)

표 3-6-1  보온재의 경우(변경 전 - 고무발포재)

표 3-6-2  보온재의 경우(변경 후 - 고무발포재)

표 3-7-1  철골의 경우(변경 전)

표 3-7-2  철골의 경우(변경 후)

표 3-8-1  가설전기, 가설용수의 경우(변경 전)

표 3-8-2  가설전기, 가설용수의 경우(변경 후)

표 3-9-1  연도의 경우(변경 전)

표 3-9-2  연도의 경우(변경 후)

표 3-10-1  배관재의 경우(변경 전)

표 3-10-2  배관재의 경우(변경 후)

표 3-11-1  덕트 기구 취부(변경 전)

표 3-11-2  덕트 기구 취부(변경 후)

표 3-12    합판 거푸집, 철근 구조물 콘크리트 펌프차 타설

표 3-13-1  석 공사(화강석 판(바닥) - 변경 전)

표 3-13-2  석 공사(화강석 판(바닥) - 변경 후)

표 3-14-1  타일 공사(압착 및 밀착 공법(바닥) - 변경 전)

표 3-14-2  타일 공사(압착 및 밀착 공법(바닥) - 변경 후)

표 3-15-1  덕트 부속(Sound Chamber - 변경 전)

표 3-15-2  덕트 부속(Sound Chamber - 변경 후)

표 3-16-1  덕트 부속(Damper - 변경 전)

표 3-16-2  덕트 부속(Damper - 변경 후)

표 3-17-1  덕트 부속(Register - 변경 전)

표 3-17-2  덕트 부속(Register - 변경 후)

표 3-18-1  창호류(변경 전)

표 3-18-2  창호류(변경 후)

표 3-19    공종별 집계표

표 3-20    단계별 작성 서류

표 3-21    내역서 표준화 및 간소화 업무처리 절차

표 4-1     표준화 내역서 적용 시 간소화율

표 4-2-1   건축공사 감소율 대안(변경 전)

표 4-2-2   건축공사 감소율 대안(변경 후)

1. 서 론

우리가 사는 지구에는 많은 건축물들이 있지만 그 형태 및 구조들이 독창성을

가진 것을 볼 수 있다. 이런 독창적인 건축물이 탄생하기 위하여는 공사의 규모를

떠나 일련의 Cycle이 있다. 건설공사의 Life cycle을 보면, 타당성 검토를 거친 후

프로젝트가 기획되어 설계․시공을 거쳐 유지관리를 하는 프로세스를 가진다고 할 수 있다.

경제발전의 원동력이 되는 건설 산업은 국가 기간산업이다.

건설 프로젝트가 원활하게 진행되려면 예산(Budget), 조직(Organization), 기술력(Engineering)의 3부문이 균형을 이루어야 된다.

1) 연구 목적

공사수행을 위한 주요 서류 중 하나가 내역서라고 할 수 있다. 내역서는 수량산출서에 의해 집계된 공종별 품명에 대한 내용을 정해진 양식에 표현하는 서류다. 또한 품명은 재료비, 노무비, 경비 등으로 구분되어 단가 및 금액이 결정되어진다. 하지만 내역서를 기술하다 보면 금액에 비하여 품목수가 많고 중요도가 적은 부분이 있다. 따라서 업무처리를 효율화하기 위하여 내역서 작성 방법에 대한 연구가 필요하게 되었다. 설계도서에 공간개념을 도입하여 수량을 산출하고 현장특성을 감안하여 할인․할증률을 적용하여 수량산출서를 작성한다. 수량산출서를 공종별로 집계하여 집계표를 만들고 집계된 물량을 표준화된 양식에 넣어 내역서를 작성한다. 이렇게 작성된 직접재료비, 직접노무비, 경비에 일정한 간접비율을 적용하여 원가계산서를 작성한다. 충실한 내역서 작성은 공사의 품질관리 및 공정관리를 원활하게 할 수 있는 근간이 된다. 공사의 혼란을 초래하지 않으며 업무의 효율화를 기할 수 있는 내역서 작성이 필요하게 되었다. 여기에는 반드시 객관성 확보가 전제되어야 한다.

2) 연구방법

본 연구에서는 먼저 선진국의 사례를 조사․분석하고, 국내에서 사용되는 내역서의 형태들에 대한 사례를 조사하며, 연구기간 동안 관련분야 전문가 간담회를 통하여 의견수렴을 하고 객관성 확보에 노력한다. 이런 과정을 통하여 표준화된 내역서 양식을 만들고 내역서 작성을 간소화하는 틀을 마련하기로 한다.  아울러 본 연구에서는 다음과 같은 중점 고려사항을 가지고 연구 용역을 수행하였다.

① 안정성

만약 독자적으로 내역서를 구축해 이것을 사용 중이라면 현재 사용 중인 내역

서를 변경하기 위해서는 많은 시간과 노력이 필요하다. 또한 많은 투자를 하여  변경한 내역서가 전보다 불편하고 익숙하지 않을 수 있다. 이러한 문제를 해결하기 위해서는 내역서가 가지고 있는 기본적인 원리와 개념을 사용자가 쉽게 이해할 수 있는 구조로 되어야 한다. 다른 내역서와의 호환이 가능하여 다른 내역서를

수용할 수 있을 만큼 포괄적인 내용을 가지고 있어야 한다. 이것이 곧 안정성이라고 할 수 있으며 안정성은 내역서에 반드시 필요한 특성이라고 할 수 있다.

② 컴퓨터 시스템에 대한 적용성

건설공사에서 발생되는 데이터들은 아주 다양하고 여러 가지 형태를 가지고 있다. 한번 만들어진 데이터는 다음 단계에서 재사용되고 대부분의 데이터들은 프로젝트가 진행함에 따라 발전하고 변화되므로 컴퓨터 시스템에 적용이 쉬워야 한다.

③ 함축성

내역서 작성 방법은 축약되어 있으면서도 가능한 많은 사항을 표현할 수 있어야 한다.

④ 객관성

내역서 작성 방법은 객관화되어야 하고, 품명은 함축되어야 하며 이해하기 쉬워야한다. 내역서는 건설공사의 성격을 파악하는 중요한 서류이다. 내역서 간소화를 통하여 공사의 특성을 알 수 없을 정도로 함축된다면 간소화에 대한 의미는 퇴색된다.

3) 시설공사 내역서 관련 규정

- 국가를 당사자로 하는 계약에 관한 법률 시행령

제14조 (공사의 입찰)

공사를 입찰에 부치고자 할 때에는 설계서, 공종별 목적물 물량이 기재된 물량    내역서를 배부 또는 열람케 하여, 입찰자 또는 계약상대자가 정확한 공사비를     산출할 수 있도록 하여야 한다.

- 공사계약 일반조건

제2조 (정의) 이 조건에서 사용하는 용어의 정의는 다음과 같다.

4. “설계서”라 함은 공사시방서, 설계도면, 현장설명서를 말한다. 다만, 공      사 추정가격이 1억원 이상인 공사에 있어서는 공종별 목적물 물량이 표시된      내역서를 포함한다.

5. “공종별 목적물 물량 내역서”라 함은 공종별 목적물을 구성하는 품목 또      는 비목과 동품목 또는 비목의 규격․수량․단위 등이 표시되고, 시행령 제14조      제1항 및 제2항의 규정에 의하여 입찰공고 후 또는 낙찰자 결정 후 입찰에       참가하고자 하는 자 또는 낙찰자에게 교부된 내역서를 말한다.

6. “산출내역서”라 함은 발주기관이 교부한 물량 내역서에 입찰자 또는 계      약상대자가 단가를 기재하여 제출한 내역서

- 내역입찰 집행요령

제3조 (산출내역서의 작성․제출)

내역입찰을 실시 할 별지 제1호 서식에 단가 등 필요한 사항을 기입한 산출내     역서를 제출하게 하여야 한다. 이 경우 계약담당공무원은 건설교통부장관이      제정한 수량산출기준을 물량 내역서 작성의 기초자료로 할 수 있다.

이번 프로젝트에서는 여러 가지 사례를 조사하고 분석하여 획기적인 시스템을  창출하기 보다는 기존 시스템을 보다 편리하고 쉽게 적용하면서 축약될 수 있도록 하고, 추후 에는 실적공사비제도에 활용될 수 있도록 하겠다.

2. 국내․외 건설공사 내역서 작성 사례조사 및 비교 분석

현재 선진국에서는 우리보다 먼저 필요성을 느껴 내역서와 관련된 연구업무가 많이 진행되었고 이와 관련된 자료들이 많이 나와 있다. 우리 연구진은 선진국에서 적용되고 있는 내역서 작성 관련 자료를 수집하였고, 우리 시스템과 비교 검토하여 표준화된 양식을 만들고, 이를 분석하여 내역서 표준화 및 간소화 방안을 제시하고자 한다.

1) 국내

우리나라에서는 공사발주방법으로 전통적인 방법으로 설계․시공 분리 발주 방

법과 최근 대형프로젝트에 도입되고 있는 설계․시공일괄 발주방법이 있다. 설계․시공 분리발주 시 내역서 작성방법으로, 재료비․노무비․경비를 분리하는 방법과 합산하는 방법이 있다. 정부에서는 실적공사비에 의한 발주 환경조건을 조성하면서 공사비 산정 시 재료비․노무비․경비를 합산하여 내역서를 작성하는 방법을 추진하고 있다.

또한, 2004년도부터 공공기관에 의해 실적공사비에 의한 발주를 시도하려고 한다. 발표된 “2004년도 실적 단가집”[표 2-1] 자료를 분석해 보면 적용단가는 단순히 품명에 대한 재료비, 노무비, 경비의 단가를 합산한 것이다. 우리나라에서 발표된 “2004년도 실적 단가집” 자료를 분석하여 보면, 내역서 간소화하고는 거리가 있다.

[표 2-1]  2004년도 실적 단가집(7월 발표)

- 철근가공 및 조립

공종코드	공종명	규격	단위	적용단가	비고
DB00050	철근가공조립	보통	ton	352,928	일반건축
DB00010	철근가공조립	보통	ton	234,892	공동주택
DB00020	철근가공조립	복잡	ton	283,428	공동주택

【단가정의】

② 현장내 운반, 절단, 가공 및 조립비용을 포함하며, 현장도착도 운반비는 제외한다.

③ 버팀재(Bar chair, Bar support), 간격재(Bar spacer), 결속선(tying wire)등 부속자재의 조달 및 설치비용을 포함한다.

④ DB00010/ DB00020은 철근콘크리트(RC) 벽식구조 공동주택에 적용한다. DB00050은 일반건축(공동주택을 제외한 건축공사)에 적용한다.

- 강관

공종코드	공종명	규격	단위	적용단가	비고
BA28100	백강관 옥내일반배관	D80㎜	m	26,235
BB21100	백강관 옥내일반배관	D100㎜	m	36,390
BB23100	백강관 옥내일반배관	D150㎜	m	61,930

【단가정의】

② 먹줄치기, 상자넣기, 인서트, 지지철물설치, 절단, 나사 혹은 용접접합, 수압 또는 통기시험, 소운반비를 포함한다.

③ 상자넣기, 지지철물 재료비는 제외되어있다.

④ 재료할증 및 잡자재를 포함한다.

⑤ 부설배관의 터파기, 되메우기, 잔토처리 등은 별도 계상한다.

⑥ 관이음 부자재(엘보, 리듀서, 플랜지, 어댑터, 티 등)의 재료비는 별도 계상한다.

⑦ 이 단가는 공동주택에 적용한다.

기계설비공사 표준품셈[표 2-2]에서는 내역 간소화 방법의 일환으로 강관의 경우 건물 용도별(일반 업무용, 병원건물), 건물 규모별(소 : 연면적 5,000㎡이하, 중 : 5,000㎡초과 30,000㎡미만, 대 : 연면적 30,000㎡이상), 시공부위별(냉온수배관, 냉각수배관, 증기배관 등)로 관이음 부속, 관지지물에 대하여 주자재에 대한 비율로 상세하게 정의되어 있다. 하지만, 대다수의 발주처에서는 산정요율에 대한 객관성 확보가 되어 있지 않아 수량산출시 표준품셈에 의한 부자재 비율을 적용하지 않고 재래식 방법에 의하여 산출하고 있다.

[표 2-2] 표준품셈(강관배관의 부자재 산정요율)

가. 일반 업무용

(강관금액에 대한 %)

구 분	관이음 부속			관 지지물
건물규모 시공부위	소	중	대	소	중	대
가. 냉온수배관 - 기계실 - 옥내일반	75 45	70 45	65 45	30 40	15 25	15 25
나. 냉각수배관 - 기계실 - 옥내일반	75 70	75 55	75 40	7 9	7 9	7 9
다. 증기배관 - 기계실 - 옥내일반	75 45	65 45	50 45	30 30	30 30	30 30
라. 급수․급탕배관 - 기계실 - 옥내일반	80 60	80 60	80 60	15 15	15 15	15 15
마. 보일러급유배관	50	50	50	15	15	15
바. 통기배관	30	30	30	10	10	10
사. 소화배관 - 옥내소화전 - 스프링쿨러	65 70	55 70	50 70	10 15	10 15	10 15

【해 설】

① 관이음 부속류는 엘보, 티, 리듀서, 유니온, 소켓, 캡, 플러그, 니플, 부싱, 플랜지 등을 말한다.

② 관 지지물류는 클레비스행어, 보온용 클레비스행어, 파이프클램프, 롤러행어, 행어볼트, U-볼트, 파이프 앵커, 턴버클, 나비밴드 등을 말한다.

나. 표준화 및 간소화 내역서에서의 부속자재 비율 비교

[표 2-3] 부속자재 비율

구 분	관이음 부속 및 지지물(%)			비고
공사별 시공부위	○○대학병원	○○도로출입국	○○전자현미경
가. 기계실배관	54.9	44.4	34.2	STS관
나. 공조배관	47.7	28.6	45.4	STS관
다. 위생배관	58.6	40.3	32.5	동관
라. 소화배관	37.9	64.5	12.2	강관

다. 가, 나 항에서 관이음 부속 및 관지지물의 주자재에 부속자재의 공사비 비율    을 보면 표준품셈의 경우와 실제 수량산출서 적용 시 차이가 크다. 실무에서     적용하기에 부적절하다.  전기부문[표 2-4] 같이 주재료에 의한 부자재 비율을    자재별로 통일 할 수 있으면 좋겠지만 기계설비 부문은 공정에 따라 공사의      성격이 다르고 공사 규모에 따라 다르기 때문에 적용 할 수 있는 자료를 만들    기 위하여는 많은 연구가 필요 할 것 같다.

라. 상세한 내용은 #부록3 기계설비공사 관이음부속 및 지지물 부자재 비율을      참조한다.

[표 2-4] 전선관 부속품률

품 명	부속품률
박강 전선관, 후강 전선관, 합성수지 전선관, 금속가요전선관	15~20%
CD전선관	40%

2) 미 국

미국의 경우 내역서의 일부를 검토하여 보면 ○○ Project에서 A-2 배수배관에 사용되는 110mm Pipe의 경우 Rate는 249.5(지지, 부속자재 및 악세서리 포함), B-1 우수배관에 사용되는 경우 145.0(지지, 부속자재 및 악세서리 포함), F-1 배수배관에 사용되는 경우 113.3(연결 포함)으로 나타나 있다. 이것은 주자재에 대한 부속자재의 소요량에 대한 차이와 작업 위치 및 장소의 할증 등에서 오는 결과이다. 사각 덕트의 경우 지지류, 벤드 등의 부속자재를 포함하여 규격별로 길이에 의한 표기를 쓰고 있다.

[표 2-5] Pipe works 내역서

Ref	Description	Quantity	Units	Rate	Amount
A	Soil, waste and vent pipework.
	Soil, waste and vent pipework and fittings, complete
	with all necessary fixings, fittings and accessories
2	110 mm	28	Mtrs	249.5	6,986.0
3	80 mm dia	53	Mtrs	183.8	9,741.4
	Rainwater pipework
B	Rainwater pipework and fittings; complete with all
	necessary fixings, fittings and accessories
1	110 mm dia	35	Mtrs	145.0	5,075.0
F	Soil, waste and vent accessories, including jointing
	to pipework
1	110 mm	2	No	113.3	226.6
2	80 mm	2	No	113.3	226.6
	DUCTWORK Rectangular ductwork
E	Rectangular ductwork, including insulated supports, joints,
	fixings, bends, branches and associated accessories
1	Size 150 x 100	10	Mtrs	48.6	486.0
2	Size 150 x 150	19	Mtrs	58.3	1,107.7
3	Size 200 x 200	22	Mtrs	77.8	1,711.6

Hai Pong Project 내역서를 검토하여 보면 4. Steel works에서 1항의 경우 페인트가 된 주자재에 설치, 조립 등의 인건비와 볼트, 앵커볼트, 프레임 등을 포함(합성단가)하여 수량은 Ton으로 표기하였고, Unit Rate를 부문별(Materials, Labors, Other's, Total) 표기를 할 수 있도록 하였다. 첫 번째 Project는 청사의 경우이고 두 번째 Project는 Plant의 경우이다. 두 Project를 검토한 결과 Rate는 발주처의 의지,  Project의 성격에 따라 혼용됨을 알 수 있다.

[표 2-6]  Steel works 내역서

No.	Description	Specification	Unit	Q'ty	Unit Rate(US＄)				(US＄)
					Materials	Labors	Other's	Total	Amount
4	Steel works
1	Structural steel with paint	ASTM A36 or equivalent including erection/fabrication drawings, high strength friction bolt, anchor bolts and anchor ftame etc. as per Tender Specification Clause 3.5.8, Volume 3.	ton	1,940.0

3) 유 럽

유럽의 경우 적산분야의 선구자적인 역할을 하고 이 분야가 전문화되어 적산사 자격제도가 있다. Item Description를 최대한 활용하고 Fitting류의 표기도 Elbow, Tee, Reducer, Union, Flange, etc 등으로 가능한 명쾌하게 표기하였고 Unit Rate를 사용한다.

[표 2-7] Pipe and Pipe Fittings 내역서

ABU DHABI		BILL OF QUANTITIES			B/N.	PAGE NO.
TRADE CENTER		HOTEL TOWERS
ABU DHABI, U.A.E.		MECHANICAL SERVICES			5	5/12/02
ITEM	ITEM DESCRIPTION		Q'Y	UNIT	UNIT	TOTAL PRICE
REF.					RATE	UAE Dhms
	SECTION 15060 - HVAC PIPE AND PIPE FITTINGS
	Chilled water system piping complete with fittings including elbows, tees, reducers, unions, flanges and any other fittings required to make a complete system all as per specifications.
A.	25mm dia		30	m	2,058	61,756
B.	32mm dia		38	m	63.47	24,309
C.	40mm dia		44	m	32.97	1,451
D.	50mm dia		15	m	39.66	6,187

4) 일 본

일본의 경우 수량에 해당하는 단가(기기․재료 등의 단가, 복합단가, 시장단가, 합성단가)에 대한 정의를 하였고 내역서도 종목별, 과목별, 중과목별, 세목별로 구분하여 단계별로 작성 하도록 하였다. 정부주관(국토교통성)으로 표준화된 내역서 작성 방법 및 표준화 양식을 만들어 사용하고 있다.

[표 2-8]  콘크리트공사 내역서

명 칭	적 요	수량	단위	단가	금액	비 고
5. 콘크리트공사
(1) 구체
보통콘크리트	재질, 강도, slump, 기초부		㎥
보통콘크리트	재질, 강도, slump, 軸部		㎥
보통콘크리트	재질, 강도, slump, 土間		㎥
콘크리트타설			㎥			(별지명세)
펌프압송		1	식			(별지명세)

.

상세한 자료는 “부록1 국내․외 사례조사”에 서술되어 있다.

5) 각국의 내역서 작성사례 비교 분석

현재 선진국에서는 실적공사비 제도가 정착되어 있으며 설계․시공일괄 발주방법으로 추진되고 있다. 내역서를 보면 많은 부분이 서술식으로 작성된다.  발주처의 의지에 따라  내역서를 Material, Labor, Other's로 분리하여 내역서를 작성하는 방법이 혼용되고 있음을 알 수 있다.

Rate는 국가 또는 공인기관에서 표준화된 시스템을 발표하고 이 시스템을 응용하여 각 건설사가 적용하고 있다. Rate에 대한 요소는 다년간의 경험과 사례에 의하여 각 사별로 상이하다. 표준화된 시스템에 의한 내역서 작성은 발주처가 예산 등을 확보하고 집행하기 위한 것 이고, 이 시스템을 응용하여 건설사는 각 사별로 축적된 자료를 확보하고 있다. 이 데이터는 건설사의 Know-how로 입찰 등의 응찰에 사용된다. 내역서 작성 시 Description을 최대한 활용하고 있다. 동일한 재질의 동일한 규격의 품명일지라도 여러 요소에 의하여 Rate는 상이하다.

[표 2-9] 각 국의 내역서 작성 방법 비교

구 분	국 내	미 국	유 럽	일 본
품명 및 규격	간단히 작성	상세하게 작성	상세하게 작성	간단히 작성
단 가	재, 노, 경	Rate	Rate	품명별단가정의
주자재, 부자재	분리	포함	포함	포함
내역서	상세내역서	단계별내역서	단계별내역서	단계별내역서

3. 표준화 및 간소화 방안 연구

각국의 사례를 조사하여 분석하고 객관화 및 정형화 된 틀을 만들어 제안한다.

- 내역서 양식 및 내역서 양식에 사용되는 용어를 통일한다.

- 표준시방서에 제시된 공종분류 체계에 의하여 내역서 작업을 할 수 있도록       한다.

- 현재 표현하고 있는 방법(이하 “변경 전”)과 이번 연구에서 제안하고자 하      는 방법(이하 “변경 후”)을 대비하여 나타낸다.

1) 내역서 양식의 표준화

내역서 양식은 여러 형태로 사용되고 있으나 아래와 같은 형태를 제안하며 제안된 안의 좌측에 Code란을 우측에 비고란을 둘 수 있다.

[표 3-1] 표준화 내역서 양식

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액

2) 공종 분류의 표준화

가) 건축공사

건축공사 표준시방서 공종 분류에 따르며 [표 3-2]와 같다

[표 3-2] 건축공사 표준시방서에 의한 공종 분류

대 공 종	중 공 종	소 공 종
건축공사	공통공사	가설사무소, 비계, 동바리
	토공 및 기초공사	토공 및 흙막이, 기초
	철근콘크리트공사	레미콘 타설, 거푸집, 철근 가공조립
	철골공사	철골 가공조립, 내화피복
	벽돌 및 블록공사	벽돌쌓기, 블록쌓기
	석공사 및 타일 공사	석재판 붙이기, 타일 붙이기
	방수공사	아스팔트방수,액체방수,시이트방수
	지붕 및 홈통공사	선홈통, 루프드레인 설치
	금속공사	계단 논슬립, 경량천정틀, 커텐박스
	미장공사	모르터 바르기, 플로어하드너 바르기, 콘크리트 면처리, 모르터 충진
	창호공사	창호달기, 창호철물 달기
	유리공사	유리 끼우기 및 닦기
	칠공사	페인트 칠
	수장공사	바닥 깔기, 벽판 및 반자지 붙임, 단열재 설치
	부대공사	기타 잡공사

나) 기계설비공사

건축기계설비 공사 표준 시방서의 공종분류에 따르며 [표 3-3]과 같다.

[표 3-3] 건축기계설비 공사 표준 시방서에 의한 공종 분류

대 공 종	중 공 종	소 공 종
기계설비공사	공통공사	가설공사
	급배수위생설비공사	급수, 급탕, 배수통기, 위생기구, 정화조설비공사
	공기조화설비공사	열원기기, 공기조화기기, 덕트, 배관 설비공사, 시험․조정 및 평가
	소화설비공사	공통공사, 옥내소화전 및 옥외소화전, 스프링클러, 연결살수, 연결송수관, 연소방지 설비공사
	가스설비공사	도시가스 설비 공사
	자동제어설비공사	현장제어설비공사, 중앙관제설비공사
	승강기설비공사	엘리베이터설비공사

다) 기계설비 ․플랜트설비공사 수량산출기준 지침서(1999년)

건설교통부 제정 기계설비 ․플랜트설비공사 수량산출기준 지침서의 공종 분류를 따르며 [표 3-4]와 같다.

[표 3-4] 기계설비 ․플랜트설비공사 수량산출기준지침서에 의한 공종 분류

대 분 류	중 분 류	대 분 류	중 분 류
A. 공통공사	가설공사, 공통장비, 현장관리비	J. 기타공사	지지금구, 도장
B. 배관공사	강관, 동관, 스테인레스관, 관이음쇠, 플랜지접합등	K. 소방공사	함설치, 소방호스, 소방밸브류, 관창, 옥외소화전
C. 덕트공사	덕트제작 및 설치, 연도, 기구	L. 가스설비	정압기실, 가스탱크저장소
D. 보온공사	관보온, 밸브보온, 덕트보온	M. 자동제어설비	계기반 및 함류, 자동제어기기설치
E. 펌프 및 공기설비	펌프, 송풍기, 압축기	N. 운송설비	엘리베이터, 에스컬레이터
F. 밸브설비	밸브, 트랩, 수격방지기	O. 특수설비	살수설치, 냉동/냉장실 설비
G. 측정기기	측정기기	P. 서비스설비	주방, 세탁장비
H. 위생기구설비	위생기구류, 배수트랩	Q. 해체 및 철거공사	기존 설치 철거, 해체
I. 공기조화설비	냉동기, 냉온수기	Z. 제잡비	간접노무비, 경비, 일반관리비, 이윤, 공사손해보험료

3) 내역서 표준화 및 간소화 방안

가) 부속자재를 주자재의 공사비 비율로 표기

부속자재 공사비를 주자재 공사비로 나누어 비율로 표현하는 방법에는 주자재품목에 부속자재를 포함시켜 표현하는 방법과 주자재에 속하는  부속자재를 전부 합산하여 한 줄로 표현하는 방법이 있다.  우리나라는 아직 환경적인 조건들이 갖추어 있지 않고, 품목별 요율이 정하여 있지 않으므로 총액에 대한 요율로 표기하고 일정기간 후 경험치를 축적하여 품목별로 요율을 정한다.  부속자재에 대한 정의는 프로젝트별로 특성이 있기 때문에 내역서 작성 시 명확한 정의를 하여야하나, 일반적으로 주자재 접속에 필요한 부속자재(인건비가 계상되지 않는 자재), 행가 및 지지류 등을 말한다.

① 배관재의 경우

각 공종에 사용되는 배관재(강관, 동관, STS관, PVC관, PLP관 등)를 “주자재” 라하고 배관재 이외의 부속품(엘보, 티이, 레듀샤, 스트레나 등), 슬리브, 행가 및 지지류 등을 포함하여 “부속자재”라고 한다. “부속자재 금액 / 주자재 금액 = 부속자재 ” 를 산출하여 내역서의 품명 란에 부속자재라고 표기하고 단가 란에 비율을 표기한다.

[표 3-5-1] 배관재의 경우(변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 304	D 50	M	98	11,940	1,170,120		-		-	1,170,120
〃	D 65	M	81	14,800	1,198,800		-		-	1,198,800
Elbow	D 65	EA	6	9,280	55,740		-		-	55,740
Tee	D 50	EA	1	6,520	6,520		-		-	6,520
Reducer	D65	EA	5	8,500	42,500		-		-	42,500
Strainer	D 50	EA	2	15,200	30,400		-		-	30,400
Flange	D 50	EA	8	21,000	168,000		-		-	168,000
행가	D 50	EA	50	1,200	60,000		-		-	60,000
슬리브	D50	EA	10	15,400	154,000		-		-	154,000

[표 3-5-2] 배관재의 경우(변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 304	D 50	M	98	11,940	1,170,120		-		-	1,170,120
〃	D 65	M	81	14,800	1,198,800		-		-	1,198,800
부속자재	주자재의	%	1	21.8%	517,160					517,160

② 보온재의 경우

각 공종 사용되는 보온재(유리솜, 아티론, 실리카, 퍼얼라이트 등) + 보온 마감재(베파베리아, 칼라함석, 아연도함석, APS 등)를 주자재로 하고 부속품(엘보, 티이, 레듀샤, 스트레나, 밸브 등) 보온하는데 소요되는 금액을 부속자재라고 한다.“부속자재 금액 / 주자재 금액 = 부속자재 ” 를 산출하여 내역서의 품명 란에 부속자재라고 표기하고 단가 란에 비율을 표기한다.

[표 3-6-1] 보온재의 경우(변경 전 -고무 발포재)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
관보온 13t	D 80	M	85	6,961	591,685	17,696	1,504,160			2,095,845
밸브보온 13t	D 80	개소	2	6,146	12,292	43,929	87,858			100,150
엘보보온 13t	D 80	개소	6	6,453	38,718	8,015	48,090			86,808
스트레나 13t	D 80	개소	5	8,274	41,370	10,250	51,250			92,620
레듀샤 13t	D65*80	개소	2	7,524	15,048	9,524	19,048			34,096
티이 13t	D 80	개소	3	6,536	19,608	7,896	23,688			43,296

[표 3-6-2] 보온재의 경우(변경 후 -고무 발포재)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
관보온 13t	D 80	M	85	6,961	591,685	17,696	1,504,160		-	2,095,845
부속자재	주자재의	식	1	21.5%	127,036	15.3%	229,934			356,970

③ 철골의 경우

철골공사의 경우, 사용되는 부자재를 주자재(H형강)에 대한 비율로 환산하여 내역서를 작성한다. Sampling하여 비율을 조사한 결과,  H형강 공사비를 100% 라고 할 때 각종 부자재 비율은 아래와 같다.

Steel plate 10.58%, 고장력 볼트 4.62%, 앙카 볼트 1.36%, 그라우트 몰탈 0.43%, ㄷ형강1.82%, Stud 볼트 2.21%, ㄴ형강 0.88%  부속자재 계 21.9%

[표 3-7-1] 철골의 경우(변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금액	단가	금액
RH형강	SS400	톤	18.018	412,000	7,423,416					7,423,416
ㄷ 형강	250*90*8*13.5	톤	2.731	395,000	1,078,745					1,078,745
ㄴ 형강	40*40*5	톤	0.366	365,000	133,590					133,590
철 판(SS41)	T=6	KG	14	288	4,032					4,032
고장력볼트	M16 L:100	EA	21	260	5,460					5,460
STUD BOLT	∅19 L:135	EA	130	294	38,220					38,220
SPRING BOLT	M20	EA	52	474	24,648					24,648

[표 3-7-2] 철골의 경우(변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
RH형강	SS400	식	18.018	412,000	7,423,416					7,423,416
부속자재	주자재의	식	1	21.9%	1,625,728					1,625,728

④ 가설전기, 가설용수의 경우

가설공사에서, 가설전기, 가설용수 및 양수기 사용료 등을 건축공사비에 대한 비율로 환산하여 내역서를 작성한다. Sampling하여 비율을 조사한 결과, 건축공사비를 100%라고 할 때 가설전기, 가설용수 및 양수기 사용료 비율은 0.24%로 나타났다.

[표 3-8-1] 가설전기, 가설용수의 경우(변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금액	단가	금액
임시동력시설		식	1						7,560,000	7,560,000
임시용수시설		식	1						2,560,000	2,560,000
양수기사용료	2HP	시간	1,600					112	179,200	179,200

[표 3-8-2] 가설전기, 가설용수의 경우(변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금액	단가	금액
임시동력․용수 등	건축공사비	식	0.24%						10,299,200	10,299,200

⑤ 연도의 경우

직관을 주자재로 하고 기타를 부속자재로 한다. “부속자재 금액 / 주자재 금액 = 부속자재 ” 를 산출하여 내역서의 품명 란에 부속자재라고 표기하고 단가 란에 비율을 표기한다.

[표 3-9-1]  연도의 경우(변경 전)

품 명		규 격	단위		수량		재 료 비			노 무 비		경 비		계
							단 가		금 액	단 가	금 액	단가	금액
0208 - 연도설치공사
옥상연돌캡	1300-H5-SK			PC		1		297,880	297,880	0	0	0	0	297,880
우수차단막	1300-H5-SC			PCS		2		47,900	95,800	0	0	0	0	95,800
477MM점검구	1300-H5-CH477			PC		1		196,400	196,400	0	0	0	0	196,400
우수차단막	1300-H5-VT			PC		1		163,460	163,460	0	0	0	0	163,460
477열팽창신축조인트	1300-H5-SS477			PC		1		238,920	238,920	0	0	0	0	238,920
477MM지관	1300-H5-477			PCS		88		178,580	15,715,040	0	0	0	0	15,715,040
고정지지대	1300-H5-PA			PCS		2		132,660	265,320	0	0	0	0	265,320
45합류관	1300-H5-LT500			PC		1		921,470	921,470	0	0	0	0	921,470

[표 3-9-2]  연도의 경우(변경 후)

품 명		규 격	단위		수량		재 료 비			노 무 비		경 비		계
							단 가		금 액	단 가	금 액	단가	금액
0208 - 연도설치공사
477MM지관	1300-H5-477			PCS		88		178,580	15,715,040	0	0	0	0	15,715,040
부속자재	주자재의			식		1		13.9%	2,179,250	0	0	0	0	2,179,250

※ 부속자재를 주자재의 공사비 비율로 표기하는 방법은 처음에는 프로젝트별, 공종별로 비율이 차이가 있으나 추후 경험치를 분석하여 프로젝트별, 공종별로 일정요율을 적용하고 필요 시 가중치를 주어 조정 할 수 있도록 한다. 이렇게 되면 적산 시 업무효율화가 될 수 있을 것 이다.

나) 일위대가화

① 배관재의 경우

강관, 동관, STS관등 배관재는 소모자재 및 설치비를 포함하여 일위대가화 한다.

[표 3-10-1] 배관재의 경우(변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 304 (SCH 10)	D 50	M	98	11,940	1,170,120		-		-	1,170,120
〃	D 65	M	81	14,800	1,198,800		-		-	1,198,80057021
STS 강관 용접	D 65	개소	70	2,603	182,210		-		-	182,210
“	D 50	개소	60	2,405	144,300					144,300
노무비	플랜트용접공	인	44			57,021	2,508,924			2,508,924
노무비	플랜트배관공	인	22			63,995	1,407,890			1,407,890
노무비	특별인부	인	22			50,160	1,103,520			1,103,520

[표 3-10-2] 배관재의 경우(변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 배관(SCH 10)	D 50	M	98	13,412	1,314,420	27,942	2,738,364		-	2,738,364
STS 배관(SCH 10)	D 65	M	81	17,050	1,381,010	47,427	2,281,970		-	2,281,970

② 덕트 기구 취부

덕트 기구 + 후렉시블 + 밴드 + 노무비를 포함한 일위대가를 작성하여 적용한다.

[표 3-11-1] 덕트 기구 취부(변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
사각디퓨져 (STL)	ND125	EA	50	8,500	425,000					425,000
후렉시블호스 (보온)	D125	M	75	3,050	228,750					228,750
STS BAND	D125	EA	100	320	32,000					32,000
노무비	덕트공	인	40			26,108	1,044,320			1,044,320

[표 3-11-2] 덕트 기구 취부(변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
사각디퓨져 (STL)	ND125	EA	50	13,715	685,750	20,886	1,044,320			1,730,070

③ 합판거푸집, 철근 구조물 콘크리트 펌프차 타설

철근콘크리트 공사 경우, 스페이서, 세퍼레이터 및 진동기 손료를 주 공사비에 대한 비율로 환산하여 적용한다.(일위대가 작성 간소화)

Sampling하여 비율을 조사한 결과 아래와 같다.

ㆍ거푸집 공사비를 100%라고 할 때 스페이서, 세퍼레이터의 비율은 0.26%,

ㆍ펌프카 붐타설(철근) 공사비를 100%라고 할 때 진동기 손료 비율은 1.48%

추후 요율을 확정 적용하기 위하여는 일정기간 경험치를 축적, 확보된 데이터를 분석하여 품목별로 정의하여야 하겠다.

공사명 품 명	단위	나노종합FAB센터			국민은행 대전콜센터
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
거푸집	M2	23,631	426,777,594	100.00	17,985	496,442,870	100.00
스페이서, 세퍼레이터	EA	65,243	1,226,362	0.29	-
펌프카 붐타설(철근)	M3	7,734	89,358,636	100.00	14,093	140,933,000	100.00
진동기 손료	M3	7,734	1,979,904	0.22	-
공사명 품 명	단위	서울 농학교 언어진료센터			국립생물자원관
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
거푸집	M2	755	322,904,492	100.00	7,654	224,557,010	100.00
스페이서, 세퍼레이터	EA	30,556	733,983	0.23	36,060	1,277,277	0.57
펌프카 붐타설(철근)	M3	3,388	44,554,329	100.00	5,423	67,207,239	100.00
진동기 손료	M3	3,388	13,552	0.03	5,423	309,111	0.46

[표 3-12] 합판 거푸집, 철근 구조물 콘크리트 펌프차 타설

공사명 품 명	단위	대전 신계중학교			차세대연구기반동
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
거푸집	M2	87,036	1,798,752,099	100.00	15,090	307,626,906	100.00
스페이서, 세퍼레이터	EA	23,397	458,518	0.03	16,938	643,644	0.21
펌프카 붐타설(철근)	M3	15,257	208,044,452	100.00	4,452	60,654,048	100.00
진동기 손료	M3	-			4,452	2,266,068	3.74

공사명 품 명	단위	핵융합실험동			전자현미경실험동
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
거푸집	M2	70,230	2,292,296,780	100.00	10,024	157,888,369	100.00
스페이서, 세퍼레이터	EA	210,690	4,424,490	0.19	10,537	421,480	0.27
펌프카 붐타설(철근)	M3	34,700	623,704,196	100.00	3,278	30,672,246	100.00
진동기 손료	M3	34,700	624,600	0.10	3,278	1,117,798	3.64
공사명 품 명	단위	핵융합지원동			평 균		비 고
		수 량	금 액(원)	비율(%)
거푸집	M2	16,412	328,882,296	100.00	100.00
스페이서, 세퍼레이터	EA	49,236	1,033,956	0.31	0.26
펌프카 붐타설(철근)	M3	4,182	44,341,746	100.00	100.00
진동기 손료	M3	4,182	75,276	0.17	1.48

④ 석 공사 및 타일공사

석재 및 타일공사의 경우, 바닥 보양 품을 가설공사 공종에 별도 계상하던 것을 석재 및 타일붙이기 일위대가표에 각각 통합하여 일위대가표를 간소화한다.

[표 3-13-1] 석 공사(화강석 판(바닥) - 변경 전)

- 화강석 판(바닥)

(㎡)

구 분	규 격	단 위	단 가	바 닥
				수 량	금 액
석 재 판		㎡	40,900	1.1	11,990
모 르 터	1:3(바름두께40mm)	㎡	103,846	0,045	4,673.0
철 물	황동	kg	4,100		-
재료비소계					49,663
석 공		인	95,056	0,49	46,577.4
보통인부		〃	52,374	0,25	13,093.5
노무비소계					59,670
합 계					109,333

- 건축물 보양

(보양면적 ㎡당)

구 분	규 격	단위	단 가	석재면, 테라조면타일(바닥)
				수량	금액
가 마 니		매	4,000	-	-
톱 밥		ℓ	별도	30	-
재료비소계					-
보 통 인 부		인	52,374	0.002	104.7
노무비소계					104
합 계					104

[표 3-13-2] 석 공사(화강석 판(바닥) - 변경 후)

(㎡당)

구 분	규 격	단 위	단 가	바 닥
				수 량	금 액
석 재 판		㎡	40,900	1.1	44,990
모 르 터	1:3(바름두께40mm)	㎡	103,846	0,045	4,673.0
철 물	황동	kg	4,100		-
재료비소계					49,663
석 공		인	95,056	0,49	46,577.4
보통인부		〃	52,374	0,25	13,093.5
〃	보양	〃	52,374	0.002	104.7
노무비소계					59,775
합 계					109,438

※ 석재 붙이기 및 보양 노무비 일위대가표 통합

[표 3-14-1] 타일 공사(압착 및 밀착공법(바닥) - 변경 전)

- 건축물 보양

(보양면적 ㎡당)

구 분	규 격	단위	단 가	석재면, 테라조면타일(바닥)
				수량	금액
가 마 니		매	4,000	-	-
톱 밥		ℓ	별도	30	-
재료비소계					-
보 통 인 부		인	52,374	0.002	104.7
노무비소계					104
합 계					104

- 압착 및 밀착공법(바닥)

(㎡)

구 분	규 격	단위	단 가	바름두께 5mm		6mm		7mm
				수 량	금 액	수 량	금 액	수량	금액
시 멘 트		kg	77.2	3.57	275.6	4.28	330.4	5.00	386.0
백시멘트		〃	200	1.48	296.0	1.48	296.0	1.48	296.0
모 래		㎥	11,000	0.0062	68.2	0.0073	80.3	0.0081	89.1
공구손료	인건비의 3%	식		1	951.4	1	951.4	1	951.4
재료비소계					1,591		1,658		1,722
타 일 공		인	98,192	0.216	21,209.4	0.216	21,209.4	0.216	21,209.4
줄 눈 공		〃	79,875	0.024	1,917.0	0.024	1,917.0	0.024	1,917.0
보통인부	붙 임	〃	52,374	0.080	4,189.9	0.080	4,189.9	0.080	4,189.9
〃	청 소	〃	52,374	0.024	1,256.9	0,024	1,256.9	0,024	1,256.9
〃	소운반	〃	52,374	0.060	3,142.4	0.060	3,142.4	0.060	3,142.4
노무비소계					31,715		31,715		31,715
합 계					33,306		33,373		33,437

[표 3-14-2] 타일 공사(압착 및 밀착공법(바닥) - 변경 후)

(㎡)

구 분	규 격	단위	단 가	바름두께 5mm		6mm		7mm
				수 량	금 액	수 량	금 액	수량	금액
시 멘 트		kg	77.2	3.57	275.6	4.28	330.4	5.00	386.0
백시멘트		〃	200	1.48	296.0	1.48	296.0	1.48	296.0
모 래		㎥	11,000	0.0062	68.2	0.0073	80.3	0.0081	89.1
공구손료	인건비의 3%	식		1	951.4	1	951.4	1	951.4
재료비 소계					19,101		19,168		19,232
타 일 공		인	98,192	0.216	21,209.4	0.216	21,209.4	0.216	21,209.4
줄 눈 공		〃	79,875	0.024	1,917.0	0.024	1,917.0	0.024	1,917.0
보통인부	붙 임	〃	52,374	0.080	4,189.9	0.080	4,189.9	0.080	4,189.9
〃	청 소	〃	52,374	0.024	1,256.9	0,024	1,256.9	0,024	1,256.9
〃	소운반	〃	52,374	0.060	3,142.4	0.060	3,142.4	0.060	3,142.4
〃	보 양	〃	52,374	0.002	104.7	0.002	104.7	0.002	104.7
노무비 소계					31,820		31,820		31,820
합 계					50,921		50,988		51,052

※ 타일 붙이기 및 보양 노무비 일위대가표 통합

다) 단위 변경

① 덕트 부속

• Sound chamber

물가자료 등에 가격 표기가 10원/cm2 으로 표기되어 있으며 수량산출 시  cm2로 산출한다. 단지 내역서에 표기 할 때 규격별 개수로 나타낸다.

[표 3-15-1] 덕트 부속( Sound Chamber - 변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
SOUND CHAMBER	3900x1800x850	EA	1	1,376,340	1,376,340					1,376,340
SOUND CHAMBER	2600x1500x850	EA	1	856,660	856,660					856,660
SOUND CHAMBER	2400x1400x900	EA	1	786,480	786,480					786,480
SOUND CHAMBER	3400x2100x850	EA	1	1,370,540	1,370,540					1,370,540
SOUND CHAMBER	1000x1200x800	EA	1	343,360	343,360					343,360
SOUND CHAMBER	1700x1200x1400	EA	1	707,600	707,600					707,600
SOUND CHAMBER	2500x1400x1400	EA	1	1,039,360	1,039,360					1,039,360

[표 3-15-2] 덕트 부속( Sound Chamber - 변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
SOUND CHAMBER		cm2	648,034	8.8	5,709,340					5,709,340

• Damper 류

물가자료 등에 가격 표기가 10원/cm2 으로 표기되어 있으며 수량산출 시 cm2로 산출한다. 단지 내역서에 표기 할 때 규격별 개수로 나타낸다.

[표 3-16-1] 덕트 부속( Damper 류 - 변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
F.V.D W/FUSE	1500x450	EA	1	46,275	46,275					46,275
F.V.D W/FUSE	1000x600	EA	1	41,400	41,400					41,400
F.V.D W/FUSE	1000x450	EA	1	31,650	31,650					31,650

[표 3-16-2] 덕트 부속( Damper 류 - 변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
V . D		cm2	17,250	6.5	112,125					112,125
FUSE		EA	3	2,400	7,200					7,200

• Register 류

물가자료 등에 가격 표기가 18원/cm2 으로 표기되어 있으며 수량산출 시 cm2로 산출한다. 단지 내역서에 표기 할 때 규격별 개수로 나타낸다.

T.V, Grille, Louver 등의 덕트 부속자재도 Register와 동일하게 표기(단위) 방법을 개수에서 cm2로 바꾸면 간소화가 된다.

[표 3-17-1] 덕트 부속( Register 류 - 변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
GRILLE (AL)	1000x650	EA	2	58,500	117,000					117,000
GRILLE (AL)	1000x700	EA	3	63,000	189,000					189,000
REGISTER (AL)	200x 150	EA	29	15,000	435,000					435,000
REGISTER (AL)	250x 150	EA	15	15,000	225,000					225,000

[표 3-17-2] 덕트 부속( Register 류 - 변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
GRILLE (AL)		cm2	34,000	9	306,000					306,000
REGISTER (AL)		cm2	14,325	46	660,000					660,000

② 창호류

SD : 개소 ⟶ 면적(㎡)으로 수량산출

AW, AG : 개소 ⟶ 중량(㎏)으로 수량 산출

[표 3-18-1] 창호류(변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
0112 창호공사
FSD-1	2600*3400	개소	1	645,320	645,320	0	0	0	0	645,320
FSD-2	2500*2400	개소	1	522,000	522,000	0	0	0	0	522,000
FSD-1A	2200*2100	개소	1	337,260	337,260	0	0	0	0	337,260
FSD-1B	2200*2100	개소	1	415,800	415,800	0	0	0	0	415,800
CAW-1A	6600*3000 (120.6KG)	개소	3	1,213,236	3,639,708	0	0	0	0	3,639,708
CAW-1B	6550*3000 (120.2KG)	개소	1	1,209,212	1,209,212	0	0	0	0	1,209,212
AG-1A	6600*900 (74.2KG)	개소	5	659,638	3,298,190	0	0	0	0	3,298,190
AG-1B	6300*900 (71.1KG)	개소	1	632,079	632,079	0	0	0	0	632,079

AW창호(개소⟶중량)

품 명	규 격	단 위	수 량	계
CAW - 1A	120.6Kg	EA	3	361.8
CAW - 1B	120.2Kg	EA	1	120.2
AG - 1A	74.2Kg	EA	5	371
AG - 1B	71.1Kg	EA	1	71.1

[표 3-18-2] 창호류(변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
0112 창호공사
FSD		m2	24	80,016	1,920,380	0	0	0	0	1,920,380
CAW		kg	482	10,060	4,848,920	0	0	0	0	4,848,920
AG		kg	442	8,892	3,930,269	0	0	0	0	3,930,269

라) 중공종별 내역서 작성

소공종(층별, 동별, 세부 공정별)별 집계표에 의해 작성한 상세 내역서를 소공종 집계표를 합산하여 중공종(급배수위생, 공기조화, 소화, 가스, 자동제어, 승강기) 수량 집계표를 작성하고 중공정 집계표에 의한 내역서를 작성하는데 이를 “표준화 내역서”라 한다.

[표 3-19] 공종별 집계표

구 분	소 공 정	중 공 종
건축공사	- 연구동 철골공사 - 행정동 철골공사	- 철골공사
기계설비공사	- 연구동 1층 배관공사 - 연구동 2층 배관공사 - 행정동 1층 배관공사 - 행정동 2층 배관공사	- 배관공사

마) 기 타

배관재를 규격별로 수량산출 한 후 중량으로 환산 (m × kg/m = kg) 하여 표기할 수는 있으나 획기적인 방법이 될 것 같다.  또한 내역서 만으로 공사의 성격을 알기에는 어려울 것 같다.  장비(보일러, 냉동기, 공기조화기, 펌프 , 송풍기, 탱크류, 헷다류 등) 등 견적서에 의하여 내역서에 적용되는 품명들은 설치비(설치부품 + 노무비)가 포함된 단가를 적용한다. “부록3 프로젝트별 표준화 내역서 작성”  참조

지금까지 시설공사 내역서 표준화 및 간소화 방안에 대하여 단계별 작성서류를 정리하면 [표 3-20]과 같다

[표 3-20] 단계별 작성 서류

간소화 항목	수량산출서	상세내역서	표준화 내역서	비고
1. 부속자재를 주자재 비율	소공종, 중공종	소공종	중공종
2. 일위대가화	일위대가표	일위대가표	일위대가표	일위대가표
3. 단위변경	규격별, 단위별	규격별	단위별	단위별로 통일
4. 공종별 작성	소공종, 중공종	소공종	중공종
5. 기 타	견적서	설치비별도	설치비포함

Note : 1. 장비(보일러, 냉동기, 공기조화기, 펌프, 송풍기, 탱크류, 헷다류 등)

등은 견적서 작성 시 설치비(설치부품 + 노무비)를 포함한 조건으로

작성한다.

4) 내역서 표준화 및 간소화 업무처리 절차

각 공정별 내역서를 수집․분석하면서 설계도서 작성단계에서 소공종에 의한 상세내역서 작성, 중공종에 의한 표준화 내역서를 작성하면 입찰 시, 계약 시, 공사집행 시, 설계변경 시 또는 준공도서 작성 시 사무 간소화로 인한 많은 효과를 가져 올 수 있을 것이다 . [표 3-21]에 내역서 표준화 및 간소화에 대한 업무처리 절차를 도식화 했다.

[표 3-21] 내역서 표준화 및 간소화 업무처리 절차

			설계도면 작성
			↓
				─	소공종 집계표 - 세부공정별 - 층별 - 동별 중공종 집계표
			수량산출서 작성
			↓
			상세 내역서 작성	─	소공종 집계표
			↓
			표준화 내역서 작성	─	중공종 집계표
			- 부속자재를 주자재 비율 (배관재, 보온재, 철골, 임시동력 및 용수, 연도) - 일위대가화 배관, 덕트기구부착, 석재 및 타일보양, 콘크리트 진 동기, 스페이서 및 세퍼레 이터) - 단위변경 (덕트 취출구 등, 창호류) - 중공종별 내역서 작성 (급․배수위생, 공기조화, 소화, 가스, 자동제어, 승 강기) - 기타

4. 표준화 내역서 작성 결과 분석

프로젝트에 대한 설계용역 성과물 제출 시 납품되는 설계도서는 여러 종류가 있다. 이번 프로젝트에서는 수량 산출서에 의해 작성되는 내역서에 대하여 국내․외 사례 등을 조사․ 분석하고 우리 실정에 맞도록 방법론적 제안을 하고자 한다.

이번 연구를 통하여 제안된 방법을 적용하면 공사의 성격에 따라 다소 차이는 있지만 공사의 특성을 유지하면서 평균적으로 50% 이상의 내역서 분량을 줄일 수 있었다.  공종 분류는 건축공사 표준시방서, 건교부 제정 수량산출기준 지침서 및 건축기계설비 표준시방서의 기준을 따른다.

1) 작성사례

설계도면에 의해 수량산출시 소공정에 의하여 상세하게 층별, 동별, 세부 공정별 수량산출을 한다. 수량산출 집계표를 소공정에 의해 작성하고 다시 중공정에 의한 집계표를 작성한다. 소공정에 의해 산출된 집계표의 수량을 내역서에 기재하고 단가를 적용하면 상세내역서가 된다. 이렇게 작성된 상세내역을 제안된 (안)을 적용하여 중공종에 의한 내역서를 작성한다. 중공종에 의해 작성된 내역서를 “표준화 내역서”라고 한다. 수량산출시 수량집계는 프로그램을 활용하여 산술적인 오차를 줄인다. “부록3 프로젝트별 표준화 내역서 작성” 참조

2) 표준화 내역서 작성 결과

○○대학병원 내역서를 가지고 시설공사 내역서 표준화 및 간소화에서 제안한 사례들을 칼라를 이용하여 알아보기 쉽도록 표시하였다.

적용칼라는 ① 부속자재를 주자재의 공사비 비율로 표기 : 노랑

② 일위대가화 : 연녹색

③ 단위변경 : 파랑

④ 중공종별 내역서 작성 : 빨강

⑤ 기타 : 회색

제안된 사례들을 가지고 시설공사 내역서를 표준화 및 간소화 해본 결과 [표 4-1]과 같은 결과를 얻을 수 있었다.  가능한 많은 자료를 가지고 분석한다면 보다 더 정확한 결과를 얻을 수 있을 것이다.

[표 4-1] 표준화 내역서 적용 시 간소화율

공 사 명	구 분	공사비	상세내역서(변경 전)	표준화내역서(변경 후)	간소화율	비 고
00대학병원	기계설비 공사	292억	5,350품목	2,235품목	58%
00도로출입국		23	1,402	450	68
초․중등학교		15	2,046	698	66
00실험동		3	856	405	53
전자현미경		8	634	316	51
00우체국		250	4,869	2,320	52
00연구기반동	건축공사	43	380	308	19
전자현미경동		29	305	264	13
00대학병원		780	1,817	1,288	29
00지방경찰청		54	810	662	18
초․중등학교		80	756	558	26
계			19,225	9,504	51

Note : 공정별 상세한 간소화율은 #첨부4 기계설비공사 공정별 상세 간소화율을          참조한다.

부록4  시뮬레이션 자료(변경 전, 변경 후)

※ 건축공사 감소율 대안

- 동일 또는 유사한 공종에 있어서 3회 이상 표기되는 품목을 1식으로              조정하면 45%내외의 감소율이 가능하나,

- 간소화된 품목의 공량을 내역서 상으로는 파악하기 곤란하며, 일위대가           표 및 수량산출서를 참조해야 한다.

[표 4-2-1] 건축공사 감소율 대안(변경 전)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금액	단가	금액
0111 철근콘크리트공사
레미콘	25-180-12	m3	321	41,836	13,429,356					13,,429,356
"	25-240-15	"	4,496	47,809	214,949,264					214,949,264
"	25-240-18	"	315	48,502	15,278,130					15,278,130
이형철근	D-10	톤	35	475,000	16,625,000					16,625,000
“	D-13	“	109	470,000	51,230,000					51,230,000
“	HD-16	“	80	465,000	37,200,000					37,200,000
“	HD-19	“	247	465,000	114,855,000					114,855,000
“	HD-22	“	42	465,000	19,530,000					19,530,000

[표 4-2-2] 건축공사 감소율 대안(변경 후)

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금액	단가	금액
0111 철근콘크리트공사
레미콘	각종(5,132m3)	식	1		243,656,750					243,656,750
이형철근	각종(513톤)	식	1		239,440,000					239,440,000

5. 기대효과

사례에 의해 기대효과를 분석하여 보면

1) 100억 이상의 공사

2003년도 건설 현황을 보면 발생건수는 98,337건, 공사금액 817,990억원이고, 공사금액 100억 이상인 계약건수는 2,796건이다. 1개 프로젝트 수행 시 내역서는 10권정도 소요되며 설계도서 중 내역과 관련된 일위대가표(154+82매), 단가리스트(80+52매), 집계표(23+21매), 내역서(191+95매)를 합산하면 분량은 698페이지가 된다.  표준화 및 간소화 시 영향을 받는 설계도서는  일위대가표를 제외한 나머지 부문의 설계도서가 된다.

① 소모품 절감

2,796건 × 10권 × 462페이지 × 50원(양면) × 50%(간소화율) =  322, 938,000원

② 인건비 절감

52,374원/보통인부 × 7.5일 × 2.3(rate) × 2,796건 = 2,526,048,996원

③ 계( ① + ② ) : 2,848,989,996원

2) 계약전문 ○○기관에서 집행하는 공사

2003년도 ○○기관청에 의뢰하여 원가계산 및 계약이 진행된 공사 건수는 773건이다. ○○기관에 의뢰하여 진행되는 공사에서 발생되는 설계도서의 수량을 보면 설계용역 완료시 납품 10부, 계약 시 5부, 기성 및 설계변경 등 6회 × 5부 = 30부가 된다. ○○기관에 의뢰되는 공사에 표준화 내역서 적용 시 80면 정도의 페이지가 줄어든다. ○○기관 사례를 기준으로 예산 절감효과(추정)를 산출하여 보면

① 2003년도 조달청 원가계산(773건) : 462,570천원 절감

- 지류 인쇄비 : 80면 × 45부 × 50원/면 × 773건 = 139,140,000원

- 소요 인건비 : 80면 × 45부 × 773건 × 0.5분/(60분×8시간) × 111,576원(중급                   기술자) = 323,430,930원

② 내역입찰 시(229건) : 380,655천원

- 지류 인쇄비 : 229건 × 100업체 × 50원/면 × 100면 = 114,500,000원

- 소요 인건비 : 100면 × 229건 × 100업체 × 0.5분/(60분×8시간) × 111,576원                    (중급기술자) = 266,155,250원

③ 계( ① + ② ) : 843,225,000원

100억 이상의 공사에서만 연간 절감효과는 28억원 정도로 나타나고 조달청에서 집행하는 공사에서는 8억원 정도의 절감 효과를 나타낸다. 우리나라에서 발생되는 건설공사 전반에 적용 될 시 파급되는 절감효과는 더욱 많을 것으로 생각된다.

6. 문제점 및 대책

“시설공사 내역서 표준화 및 간소화 방안에 관한 연구” 용역에서 제출된 성과물이 빛을 보기 위하여는 다음과 같은 부문의 건설관련법규, 계약관련법규 등의 개정이 필요하다.

- 건설관련법규 : 설계도서 작성 지침, 표준품셈

- 계약관련법규 : 건설관련 법규가 개정이 되기 전이라도 조달청이나 발주처에                    서 용역계약 일반조건에 “설계도서 납품 시 소공종에 의한                     상세내역서 및 중공종에 의한 표준화 내역서를 제출하도록 한                    다”는 조항을 반영한다.

7. 결  론

건설 산업은 무에서 유를 창조하는 종합예술로서 지금 이 순간에도 수많은 공사가 진행되고 있고 현장에서는 복잡한 내역서 구조에 의해 설계변경 작업을 하고 있다. 아마도 건설기술인이라면 설계변경 작업을 별도의 숙소를 잡아 날을 새면서 작업을 한 경험들이 있으리라 생각한다. 공사의 흐름에 별 영향이 없는 엘보, 티 개수를 세면서 산수적인 덧셈, 뺄셈을 두 번, 세 번 한 적이 있을 것이다. 얼마나 무의미한 일이었는지를 생각해본다. 연구 용역 범위가 설계도서 전반에 대한 표준화 및 간소화였으면 보다 체계적이고 효율적인 결과가 도출되었을 것이라는 아쉬움이 남는다.

연구를 마치면서 다음과 같이 결론을 맺고자 한다.

1. 건설교통부에서 검토되어 진행되고 있는 실적공사비제도를 정의 할 때 “시     설공사 내역서 표준화 및 간소화 방안에 관한 연구”에서 제안된 (안)을 도입     하여 표준화 및 간소화가 될 수 있었으면 좋겠다.

2. 제안된 안을 적용하여 표준화 내역서 작성 시 품목수로 대비하였을 때 기계    설비공사는 58%, 건축공사는 24%의 간소화됨을 볼 수 있었다. 건축공사의 경우    간소화율이 적은 이유는 상당부분이 이미 일위대가화 되어 있으며 철골공사,     창호공사 등에서 많은 부분이 간소화 된다.  획기적인 내역서 간소화를 하기     위하여는 기계설비공사의 경우 파이프를 중량으로 표기하는 방법과 건축공사에    서 동일 또는 유사한 공종에 있어서 3회 이상 표기되는 품목을 1식으로 조정 할 수 있    으나 객관성 확보가 어렵고 내역서 만으로 공사성격을 파악하기에는 어려움이 많기 때    문에 제안하지 않는다.

3. 부속자재를 주자재의 공사비 비율에 의하여 표준화하는 작업은 상세 내역서    에서 표준화 내역서를 작성하는 과정에서 공종별로 상이하게 나타나는데 실무    에 적용하면서 실적치를 검토하여 추후 공종별로 Rate를 확정하는 것이 좋겠     다.

4. 일회성 연구 용역에 의하여 획기적인 아이디어를 도출 할 수도 있겠지만, 이번 연구    용역의 성격은 건설시장에서 발생되는 자료를 기준으로 아이디어를 도출하여야 하므로    주기적으로 제안된 연구결과를 가지고 검토 및 분석을 하여 변화된 환경조건들을 반영    하여야 할 것으로 사료된다.

5. 국가계약 전문기관인 조달청은 여러 부문에서 표준화 및 간소화를 통하여 업    무 효율화를 기할 수 있도록 선도적인 역할을 하여야 한다. 건설공사에 대하여    표준화 및 간소화에 관한 연구용역은 이제 시작에 불과하다고 생각한다. 사회    적으로 건설 환경은 급변하고 있으며, 이런 환경에 적응 할 수 있도록 정부기    관에서 주도적인 역할을 하여야 한다.

참고문헌

1. 건설공사표준품셈  대한건설진흥회(주)건설교통저널

2. 기계설비공사 표준품셈  (주)높은오름

3. 건축공사 표준시방서  (사)대한건축학회

4. 건축기계설비공사 표준시방서 (사)대한설비공학회

5. 건축공사 내역서 표준서식 ․동해설  대성출판사

6. 공공건축공사내역서 표준서식(설비공사편)․동해설 대성출판사

7. 공공건축공사적산기준․해설   (건축공사편) RIBC

8. 공공 건축공사 적산기준․해설 (설비공사편) RIBC

9. 공사보괘요람(건축․설비편)     (재)경제조사회

10. 2004년도 실적 단가집          건설교통부

11. 수량산출기준지침서(1999)       건설교통부

12. 국가 계약법 편람            (사)한국경영연구원

부록

1. 국내․외 사례조사

2. 공종별 표준화 내역서 작성(변경 전․후 대비)

3. 기계설비공사 관이음부속 및 지지물 부자재 비율

4. 기계설비공사 공정별 상세 간소화율

5. 프로젝트별 표준화 내역서 작성(○○대학병원)

6. 시뮬레이션 자료(변경 전, 변경 후)

7. 건축공사 내역서 표준서식 ․동해설 번역서

8. 공공건축공사내역서 표준서식(설비공사편)․동해설 번역서

# 부록1  국내․외 사례조사

1) 국내

(1) 배관공사

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 304 (SCH 10)	D 50	M	98	11,940	1,170,120		-		-	1,170,120
〃	D 65	M	81	14,800	1,198,800		-		-	1,198,800
〃	D 150	M	81	36,990	2,996,190		-		-	2,996,190
〃	D 350	M	153	135,690	20,760,570		-		-	20,760,570
STS 316 (SCH 10)	D 65	M	47	21,784	1,023,848		-		-	1,023,848
〃	D 80	M	94	25,592	2,405,648		-		-	2,405,648
〃	D 100	M	128	33,096	4,236,288		-		-	4,236,288
〃	D 125	M	49	47,306	2,317,994		-		-	2,317,994
〃	D 150	M	45	56,140	2,526,300		-		-	2,526,300
〃	D 200	M	2	88,424	176,848		-		-	176,848
〃	D 300	M	17	156,968	2,668,456		-		-	2,668,456
〃	D 350	M	27	205,604	5,551,308		-		-	5,551,308
〃	D 400	M	72	235,354	16,945,488		-		-	16,945,488
〃	D 450	M	40	246,480	9,859,200		-		-	9,859,200
STS 316 (SCH 10)	D 65	M	56	22,040	1,234,240		-		-	1,234,240
〃	D 100	M	122	38160	4,655,520		-		-	4,655,520
〃	D 200	M	75	141590	10,619,250		-		-	10,619,250
〃	D 300	M	28	210560	5,895,680		-		-	5,895,680

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
〃	D 350	M	71	255945	18,172,095		-		-	18,172,095
〃	D 450	M	41	371,925	15,248,925		-		-	15,248,925
ELBOW (SCH80)	D 20	EA	9	5,170	46,530		-		-	46,530
ELBOW (SCH10)	D 50	EA	8	3,600	28,800		-		-	28,800
〃	D 65	EA	6	5,730	34,380		-		-	34,380
〃	D 150	EA	14	32,980	461,720		-		-	461,720
〃	D 300	EA	3	184,050	552,150		-		-	552,150
〃	D 350	EA	6	241,500	1,449,000		-		-	1,449,000
ELBOW, (STS-316, SCH10)	D 65	EA	6	9,290	55,740		-		-	55,740
〃	D 80	EA	6	11,510	69,060		-		-	69,060
〃	D 100	EA	18	18,380	330,840		-		-	330,840
〃	D 125	EA	8	36,620	292,960		-		-	292,960
〃	D 150	EA	3	46,840	140,520		-		-	140,520
〃	D 200	EA	2	100,780	201,560		-		-	201,560
〃	D 300	EA	5	256,160	1,280,800		-		-	1,280,800
〃	D 350	EA	4	358,800	1,435,200		-		-	1,435,200
〃	D 400	EA	2	510,340	1,020,680		-		-	1,020,680
〃	D 450	EA	3	767,140	2,301,420		-		-	2,301,420
ELBOW, (STS-316, SCH20)	D 65	EA	8	11,330	90,640		-		-	90,640
〃	D 100	EA	10	24,250	242,500		-		-	242,500
〃	D 200	EA	4	179,240	716,960		-		-	716,960
〃	D 300	EA	5	334,130	1,670,650		-		-	1,670,650

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
〃	D 350	EA	2	635,140	1,270,280		-		-	1,270,280
〃	D 450	EA	3	1,141,430	3,424,290		-		-	3,424,290
ELBOW, (STS-304, SCH10)	D 300	EA	2	146,010	292,020		-		-	292,020
ELBOW, (STS-316, SCH10)	D 100	EA	1	12,870	12,870		-		-	12,870
〃	D 350	EA	2	251,160	502,320		-		-	502,320
TEE, (STS-304, SCH10)	D 50	EA	1	6,520	6,520		-		-	6,520
REDUCER(STS-316, SCH10)	D 350 x D 300	EA	1	154,910	154,910		-		-	154,910
〃	D 400 x D 350	EA	1	192,960	192,960		-		-	192,960
REDUCER(STS-316, SCH20)	D 350 x D 300	EA	1	245,680	245,680		-		-	245,680
NIPPLE, (STS-316, SCH40)	D 15	EA	1	3,280	3,280		-		-	3,280
〃	D 20	EA	10	4,300	43,000		-		-	43,000
NIPPLE, (STS-316, SCH40)	D 15	EA	1	5,930	5,930		-		-	5,930

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
HALF COUPLIN (STS-304, SCH80)	D 20	EA	8	3,040	24,320		-		-	24,320
PLUG(STS-316)	D 20	EA	9	3,030	27,270		-		-	27,270
GATE VALVE (STS304)	D 20	EA	14	44,500	623,000		-		-	623,000
GLOBE VALVE (STS 316)	D 15	EA	2	58,000	116,000		-		-	116,000
TRAP(STS 304 )	D 20	EA	2	261,000	522,000		-		-	522,000
STS 배관(옥내배관)	D 50	M	89	859	76,451	36,590	3,256,510		-	3,332,984
STS 배관(옥내배관)	D 65	M	167	1,091	182,197	47,427	7,920,309		-	8,102,538
STS 배관(옥내배관)	D 80	M	85	1,258	106,930	54,647	4,644,995		-	4,751,950
STS 배관(옥내배관)	D 100	M	225	1,632	367,200	72,512	16,315,200		-	16,682,346
STS 배관(옥내배관)	D 125	M	44	1,972	86,768	88,807	3,907,508		-	3,994,297
STS 배관(옥내배관)	D 150	M	126	2,435	306,810	111,191	14,010,066		-	14,316,904
STS 배관(옥내배관)	D 200	M	69	3,384	233,496	160,302	11,060,838		-	11,294,361
STS 배관(옥내배관)	D 300	M	179	5,387	964,273	268,030	47,977,370		-	48,941,709
STS 배관(옥내배관)	D 350	M	227	5,763	1,308,201	296,572	67,321,844		-	68,630,045
STS 배관(옥내배관)	D 400	M	65	6,500	422,500	350,806	22,802,390		-	23,224,867
STS 배관(옥내배관)	D 450	M	72	7,291	524,952	412,316	29,686,752		-	30,211,671
STS 강관 용접	D 65	개소	70	2,603	182,210		-		-	182,210
STS 강관 용접	D 80	개소	27	3,281	88,587		-		-	88,587
STS 강관 용접	D 100	개소	101	5,090	514,090		-		-	514,090

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
STS 강관 용접	D 125	개소	24	7,639	183,336		-		-	183,336
STS 강관 용접	D 150	개소	56	9,545	534,520		-		-	534,520
STS 강관 용접	D 200	개소	25	16,061	401,525		-		-	401,525
STS 강관 용접	D 300	개소	64	30,953	1,980,992		-		-	1,980,992
STS 강관 용접	D 350	개소	69	34,560	2,384,640		-		-	2,384,640
STS 강관 용접	D 400	개소	16	39,495	631,920		-		-	631,920
STS 강관 용접	D 450	개소	16	44,434	710,944		7,612,764		-	8,323,708
관보온 (고무발포재) 13t	D 80	M	85	6,961	591,685	17,696	1,504,160		-	2,095,845
관보온 (고무발포재) 13t	D 100	M	3	7,616	22,848	21,242	63,726		-	86,574
관보온 (고무발포재) 19t	D 65	M	93	7,663	712,659	16,334	1,519,062		-	2,231,721
관보온 (고무발포재) 19t	D 100	M	94	9,939	934,266	21,242	1,996,748		-	2,931,014
관보온 (고무발포재) 19t	D 125	M	44	11,483	505,252	23,689	1,042,316		-	1,547,568
관보온 (고무발포재) 19t	D 200	M	69	16,127	1,112,763	30,901	2,132,169		-	3,244,932
관보온 (고무발포재) 19t	D 300	M	40	22,336	893,440	42,339	1,693,560		-	2,587,000
관보온 (고무발포재) 19t	D 350	M	88	24,710	2,174,480	48,047	4,228,136		-	6,402,616
관보온 (고무발포재) 19t	D 400	M	65	27,900	1,813,500	52,954	3,442,010		-	5,255,510

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
관보온 (고무발포재) 19t	D 450	M	72		-		-		-	-
관보온(PERLITE) 50t	D 100	M	128	13,216	1,691,648	35,653	4,563,584		-	6,255,232
관보온(PERLITE) 50t	D 150	M	40	16,760	670,400	39,199	1,567,960		-	2,238,360
밸브보온(고무발포) 13t	D 50	개소	2	6,146	12,292	43,929	87,858		-	100,150
밸브보온(고무발포) 19t	D 50	개소	8	7,753	62,024	43,929	351,432		-	413,456
밸브보온(PERLITE) 50t	D 50	개소	2	8,901	17,802	74,130	148,260		-	166,062
엘보보온 13t	D 80	개소	6	6,453	38,718	8,015	48,090		-	86,808
엘보보온 13t	D 100	개소	6	8,024	48,144	12,605	75,630		-	123,774
엘보보온 19t	D 65	개소	14	6,754	94,556	6,165	86,310		-	180,866
엘보보온 19t	D 100	개소	13	8,874	115,362	12,605	163,865		-	279,227
엘보보온 19t	D 125	개소	8	10,465	83,720	17,953	143,624		-	227,344
엘보보온 19t	D 200	개소	6	20,504	123,024	36,977	221,862		-	344,886
엘보보온 19t	D 300	개소	10	35,967	359,670	75,715	757,150		-	1,116,820
엘보보온 19t	D 350	개소	8	45,481	363,848	100,038	800,304		-	1,164,152
엘보보온 19t	D 400	개소	2	49,187	98,374	126,075	252,150		-	350,524
엘보보온 19t	D 450	개소	6	66,546	399,276	156,237	937,422		-	1,336,698
엘보보온 25t	D 150	개소	10	12,379	123,790	22,955	229,550		-	353,340
엘보보온 25t	D 300	개소	5	35,967	179,835	75,715	378,575		-	558,410

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
엘보보온 50t	D 100	M	10	12,330	123,300	21,308	213,080		-	336,380
엘보보온 50t	D 150	M	3	20,516	61,548	37,395	112,185		-	173,733
후렌지접합(합) (STS316)	D350	EA	2	326,250	652,500	-	-		-	652,500
후렌지접합(절연) (STS316)	D 65	EA	1	111,246	111,246	-	-		-	111,246
후렌지접합(절연) (STS316)	D100	EA	1	159,640	159,640	-	-		-	159,640
후렌지접합(절연) (STS316)	D125	EA	1	246,378	246,378	-	-		-	246,378
후렌지접합(절연) (STS316)	D450	EA	1	1,490,168	1,490,168	-	-		-	1,490,168
후렌지접합(절연) (STS316)	D 65	EA	1	170,586	170,586	-	-		-	170,586
후렌지접합(절연) (STS316)	D100	EA	1	308,720	308,720	-	-		-	308,720
후렌지접합(절연) (STS316)	D450	EA	1	3,797,928	3,797,928	-	-		-	3,797,928
SHOP DRAWING	중급1인x 90일	M/D	90		-	96,387	8,674,830		-	8,674,830
잡재료비	주자재의 5%	식	1		-		-		-	2,367,120
시운전비	배관계통	M	1348		-	1,997	2,691,956		-	2,691,956
시운전비	실내기기 (5000M2 이하)	식	1		-	614,584	614,584		-	614,584

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
CS CRADLE ANCHOR	D 65	EA	14	5,733	80,262	-	-		-	80,262
〃	D 80	EA	10	5,733	57,330	-	-		-	57,330
〃	D100	EA	27	5,733	154,791	-	-		-	154,791
〃	D125	EA	8	6,628	53,024	-	-		-	53,024
〃	D150	EA	4	6,628	26,512	-	-		-	26,512
〃	D200	EA	10	7,435	74,350	-	-		-	74,350
〃	D300	EA	24	7,435	178,440	-	-		-	178,440
〃	D350	EA	11	10,833	119,163	-	-		-	119,163
〃	D400	EA	9	10,833	97,497	-	-		-	97,497
〃	D450	EA	12	10,833	129,996	-	-		-	129,996
CG CRADLE ANCHOR	D 65	EA	6	5,733	34,398	-	-		-	34,398
〃	D 80	EA	5	5,733	28,665	-	-		-	28,665
〃	D100	EA	11	5,733	63,063	-	-		-	63,063
〃	D125	EA	3	6,628	19,884	-	-		-	19,884
〃	D200	EA	5	7,435	37,175	-	-		-	37,175
〃	D300	EA	10	7,435	74,350	-	-		-	74,350
〃	D350	EA	4	10,833	43,332	-	-		-	43,332
〃	D400	EA	4	10,833	43,332	-	-		-	43,332
〃	D450	EA	4	10,833	43,332	-	-		-	43,332
D3 ANCHOR SHOE	D 50	EA	1	37,531	37,531	-	-		-	37,531
〃	D 65	EA	1	37,531	37,531	-	-		-	37,531

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
〃	D150	EA	1	58,324	58,324	-	-		-	58,324
〃	D350	EA	2	72,290	144,580	-	-		-	144,580
DA3 ANCHOR SHOE	D100	EA	2	37,531	75,062	-	-		-	75,062
〃	D150	EA	1	58,324	58,324	-	-		-	58,324
DA5 ANCHOR SHOE	D 80	EA	1	37,531	37,531	-	-		-	37,531
〃	D100	EA	1	37,531	37,531	-	-		-	37,531
〃	D200	EA	1	72,290	72,290	-	-		-	72,290
〃	D300	EA	4	72,290	289,160	-	-		-	289,160
〃	D350	EA	2	72,290	144,580	-	-		-	144,580
G3 ANCHOR SHOE	D100	EA	14	37,531	525,434	-	-		-	525,434
〃	D150	EA	13	58,324	758,212	-	-		-	758,212
S3 ANCHOR SHOE	D100	EA	8	37,531	300,248	-	-		-	300,248
〃	D150	EA	6	58,324	349,944	-	-		-	349,944
TR4 TRUNNIONS	D 65	EA	1	23,585	23,585	13,075	13,075		-	36,660
〃	D100	EA	4	36,149	144,596	17,696	70,784		-	215,380
〃	D125	EA	4	46,623	186,492	21,242	84,968		-	271,460
〃	D150	EA	2	46,623	93,246	21,242	42,484		-	135,730
DS2 DUMMY SUPPORT	D100	EA	2	41,645	83,290	17,696	35,392		-	118,682

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
DS3 DUMMY SUPPORT	D 50	EA	1	26,331	26,331	13,075	13,075		-	39,406
〃	D 65	EA	1	26,331	26,331	13,075	13,075		-	39,406
〃	D150	EA	1	54,508	54,508	21,242	21,242		-	75,750
DS4 DUMMY SUPPORT	D100	EA	2	41,645	83,290	17,696	35,392		-	118,682
〃	D150	EA	2	54,508	109,016	21,242	42,484		-	151,500
DS5 DUMMY SUPPORT	D 65	EA	4	26,331	105,324	13,075	52,300		-	157,624
〃	D100	EA	4	41,645	166,580	17,696	70,784		-	237,364
〃	D125	EA	2	54,508	109,016	21,242	42,484		-	151,500
GB BARE PIPE GUIDES	D 50	EA	5	17,498	87,490	-	-		-	87,490
〃	D 65	EA	5	17,498	87,490	-	-		-	87,490
〃	D150	EA	5	26,227	131,135	-	-		-	131,135
〃	D350	EA	8	56,583	452,664	-	-		-	452,664
계					194,848,272		277,796,233		-	472,644,505

(2) 덕트공사

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				금 액	단 가	금 액	단 가	단가	금액
010301 공조덕트설치공사
덕트제작설치	#26 (0.5T)	M2	1823	5,893	10,742,939	9,921	18,085,983			28,828,922
덕트제작설치	#24 (0.6T)	M2	1517	6,139	9,312,863	10,443	15,842,031			25,154,894

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
덕트제작설치	#22 (0.8T)	M2	2564	6,854	17,573,656	11,226	28,783,464			46,357,120
덕트제작설치	#20 (1.0T)	M2	631	7,845	4,950,195	13,315	8,401,765			13,351,960
덕트제작설치	#18 (1.2T)	M2	25	9,142	228,550	15,142	378,550			607,100
덕트제작설치	#14 (1.6T)	M2	35	14,342	501,970	19,581	685,335			1,187,305
STS덕트제작설치	#26 (0.5T)	M2	144	22,798	3,282,912	16,970	2,443,680			5,726,592
각형덕트보온	은박지	M2	2992	2,357	7,052,144	14,343	42,914,256			49,966,400
조합페인트칠	함석면2회	M2	1547	648	1,002,456	835	1,291,745			2,294,201
F.V.D W/FUSE	1500x450	EA	1	46,275	46,275					46,275
F.V.D W/FUSE	1000x600	EA	1	41,400	41,400					41,400
F.V.D W/FUSE	1000x450	EA	1	31,650	31,650					31,650
F.V.D W/FUSE	1000x550	EA	1	38,150	38,150					38,150
F.V.D W/FUSE	1100x550	EA	1	41,725	41,725					41,725
F.V.D W/FUSE	1400x550	EA	1	52,450	52,450					52,450
F.V.D W/FUSE	1700x550	EA	1	63,175	63,175					63,175
F.V.D W/FUSE	2200x550	EA	1	81,050	81,050					81,050
F.V.D W/FUSE	300x 200	EA	3	9,400	28,200					28,200
F.V.D W/FUSE	350x 175	EA	1	9,400	9,400					9,400
F.V.D W/FUSE	400x 175	EA	2	9,400	18,800					18,800
F.V.D W/FUSE	400x 200	EA	3	9,400	28,200					28,200
F.V.D W/FUSE	450x 175	EA	2	9,400	18,800					18,800
F.V.D W/FUSE	450x 200	EA	3	9,400	28,200					28,200

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
F.V.D W/FUSE	450x 250	EA	1	9,713	9,713					9,713
F.V.D W/FUSE	450x 400	EA	1	14,100	14,100					14,100
F.V.D W/FUSE	500x 175	EA	1	8,088	8,088					8,088
F.V.D W/FUSE	550x 150	EA	2	9,400	18,800					18,800
F.V.D W/FUSE	550x 350	EA	1	14,913	14,913					14,913
F.V.D W/FUSE	600x 175	EA	5	9,225	46,125					46,125
F.V.D W/FUSE	600x 400	EA	1	18,000	18,000					18,000
F.V.D W/FUSE	700x 400	EA	1	20,600	20,600					20,600
F.V.D W/FUSE	750x 800	EA	1	41,400	41,400					41,400
F.V.D W/FUSE	800x 400	EA	1	23,200	23,200					23,200
F.V.D W/FUSE	850x 450	EA	1	27,263	27,263					27,263
F.V.D W/FUSE	900x 500	EA	1	31,650	31,650					31,650
F.V.D W/FUSE	900x 900	EA	1	55,050	55,050					55,050
F.V.D W/FUSE	950x 500	EA	1	33,275	33,275					33,275
F.V.D W/FUSE	200x 200	EA	1	14,400	14,400					14,400
F.V.D W/FUSE	2200x550	EA		81,050						81,050
F.V.D W/FUSE	1550x550	EA		57,813						57,813
F.V.D W/FUSE	1400x550	EA		52,450						52,450
F.V.D W/FUSE	1200x450	EA		37,500						37,500
F.V.D W/FUSE	900x 900	EA		55,050						55,050
F.V.D W/FUSE	850x 450	EA		27,263						27,263

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
F.V.D W/FUSE	750x 800	EA		41,400						41,400
F . D W/FUSE	1000x1000	EA	1	67,400	67,400					67,400
F . D W/FUSE	1000x550	EA	1	38,150	38,150					38,150
F . D W/FUSE	1100x450	EA	2	34,575	69,150					69,1505
F . D W/FUSE	1400x550	EA	2	52,450	104,900					104,900
F . D W/FUSE	200x 150	EA	4	9,400	37,600					37,600
F . D W/FUSE	2300x1900	EA	2	286,450	572,900					572,900
F . D W/FUSE	300x 175	EA	1	9,400	9,400					9,400
F . D W/FUSE	350x 175	EA	1	9,400	9,400					9,400
F . D W/FUSE	400x 175	EA	1	9,400	9,400					9,400
F . D W/FUSE	400x 250	EA	1	9,400	9,400					9,400
F . D W/FUSE	450x 200	EA		8,250
F . D W/FUSE	500x 250	EA	1	10,525	10,525					10,525
F . D W/FUSE	600x 300	EA	2	14,100	28,200					28,200
F . D W/FUSE	650x 175	EA	1	9,794	9,794					9,794
F . D W/FUSE	650x 350	EA	4	17,188	68,752					68,752
F . D W/FUSE	700x 400	EA	1	20,600	20,600					20,600
F . D W/FUSE	800x 400	EA	2	23,200	46,400					46,400
F . D W/FUSE	850x 400	EA	2	24,500	49,000					49,000
F . D W/FUSE	900x 750	EA	2	46,275	92,550					92,550
F . D (STS 1.5t)	600x 350	EA	1	63,000	63,000					63,000

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
M.F.D (STL)	300x 200	EA	1	7,000	7,000					7,000
M.F.D (STL)	400x 200	EA	1	7,000	7,000					7,000
M.F.D (STL)	400x 300	EA	1	7,800	7,800					7,800
M.F.D (STL)	450x 200	EA	1	7,000	7,000					7,000
M.F.D (STL)	700x 400	EA	1	18,200	18,200					18,200
M.F.D (STL) W/모타	1100x500	EA	1	78,750	78,750					78,750
M.F.D (STL) W/모타	1100x450	EA	1	75,175	75,175					75,175
V . D (STL)	200x 100	EA	18	7,000	126,000					126,000
V . D (STL)	200x 150	EA	60	7,000	420,000					420,000
V . D (STL)	200x 200	EA	3	7,000	21,000					21,000
V . D (STL)	250x 150	EA	18	7,000	126,000					126,000
V . D (STL)	250x 200	EA	24	7,000	168,000					168,000
V . D (STL)	250x 250	EA	1	7,000	7,000					7,000
V . D (STL)	300x 150	EA	33	7,000	231,000					231,000
V . D (STL)	300x 200	EA	30	7,000	210,000					210,000
V . D (STL)	300x 250	EA	4	7,000	28,000					28,000
V . D (STL)	350x 150	EA	8	7,000	56,000					56,000
V . D (STL)	350x 200	EA	7	7,000	49,000					49,000
V . D (STL)	350x 250	EA	6	7,000	42,000					42,000
V . D (STL)	350x 300	EA		7,000

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
V . D (STL)	400x 150	EA	4	7,000	28,000					28,000
V . D (STL)	400x 200	EA	8	7,000	56,000					56,000
V . D (STL)	400x 250	EA	3	7,000	21,000					21,000
V . D (STL)	450x 200	EA	6	7,000	42,000					42,000
V . D (STL)	450x 250	EA	7	7,313	51,191					51,191
V . D (STL)	500x 250	EA	4	8,125	32,500					32,500
V . D (STL)	500x 300	EA	2	9,750	19,500					19,500
V . D (STL)	550x 250	EA	2	8,938	17,876					17,876
V . D (STL)	550x 300	EA	4	10,725	42,900					42,900
V . D (STL)	600x 300	EA	1	11,700	11,700					11,700
V . D (STL)	600x 350	EA	1	13,650	13,650					13,650
V . D (STL)	650x 350	EA	1	14,788	14,788					14,788
V . D (STL)	650x 400	EA	1	16,900	16,900					16,900
V . D (STL)	700x 350	EA	1	15,925	15,925					15,925
V . D (STL)	700x 400	EA	2	18,200	36,400					36,400
V . D (STL)	950x 450	EA	1	27,788	27,788					27,788
V . D (STL)	1100x450	EA	1	32,175	32,175					32,175
V . D (STS 1.5t)	600x 350	EA	2	63,000	126,000					126,000
V . D (STS)	200x 200	EA	1	12,000	12,000					12,000
P.R.D (STL)	1100x500	EA	2	92,750	185,500					185,500
T . V	1000x1000	EA	4	115,000	460,000					460,000

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
T . V	1000x1100	EA	1	126,500	126,500					126,500
T . V	1000x450	EA	1	51,750	51,750					51,750
T . V	1200x450	EA	1	62,100	62,100					62,100
T . V	1800x600	EA	1	124,200	124,200					124,200
T . V	750x 800	EA	1	69,000	69,000					69,000
GRILLE (AL)	1000x650	EA	2	58,500	117,000					117,000
GRILLE (AL)	1000x700	EA	3	63,000	189,000					189,000
GRILLE (AL)	600x 450	EA	1	24,300	24,300					24,300
GRILLE (AL)	650x 400	EA	4	23,400	93,600					93,600
REGISTER (AL)	1100x700	EA	8	115,500	924,000					924,000
REGISTER (AL)	1000x550	EA	12	82,500	990,000					990,000
REGISTER (AL)	200x 150	EA	29	15,000	435,000					435,000
REGISTER (AL)	250x 150	EA	15	15,000	225,000					225,000
REGISTER (AL)	250x 200	EA	6	15,000	90,000					90,000
REGISTER (AL)	250x 250	EA	14	15,000	210,000					210,000
REGISTER (AL)	250x 400	EA	6	15,000	90,000					90,000
REGISTER (AL)	300x 250	EA	1	15,000	15,000					15,000
REGISTER (AL)	350x 250	EA	4	15,000	60,000					60,000
REGISTER (AL)	350x 300	EA	2	15,750	31,500					31,500
REGISTER (AL)	400x 300	EA	4	18,000	72,000					72,000
REGISTER (AL)	450x 250	EA	10	16,875	168,750					168,750

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
REGISTER (AL)	500x 250	EA	7	18,750	131,250					18,750
REGISTER (AL)	600x 400	EA	3	36,000	108,000					36,000
REGISTER (AL)	650x 400	EA	1	39,000	39,000					39,000
REGISTER (AL)	700x 550	EA	2	57,750	115,500					115,500
REGISTER (AL)	800x 500	EA	10	60,000	600,000					600,000
LOUVER (AL)	550x 300	EA	8	24,750	198,000					198,000
SOUND CHAMBER	3900x1800x850	EA	1	1,376,340	1,376,340					1,376,340
SOUND CHAMBER	2600x1500x850	EA	1	856,660	856,660					856,660
SOUND CHAMBER	2400x1400x900	EA	1	786,480	786,480					786,480
SOUND CHAMBER	3400x2100x850	EA	1	1,370,540	1,370,540					1,370,540
SOUND CHAMBER	1000x1200x800	EA	1	343,360	343,360					343,360
SOUND CHAMBER	1700x1200x1400	EA	1	707,600	707,600					707,600
SOUND CHAMBER	2500x1400x1400	EA	1	1,039,360	1,039,360					1,039,360
주방후드(식기본형)	1200x950x 600		1	541,800	541,800					541,800
사각디퓨져 (STL)	ND125	EA	191	8,500	1,623,500					1,623,500
사각디퓨져 (STL)	ND150	EA	161	8,500	1,368,500					1,368,500
사각디퓨져 (STL)	ND200	EA	1	8,500	8,500					8,500

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
원형디퓨져 (STL)	ND125	EA	44	9,500	418,000					418,000
원형디퓨져 (STL)	ND150	EA	72	9,500	684,000					684,000
노즐디퓨져 (STL)	ND150	EA	39	11,400	444,600					444,600
T.L.D W/CHAM	1200L	EA	84	26,600	2,234,400					2,234,400
후렉시블호스 (보온)	D125	M	311	3,050	948,550					948,550
후렉시블호스 (보온)	D150	M	476	3,660	1,742,160					1,742,160
후렉시블호스 (무)	D125	M	60	1,350	81,000					81,000
후렉시블호스 (무)	D150	M	40	1,620	64,800					64,800
후렉시블호스 (무)	D200	M	1	2,160	2,160					2,160
STS BAND	D125	EA	494	320	158,080					158,080
STS BAND	D150	EA	685	330	226,050					226,050
STS BAND	D200	EA	2	390	780					780
닥트스리브제작	거푸집1회	M2	33.1	11,002	364,166	22,644	749,516			1,113,682
캔버스제작설치	3.2T	M2	53.34	4,500	240,030					240,030
동망	# 24	M2	38.4	11,000	422,400					422,400
점검구	300x 200	EA	18	7,000	126,000					126,000
점검구	200x 200	EA	68	7,000	476,000					476,000
핸 들	F.V.D	EA	41	11,000	451,000					451,000
휀주위닥트		LS	1	1,000,000	1,000,000					1,000,000
노무비	덕트공	인	989.5			26,108	25,833,866			25,833,866
노임할증	노 %	식	1			258,605	258,605			258,605
공구손료	노3%	식	1	775,249	775,249					775,249
합 계					102,689,741		146,528,796			249,218,537

(3) 창호공사

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금 액	단가	금액
0112 창호공사
FSD-1	2600*3400	개소	1	645,320	645,320	0	0	0	0	645,320
FSD-2	2500*2400	개소	1	522,000	522,000	0	0	0	0	522,000
FSD-3	2400*3400	개소	1	734,400	734,400	0	0	0	0	734,400
FSD-4A	1800*2100	개소	2	275,940	551,880	0	0	0	0	551,880
FSD-4B	1800*2100	개소	1	340,200	340,200	0	0	0	0	340,200
FSD-5	2600*2400	개소	1	455,520	455,520	0	0	0	0	455,520
FSD-6	2400*2400	개소	1	420,480	420,480	0	0	0	0	420,480
FSD-7	1000*2100	개소	2	210,000	420,000	0	0	0	0	420,000
SD-1A	2200*2100	개소	1	337,260	337,260	0	0	0	0	337,260
SD-1B	2200*2100	개소	1	415,800	415,800	0	0	0	0	415,800
SD-2A	1800*2100	개소	1	275,940	275,940	0	0	0	0	275,940
SD-2B	1800*2100	개소	2	340,200	680,400	0	0	0	0	680,400
SD-3	1800*2100	개소	16	272,160	4,354,560	0	0	0	0	4,354,560
SD-4	1800*2000	개소	1	307,680	307,680	0	0	0	0	307,680
SD-5A	1000*2100	개소	1	210,000	210,000	0	0	0	0	210,000
SD-5B	1000*2100	개소	5	186,900	934,500	0	0	0	0	934,500
SD-5C	1000*2100	개소	3	186,900	560,700	0	0	0	0	560,700
SD-6	750*2100	개소	2	114,975	229,950	0	0	0	0	229,950
SD-7	750*1500	개소	2	79,875	159,750	0	0	0	0	159,750
SD-8	2300*2700	개소	1	465,750	465,750	0	0	0	0	465,750
SD-9	2400*2700	개소	1	583,200	583,200	0	0	0	0	583,200
SSD-1	6400*2600*3600	개소	1	4,571,850	4,571,850	0	0	0	0	4,571,850
자동문	양개	조	2	1,500,000	3,000,000	0	0	0	0	3,000,000
SSD-2	1100*2000	개소	1	210,180	210,180	0	0	0	0	210,180
SSD-3	5100*3600	개소	1	1,768,894	1,768,894	0	0	0	0	1,768,894
SSD-4	4300*3600	개소	1	1,213,571	1,213,571	0	0	0	0	1,213,571
SSD-5	1985*3600	개소	1	681,642	681,642	0	0	0	0	681,642

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금 액	단가	금액
SSD-6	3100*3600	개소	1	793,130	793,130	0	0	0	0	793,130
ATD-1	940*2300	개소	2	1,500,000	3,000,000	0	0	0	0	3,000,000
SPD-1	3000*3600	개소	1	11,820,000	11,820,000	0	0	0	0	11,820,000
SPD-2	3100*3000	개소	1	10,180,000	10,180,000	0	0	0	0	10,180,000
SSF-1A	1800*2400	개소	1	320,100	320,100	0	0	0	0	320,100
SSF-1B	1800*2400	개소	1	425,040	425,040	0	0	0	0	425,040
SSW-1A	2300*3600	개소	1	878,891	878,891	0	0	0	0	878,891
SSW-1B	2350*3600	개소	1	889,686	889,686	0	0	0	0	889,686
GB-1	6850*2700	개소	1	647,490	647,490	0	0	0	0	647,490
GB-2	6850*1800	개소	1	586,470	586,470	0	0	0	0	586,470
CAW-1A(100MM SL)	6600*3000(120.6KG) 불소코팅	개소	3	1,213,236	3,639,708	0	0	0	0	3,639,708
CAW-1B(100MM SL)	6550*3000(120.2KG) 불소코팅	개소	1	1,209,212	1,209,212	0	0	0	0	1,209,212
CAW-1C (100MM SL)	6300*3000(117.8KG) 불소코팅	개소	1	1,185,068	1,185,068	0	0	0	0	1,185,068
CAW-2A(100MM SL)	1750*3000(35.3KG) 불소코팅	개소	1	355,118	355,118	0	0	0	0	355,118
CAW-2B(100MM SL)	1600*3000(33.9KG) 불소코팅	개소	1	341,034	341,034	0	0	0	0	341,034
CAW-3A(100MM SL)	6600*900 (43.2KG) 불소코팅	개소	1	434,592	434,592	0	0	0	0	434,592
CAW-3B(100MM SL)	6600*1200(57.6KG) 불소코팅	개소	1	579,456	579,456	0	0	0	0	579,456
CAW-4 (100MM SL)	2400*1200(20.1KG) 불소코팅	개소	1	202,206	202,206	0	0	0	0	202,206
CAW-5 (100MM FIX)	2400*1200(13.3KG) 불소코팅	개소	1	118,237	118,237	0	0	0	0	118,237

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금 액	단가	금액
CAW-6 (120MM 2TT)	4800*1800 불소코팅	개소	1	2,260,770	2,260,770	0	0	0	0	2,260,770
CAW-7 (120MM 2TT)	4150*1800 불소코팅	개소	2	2,092,740	4,185,480	0	0	0	0	4,185,480
CAW-8 (100MM FIX+PJ)	2700*2100(121.5KG) 불소코팅	개소	2	1,458,000	2,916,000	0	0	0	0	2,916,000
CAW-9A(120MM 2TT)	6700*2700 불소코팅	개소	8	3,178,900	25,431,200	0	0	0	0	25,431,200
CAW-9B(120MM 2TT)	6400*2700 불소코팅	개소	1	3,139,600	3,139,600	0	0	0	0	3,139,600
CAW-10(100MM FIX)	3000*1200(36.0KG) 불소코팅	개소	2	320,040	640,080	0	0	0	0	640,080
CAW-11(100MM FIX)	1800*1800(28.1KG) 불소코팅	개소	6	249,809	1,498,854	0	0	0	0	1,498,854
CAW-12A(100MM FIX)	3130*900 (29.5KG) 불소코팅	개소	1	262,255	262,255	0	0	0	0	262,255
CAW-12B(100MM FIX)	2495*900 (25.1KG) 불소코팅	개소	1	223,139	223,139	0	0	0	0	223,139
CAW-13A(100MM FIX)	1550*900 (18.6KG) 불소코팅	개소	2	165,354	330,708	0	0	0	0	330,708
CAW-13B(100MM FIX)	1250*900 (16.5KG) 불소코팅	개소	2	146,685	293,370	0	0	0	0	293,370
CAW-14A(100MM PJ)	4400*900 (124.8KG) 불소코팅	개소	1	1,497,600	1,497,600	0	0	0	0	1,497,600
CAW-14B(100MM PJ)	4150*900 (120.6KG) 불소코팅	개소	2	1,447,200	2,894,400	0	0	0	0	2,894,400
CAW-15(100MM PJ)	4800*900 (135.9KG) 불소코팅	개소	1	1,630,800	1,630,800	0	0	0	0	1,630,800

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금 액	단가	금액
CAW-16A(120MM 2TT)	6700*1800 불소코팅	개소	8	2,540,890	20,327,120	0	0	0	0	20,327,120
CAW-16B(120MM 2TT)	6400*1150 불소코팅	개소	2	2,513,990	5,027,980	0	0	0	0	5,027,980
CAW-17(120MM FIX)	7800*3800(225.8KG) 불소코팅	개소	1	2,007,362	2,007,362	0	0	0	0	2,007,362
CAW-18(120MM FIX+PJ)	7800*3800(337.7KG) 불소코팅	개소	3	4,052,400	12,157,200	0	0	0	0	12,157,200
CAW-19(120MM FIX+PJ)	3550*3800(161.4KG) 불소코팅	개소	2	1,936,800	3,873,600	0	0	0	0	3,873,600
CAW-20(120MM FIX)	9440*3800(277.5KG) 불소코팅	개소	1	2,466,975	2,466,975	0	0	0	0	2,466,975
CAW-21(120MM FIX+PJ)	9440*3800(419.7KG) 불소코팅	개소	1	5,036,400	5,036,400	0	0	0	0	5,036,400
CAW-22(150MM FIX+PJ,커턴월)	4200*13200(789.7KG) 불소코팅	개소	1	9,775,440	9,775,440	0	0	0	0	9,775,440
CAW-23(150MM FIX+PJ,커턴월)	4300*12000(740.1KG) 불소코팅	개소	1	9,154,760	9,154,760	0	0	0	0	9,154,760
AG-1A (100MM)	6600*900 (74.2KG) 불소코팅	개소	5	659,638	3,298,190	0	0	0	0	3,298,190
AG-1B (100MM)	6300*900 (71.1KG) 불소코팅	개소	1	632,079	632,079	0	0	0	0	632,079
AG-2 (100MM)	3300*900 (37.8KG) 불소코팅	개소	1	336,042	336,042	0	0	0	0	336,042
AG-4 (100MM)	2350*1600(45.4KG) 불소코팅	개소	8	403,606	3,228,848	0	0	0	0	3,228,848

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금 액	단가	금액
AG-5 (100MM)	1650*1600(34.1KG) 불소코팅	개소	12	303,149	3,637,788	0	0	0	0	3,637,788
AG-6 (100MM)	2350*1600(47.9KG) 불소코팅	개소	4	425,831	1,703,324	0	0	0	0	1,703,324
AG-7 (100MM)	3300*1000(42.0KG) 불소코팅	개소	1	373,380	373,380	0	0	0	0	373,380
AG-8 (100MM)	500*200 (2.8KG) 불소코팅	개소	1	24,892	24,892	0	0	0	0	24,892
AG-9 (100MM)	3000*1600(59.3KG) 불소코팅	개소	1	527,177	527,177	0	0	0	0	527,177
강화유리문	투명, 12mm*0.9*2.25m	개	4	140,000	560,000	0	0	0	0	560,000
강화유리문	투명, 12mm*0.9*2.5m	개	2	180,000	360,000	0	0	0	0	360,000
강화유리문	투명, 12mm*1.0*2.25m	개	2	160,000	320,000	0	0	0	0	320,000
강화유리문	컬러, 12mm* 1.086*2.1m	개	1	170,000	170,000	0	0	0	0	170,000
강화유리문	컬러, 12mm* 1.175*2.1m	개	2	190,000	380,000	0	0	0	0	380,000
후로아힌지설치		개소	11	47,325	520,575	10,852	119,372	0	0	639,947
도아체크달기 (강재)	방화용	개소	18	39,211	705,798	7,060	127,080	0	0	832,878
도아체크달기(강재)	일반용	개소	34	18,211	619,174	7,060	240,040	0	0	859,214
도아록설치	철문용	개소	47	9,026	424,222	898	42,206	0	0	466,428

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금 액	단가	금액
도아록설치	공정	개소	32	4,126	132,032	898	28,736	0	0	160,768
철제정첩	4"	개	50	1,500	75,000	0	0	0	0	75,000
피벗힌지	140kg이하 (K1400)	조	65	16,000	1,040,000	0	0	0	0	1,040,000
AL방충망(미서기,후레임포함)	불소코팅, 시공도	M2	61	15,900	969,900	0	0	0	0	969,900
계					0		0		0	0

2) 미국

Ref	Description	Quantity	Units	Rate	Amount
	MECHANICAL ENGINEERING INSTALLATIONS
	PIPEWORK
A	Soil, waste and vent pipework.
	Soil, waste and vent pipework and fittings, complete
	with all necessary fixings, fittings and accessories
1	160 mm	54	Mtrs	356.4	19,245.6
2	110 mm	28	Mtrs	249.5	6,986.0
3	80 mm dia	53	Mtrs	183.8	9,741.4
4	40 mm	27	Mtrs	137.1	3,701.7
5	32 mm	29	Mtrs	137.1	3,975.9
	Rainwater pipework
B	Rainwater pipework and fittings; complete with all
	necessary fixings, fittings and accessories
1	110 mm dia	35	Mtrs	145.0	5,075.0
	Domestic cold water pipework
C	Domestic cold water pipework and fittings; complete
	with all necessary fixings, fittings and accessories
1	15 mm dia Pipe	67	Mtrs	30.9	2,070.3
2	22 mm dia pipe	61	Mtrs	40.3	2,458.3
3	28 mm dia pipe	21	Mtrs	50.4	1,058.4
4	35 mm dia Pipe	9	Mtrs	73.8	664.2
5	42 mm dia pipe	7	Mtrs	86.7	606.9
6	54 mm dia pipe	23	Mtrs	114.4	2,631.2
7	67 mm dia pipe	10	Mtrs	156.5	1,565.0
8	67 mm dia pipe (U/G)	5	Mtrs	30.3	151.5
	Domestic hot water pipework
D	Domestic hot water pipework and fittings; complete
	with all necessary fixings, fittings and accessories
1	15 mm dia pipe	33	Mtrs	30.9	1,019.7
2	22 mm dia pipe	13	Mtrs	40.3	523.9
3	28 mm dia pipe	9	Mtrs	50.4	453.6
4	35 mm dia pipe	9	Mtrs	73.8	664.2
5	42 mm dia Pipe	9	Mtrs	86.7	780.3
	Refrigerant pipework
E	Refrigerant pipework and fittings; including jointing and
	fixing with clips	1	item	3,300.0	3,300.0
	Accessories
F	Soil, waste and vent accessories, including jointing
	to pipework
1	110 mm	2	No	113.3	226.6
2	80 mm	2	No	113.3	226.6
	Rainwater accessories; including jointing to pipework
G	100 mm Dia	2	No	541.2	1,082.4
			To Collection		68,208.7

Ref	Description	Quantity	Units	Rate	Amount
A	Domestic cold water accessories; including jointing to pipework
	Bronze gate valves to BS 5154 PN20, BSP screwed ds
1	15 mm dia	15	No	41.5	622.5
2	22 mm dia	5	No	45.9	229.5
3	28 mm dia	2	No	58.0	116.0
4	35 mm dia	18	No	73.4	1,321.2
5	42 mm dia	2	No	88.8	177.6
6	50 mm dia	5	No	126.2	631.0
7	Cast iron gate valves with internal fusion bonded epoxy
	lining to BS 5163, flanged PN16, c/w bi-metallic mating
	flanges 80 mm dia	1	No	798.8	798.8
8	Chrome plated bronze angle pattern valves with
	escutcheon plates at final connections to sanitaryware
	15mm dia	45	No	64.6	2,907.0
9	3 way ablution area constant temperature mixing valve
	with 42 mm dia	1	set	6,609.6	6,609.6
10	CP bib tap 15 mm	24	No	87.9	2,109.6
11	CP bib tap 22 mm	1	No	87.9	87.9
B	Domestic hot water accessories; including jointing to pipework
1	15 mm dia pipe	33	Mtrs	15.1	498.3
2	22 mm dia pipe	13	Mtrs	17.3	224.9
3	28 mm dia pipe	9	Mtrs	19.5	175.5
4	35 mm dia pipe	8	Mtrs	21.7	173.6
5	42 mm dia Pipe	8	Mtrs	22.3	178.4
	Bronze gate valves to BS 5154 PN20, BSP screwed
6	15 mm dia	1	No	41.5	41.5
7	22 mm dia	1	No	45.9	45.9
8	28 mm dia	1	No	58.0	58.0
C	Refrigerant accessories; including jonting to
	pipework	1	Item	-	included
D	Connecting to main pipelines	1	Item	-	included
	DUCTWORK Rectangular ductwork
E	Rectangular ductwork, including insulated supports, joints,
	fixings, bends, branches and associated accessories
1	Size 150 x 100	10	Mtrs	48.6	486.0
2	Size 150 x 150	19	Mtrs	58.3	1,107.7
3	Size 200 x 200	22	Mtrs	77.8	1,711.6
4	Size 200 x 200	13	Mtrs	77.8	1,011.4
5	Size 250 x 200	7	Mtrs	97.2	680.4
6	Size 300 x 225	7	Mtrs	102.1	714.7
7	Size 300 x 250	3	Mtrs	107.0	321.0
8	Size 350 x 250	13	Mtrs	116.7	1,517.1
9	Size 300 x 300	38	Mtrs	116.7	4,434.6
10	Size 350 x 350	27	Mtrs	136.1	3,674.7
11	Size 450 x 300	20	Mtrs	145.9	2,918.0
12	Size 500 x 450	28	Mtrs	203.8	5,706.4
			To Collection		73,424.5

Hai Phong TPP 2 × 300MW               BQ List(REV.1)                                    AUG. 2003

No.	Description	Specification	Unit	Q'ty	Unit Rate(US＄)				(US＄)
					Materials	Labors	Other's	Total	Amount
B	STG Area
B-1	Turbine Generator House with Control room
1	Piling works
1	Bored cast-in place pile 800mm dia.	L=25m, as per Tender Specification Clause 3.5.6, Volume 3.	pcs	294.0
2	Earth works
1	Excavation	As per Tender Specification Clause 3.5.1, Volume 3.	m3	19,453.0
2	Backfilling	As per TenderSpecification Clause 3.5.1, Volume 3.	m3	11,621.0
3	Soil disposal	As per Tender Specification Clause 3.5.1, Volume 3.	m3	7,832.0
4	Rubble subgrade	min.150mm thick	m3	792.4
5	Anti termite treatment	As per Tender Specification Clause 3.5.20, Volume 3.	lot	1.0
3	Concrete works
1	Moisture vapor barrier	0.12mm thick, as per Tender Specification Clause 3.5.5 and 3.5.22, Volume 3.	m2	5,282.8
2	Le-concrete	min. 50mm thick, Fc28=140 Kg/cm2, Cement type: Type-I ASTM C150. As per Tender Specification Clause 3.5.5, Volume 3.	m3	264.2
3	concrete	Fc28=240 Kg/cm2, Cement type: Type-I ASTM C150. As per Tender Specification Clause 3.5.5, Volume 3.	m3	6,947.5
4	Re-bar	Gr.60 ASTM A615 and Tender Specification Clause 3.5.5, Volume 3.	ton	684.9
5	Form work	As per ACI 347and Tender Specification Clause 3.5.5, Volume 3.	m2	24,316.0
6	Water stop	PVC 250mm width, as per Tender Specification Clause 3.5.5, Volume 3.	m	200.0
7	Waterproofing	Three coats of asphalt emulsion or three coats of coal tar pitch as per Tender Specification Clause 3.5.5, Volume 3.	m2	1,320.0
4	Steel works
1	Structural steel with paint	ASTM A36 or equivalent including erection/fabrication drawings, high strength friction bolt, anchor bolts and anchor ftame etc. as per Tender Specification Clause 3.5.8, Volume 3.	ton	1,940.0

No.	Description	Specification	Unit	Q'ty	Unit Rate(US＄)				(US＄)
					Materials	Labors	Other's	Total	Amount
2	Miscellaneous steel with galvanizing	ASTM A36 or equivalent including erection/fabrication drawings, bolt, anchor bolts, anchor frame etc. as per Tender Specification Clause 3.5.9, Volume 3.	ton	20.0
3	Galvanized steel grating (32mm thick)	ASTM A36 or equivalent including erection/fabrication drawings, bolt, anchor bolts, anchor frame etc. as per Tender Specification Clause 3.5.9, Volume 3.	m2	300.0
4	Deck-plate	1.6mm thick, 50mmH	m2	15,288.0
5	Floor finish works
1	Mortar with floor hardener	As per Tender Specification Clause 3.5.23, Volume 3.	m2	15,261.1
2	PVC tile	304mm×304mm×3mm thick, as per Tender Specification Clause 3.5.23, Volume 3.	m2	514.6
3	Anti-slip tile	As per Tender Specification Clause 3.5.23, Volume 3.	m2	28.5
4	Oil proof paint		m2	232.0
6	Base board works
1	Poly vinyl chloride	As per Tender Specification Clause 3.5.23, Volume 3.	m	244.0
2	Ceramic tile	As per Tender Specification Clause 3.5.23, Volume 3.	m	38.0
7	Wall finish works
1	Concrete hollow block (for internal)	100mm×200mm×400mm including mortar and reinforcing bar, as per Tender Specification Clause 3.5.21, Volume 3.	m2	2,176.0
2	Plaster on CHB/ Concrete (for internal)	As per Tender Specification Clause 3.5.24, Volume 3.	m2	4,352.0
3	Paint on plaster/ concrete (for external)	As per Tender Specification Clause 3.5.37, Volume 3.	m2	420.8
4	Paint on plaster/ concrete (for internal)	As per Tender Specification Clause 3.5.37, Volume 3.	m2	4,772.8
5	Galvanized steel sheet cladding	As per Tender Specification Clause 3.5.30, Volume 3.	m2	12,211.2
6	Mineral insulation	As per Tender Specification Clause 3.5.37, Volume 3.	m2	12,211.2
8	Ceiling finish works
1	Suspended acoustic board	As per Tender Specification Clause 3.5.27, Volume 3.	m2	82.6
2	Insulation	As per Tender Specification Clause 3.5.25, Volume 3.	m2	82.6
9	Roof finish works
1	Galvanized steel sheet roofing	As per Tender Specification Clause 3.5.30, Volume 3.	m2	3,920.0
2	Mineral insulation	As per Tender Specification Clause 3.5.30, Volume 3.	m2	3,920.0

No.	Description	Specification	Unit	Q'ty	Unit Rate(US＄)				(US＄)
					Materials	Labors	Other's	Total	Amount
3	Bituminous water- proofing membrane on concrete with mortar	As per Tender Specification Clause 3.5.36, Volume 3.	m2	2,570.0
4	Roof drain 150mm dia	As per Tender Specification Clause 3.5.30, Volume 3.	ea	12.0
5	Eaves gutter 350mm×350mm	As per Tender Specification Clause 3.5.36, Volume 3.	m	264.0
6	Downspout 150mm dia	As per Tender Specification Clause 3.5.36, Volume 3.	m	592.0
10	Door and window works
1	Steel roll-up shutter with paint	6m×6mH, as per Tender Specification Clause 3.5.29 and 3.5.32, Volume 3.	ea	1.0
2	Steel double swing door with paint	2m×3mH, as per Tender Specification Clause 3.5.29 and 3.5.32, Volume 3.	ea	3.0
3	Steel double swing door with paint	2m×2.5mH, as per Tender Specification Clause 3.5.29 and 3.5.32, Volume 3.	ea	10.0
4	Steel single swing door with paint	1m×2.5mH, as per Tender Specification Clause 3.5.29 and 3.5.32, Volume 3.	ea	37.0
5	Laminated toilet door	1m×2mH, as per Tender Specification Clause 3.5.26, 3.5.27 3.5.32 and 3.5.37, Volume 3.	ea	8.0
6	Aluminum sliding window with glass, insect screen	1.5m×1mH, as per Tender Specification Clause 3.5.28, 3.5.32, 3.5.33 and 3.5.34, Volume 3.	ea	80.0
7	Aluminum fixed window with double glass	2m×1mH, as per Tender Specification Clause 3.5.26, 3.5.27 3.5.32 and 3.5.37, Volume 3.	ea	2.0
8	Steel louver with paint	As per Tender Specification Clause 3.5.29, Volume 3.	m2	800.0
11	Plumbing works
1	Water closet with accessory	As per Tender Specification Clause 3.5.40, Volume 3.	ea	5.0
2	Urinal with accessory	As per Tender Specification Clause 3.5.40, Volume 3.	ea	4.0
3	Wash basin with accessory	As per Tender Specification Clause 3.5.36, Volume 3.	ea	5.0
4	Shower head with accessory	As per Tender Specification Clause 3.5.40, Volume 3.	ea	5.0
5	Piping system (water supply, drain, air) inc. floor drain, trap etc.	As per Tender Specification Clause 3.5.40, Volume 3.	lot	1.0
6	Septic Tank	As per local regulation	ea	1.0

3) 유럽

ABU DHABI		BILL OF QUANTITIES			B/N.	PAGE NO.
TRADE CENTER		HOTEL TOWERS
ABU DHABI, U.A.E.		MECHANICAL SERVICES			5	5/12/01
ITEM	ITEM DESCRIPTION		Q‘Y	UNIT	UNIT	TOTAL PRICE
REF.					RATE	UAE Dhms
	MECHANICAL SERVICES
	Unless otherwise stated, the work shall pertain to the design, supply, installation, testing, commissioning, warranty & maintenance of the following works. Where quantities have not been included, the contractor shall indicate the quantities as per the Tender Document.
	SECTION 15050 - PLUMBING AND FIRE PROTECTION BASIC MATERIALS AND METHODS
	General construction materials and methods for application with Mechanical installation as follows:
A.	Mechanical equipment nameplate data			Item		INCLUDED
B.	Miscellaneous metals for support of mechanical materials and equipment.			Item		INCLUDED
C.	Wood Grounds, mailers, blocking, fasteners and anchorage for support of mechanical materials and equipment.			Item		INCLUDED
D.	Joint Sealers for sealing around mechanical materials and equipment; and for sealing penetrations in fire and smoke barriers, floors and foundation walls.			Item		INCLUDED
E.	Access panels and doors in walls, ceillings and floors for access to mechanical materials and equipment.			Item		INCLUDED
F.	Excavation for underground utilities and services including underground piping(under the building and from building to utility connection), tanks, basins and equipment.			Item		N/A
	Additional Items
G.	The tenderer is to attach with this bill of quantities, any			Item		N/A
	additional items with quantities, enumerated or itemized
	and rates which are not previously included to complete
	the build up of the lump-sum tender price for this section
	of the works.Should the tenderer fail to insert any items
	here, it will be deemed that his lump-sum price for the
	tender includes all items either shown on the drawings
	and described in the specification or deemed necessary
	by the tenderer to develop the drawings and specification
	to represent the entire cost of the works and no subsequent
	subsequent claim for any additional item will be enertained.
		To Collection				0

ABU DHABI		BILL OF QUANTITIES			B/N.	PAGE NO.
TRADE CENTER		HOTEL TOWERS
ABU DHABI, U.A.E.		MECHANICAL SERVICES			5	5/12/02
ITEM	ITEM DESCRIPTION		Q'Y	UNIT	UNIT	TOTAL PRICE
REF.					RATE	UAE Dhms
	SECTION 15060 - HVAC PIPE AND PIPE FITTINGS
	Chilled water system piping complete with fittings including elbows, tees, reducers, unions, flanges and any other fittings required to make a complete system all as per specifications.
A.	25mm dia		30	m	2,058.	61,756
B.	32mm dia		38	m	63.47	24,309
C.	40mm dia		44	m	32.97	1,451
D.	50mm dia		15	m	39.66	6,187
E.	65mm dia		20	m	60.97	12,560
F.	80mm dia		18	m	72.57	13,208
G.	100mm dia		32	m	65.29	21,219
H.	150mm dia		14	m	168.11	23,535
I	Condenser water system piping complete with fittings including elbows, tees, reducers, unions, flanges and any other fittings required to make a complete system all as per .
J.	600mm dia		19	m	835.64	162,950
K.	Drain water system piping complete with fittings including elbows, tees, reducers, unions, flanges and any other fittings required to make a complete system all as per specifications.			Item		INCLUDED
	Additional Items
L.	The tenderer is to attach with this bill of quantities, any		1	Item		497,936
	additional items with quantities, enumerated or itemized
	and rates which are not previously included to complete
	the build up of the lump-sum tender price for this section
	of the works.Should the tenderer fail to insert any items
	here, it will be deemed that his lump-sum price for the
	tender includes all items either shown on the drawings
	and described in the specification or deemed necessary
	by the tenderer to develop the drawings and specification
	to represent the entire cost of the works and no
	subsequent claim for any additional item will be enertained.
	SECTION 15080 - HVAC PIPING SPECIALTIES
	HVAC piping specialties including fittings and connections all as per specifications.
A.	Air Vents		22	No.	38.63	8,576
B.	Relief Valves			No.		INCLUDED
		To Collection				833,686

4) 일본

(건축공사)

명 칭	적 요	수량	단위	단가	금액	비 고
5. 콘크리트공사
(1) 구체
보통콘크리트	재질, 강도, slump 기초부		㎥
보통콘크리트	재질, 강도, slump 軸部		㎥
보통콘크리트	재질, 강도, slump 土間		㎥
콘크리트타설		(1	㎥ 식)			(별지명세)
펌프압송		1	식			(별지명세)
(폭이음처리)		(1	m 식)			(별지명세)
(지수판)	재질, 치수		m
온도보정		1	식			(별지명세)
콘크리트발판		1	식			(별지명세)
계
(2) 외부마감
무근콘크리트	방수누름 材工共		㎥
계
(3) 내부마감
무근콘크리트	콘용 材工共		㎥
계

(  )는 필요에 따라 계상한다.

명 칭	적 요	수량	단위	단가	금액	비 고
7. 철골
(1) 본체철골
절판강판	규격, 판두께		t			소요수량
형강	규격, 형상, 치수		t			소요수량
box기둥	규격, 형상, 치수		t			소요수량
평강	규격, 치수		t			소요수량
환강	규격, 직경		t			소요수량
철골 scrap공제		▲ 1	식		▲
공장가공조립	용접재료 및 용접수간공		t			설계수량
공장도장	下地의 종별 강재면, 도금면 구분	( 1	㎡ 식)			(별지명세)
철골운반			t			설계수량
현장 建方			t			설계수량
高力 볼트류	규격, 형상, 치수, 재료비		t			수요수량
고력 볼트류 체결	규격, 형상, 치수		본			설계수량
현장용접	6 mm 환산		m			설계수량
현장도장		( 1	㎡ 식)			(별지명세)
계

(  )는 필요에 따라 계상한다.

명 칭	적 요	수량	단위	단가	금액	비 고
(2) 부대철골 등
철골계단	材工共	( 1	개소 식)			(별지명세)
커튼월취부 1차 fastener		( 1	개소 식)			(별지명세)
sleeve	직경, 길이	( 1	개소 식)			(별지명세)
anchor bolt	종별, 직경, 길이, 材工共		본
용접부시험	공장 및 현장 제3자 시험기관	( 1	개소 식)			(별지명세)
deck plate 등	형상, 두께, 材工共		㎡
(deck받이철물)			개소 (m)
외주콘크리트止	材工共		m
경량형강구조	볼트류, 材工共	1	식			(별지명세)
몰탈	사양, 치수	( 1	개소 식)			(별지명세)
stud bolt	재공공		본
(가설철물)		1	식			(별지명세)
철골발판		1	식			(별지명세)
계
(3) 내화피복
내화피복	사양, 성능, 부위		㎡
내화피복	사양, 성능		m
계

(  )는 필요에 따라 계상한다.

일본의 경우 건설공사 시행 시 실적공사비제도를 많이 활용하고 있으며 품목별로 단가에 대한 적용기준을 다음과 같이 정의하고 있다.

수량에 해당하는 단가는 기기·재료 등의 단가, 복합단가, 시장단가, 합성단가로

구분하며 각각의 정의는 다음과 같은 것이다.

① 기기 · 재료 등의 단가

기기단가는 설비기기의 가격이고, 재료단가는 전선, 배관재 등의 가격(노무비를 포함하지 않는다.)이다.

② 복합단가

단위량당의 재료비, 노무비, 잡 재료비, 기계기구경비, 하청경비 등의 조합에 의하여 계산된다.

③ 시장단가

품셈에 의한 일위대가 단가로 재료비, 노무비, 하청경비 등을 포함하는 단위 공사량당의 단가이다. 시장에서의 원청·하청사이의 거래가격을 파악하여 직접, 공사비의 적산에 이용하는 방식이다.

또, 구체적인 시장단가에 있어서는 계간발행의 물가자료에 게재되어 있다.

④ 합성단가

몇 개의 복합단가 및 시장단가를 조합하여 합성한 단가이다.

내역서는 종목별내역서, 과목별내역서, 중과목별내역서 및 세목별내역서로 구성되며 다음과 같이 정의한다.

① 종목별 내역서

종목별 내역서는 직접공사비, 공통비 및 부가세등 상당액을 기재한다. 또 직접공사비는 건물별, 옥외, 건축공사 등의 공사종목마다 구분하여 계상하여, 공통비(공통가설비·현장관리비·일반관리비 등) 및 부가세등 상당액을 각각 구분하고 기재한다. 공사종목의 구분은 설계도서에 의한다.

② 과목별 내역서

과목별 내역서는 설계도서의 공사종목 등을 표준 시방서에 의하여 직접공사비를 과목에 구분하여 그 과목의 금액을 기재한다.

③ 중과목별 내역서

중과목별 내역서는 과목별내역에 있어서 구분한 과목을 더욱 주요한 구성에 따라서 구분하고, 그 중과목의 금액을 기재한다. 공사내용 등에 의해 구분할 필요가 없는 경우는 생략할 수 있다.

④ 세목별 내역서

세목별 내역서는 각 과목 혹은 중과목에 속하는 세목마다 수량, 단위, 단가 및 금액을 기재한다.

공사비 산정은 다음과 같이 산정한다.

공사비

공사가격

공사원가

순공사비

직접공사비

공통가설비

현장관리비

일반관비리 등

부가세등 상당액

공통비

① 직접공사비

직접공사비는 공사목적물을 만들기 위해 직접 필요로 하는 비용이며, 공사종목마다 기재한다.

② 공통비

공통비는 공통가설비·현장관리비·일반관리비등으로 구성되어 있다. 직접공사비에 공통가설비와 현장관리비를 더한 것이 공사원가가 된다.

일반관리비 등은 일반관리비와 부가이익으로 구성되어 있고, 이것을 공사원가에 더한 것이 공사가격이 된다.

③ 부가세 등 상당액

부가세 등 상당액은 부가세 및 지방부가세 상당분으로 이루어지며 세율을 곱한 값으로 한다.

#부록2 공종별 표준화 내역서 작성(변경 전․후 대비)

(1) 배관 부속자재의 경우

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 304 (SCH 10)	D 50	M	98	11,940	1,170,120		-		-	1,170,120
〃	D 65	M	81	14,800	1,198,800		-		-	1,198,800
〃	D 150	M	81	36,990	2,996,190		-		-	2,996,190
〃	D 350	M	153	135,690	20,760,570		-		-	20,760,570
STS 316 (SCH 10)	D 65	M	47	21,784	1,023,848		-		-	1,023,848
〃	D 80	M	94	25,592	2,405,648		-		-	2,405,648
〃	D 100	M	128	33,096	4,236,288		-		-	4,236,288
〃	D 125	M	49	47,306	2,317,994		-		-	2,317,994
〃	D 150	M	45	56,140	2,526,300		-		-	2,526,300
〃	D 200	M	2	88,424	176,848		-		-	176,848
〃	D 300	M	17	156,968	2,668,456		-		-	2,668,456
〃	D 350	M	27	205,604	5,551,308		-		-	5,551,308
〃	D 400	M	72	235,354	16,945,488		-		-	16,945,488
〃	D 450	M	40	246,480	9,859,200		-		-	9,859,200
STS 316 (SCH 10)	D 65	M	56	22,040	1,234,240		-		-	1,234,240
〃	D 100	M	122	38160	4,655,520		-		-	4,655,520
〃	D 200	M	75	141590	10,619,250		-		-	10,619,250

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
〃	D 300	M	28	210560	5,895,680		-		-	5,895,680
〃	D 350	M	71	255945	18,172,095		-		-	18,172,095
〃	D 450	M	41	371,925	15,248,925		-		-	15,248,925
ELBOW (SCH80)	D 20	EA	9	5,170	46,530		-		-	46,530
ELBOW (SCH10)	D 50	EA	8	3,600	28,800		-		-	28,800
ELBOW (SCH10)	D 65	EA	6	5,730	34,380		-		-	34,380
〃	D 150	EA	14	32,980	461,720		-		-	461,720
〃	D 300	EA	3	184,050	552,150		-		-	552,150
〃	D 350	EA	6	241,500	1,449,000		-		-	1,449,000
ELBOW, (STS-316, SCH10)	D 65	EA	6	9,290	55,740		-		-	55,740
〃	D 80	EA	6	11,510	69,060		-		-	69,060
〃	D 100	EA	18	18,380	330,840		-		-	330,840
〃	D 125	EA	8	36,620	292,960		-		-	292,960
〃	D 150	EA	3	46,840	140,520		-		-	140,520
〃	D 200	EA	2	100,780	201,560		-		-	201,560
〃	D 300	EA	5	256,160	1,280,800		-		-	1,280,800
〃	D 350	EA	4	358,800	1,435,200		-		-	1,435,200
〃	D 400	EA	2	510,340	1,020,680		-		-	1,020,680
〃	D 450	EA	3	767,140	2,301,420		-		-	2,301,420
ELBOW, (STS-316, SCH20)	D 65	EA	8	11,330	90,640		-		-	90,640
〃	D 100	EA	10	24,250	242,500		-		-	242,500
〃	D 200	EA	4	179,240	716,960		-		-	716,960
〃	D 300	EA	5	334,130	1,670,650		-		-	1,670,650

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
〃	D 350	EA	2	635,140	1,270,280		-		-	1,270,280
〃	D 450	EA	3	1,141,430	3,424,290		-		-	3,424,290
ELBOW, (STS-304,	D 300	EA	2	146,010	292,020		-		-	292,020
“	D 100	EA	1	12,870	12,870		-		-	12,870
〃	D 350	EA	2	251,160	502,320		-		-	502,320
TEE, (STS-304,	D 50	EA	1	6,520	6,520		-		-	6,520
REDUCER(STS-316, SCH10)	D 350 x D 300	EA	1	154,910	154,910		-		-	154,910
〃	D 400 x D 350	EA	1	192,960	192,960		-		-	192,960
REDUCER(STS-316	D 350 x D300	EA	1	245,680	245,680		-		-	245,680
NIPPLE, (STS-316,	D 15	EA	1	3,280	3,280		-		-	3,280
〃	D 20	EA	10	4,300	43,000		-		-	43,000
NIPPLE, (STS-316,	D 15	EA	1	5,930	5,930		-		-	5,930
HALF COUPLIN	D 20	EA	8	3,040	24,320		-		-	24,320
PLUG (STS-316)	D 20	EA	9	3,030	27,270		-		-	27,270

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 304 (SCH 10)	D 50	M	98	11,940	1,170,120		-		-	1,170,120
〃	D 65	M	81	14,800	1,198,800		-		-	1,198,800

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
STS 304 (SCH 10)	D 150	M	81	36,990	2,996,190		-		-	2,996,190
〃	D 350	M	153	135,690	20,760,570		-		-	20,760,570
STS 316 (SCH 10)	D 65	M	47	21,784	1,023,848		-		-	1,023,848
〃	D 80	M	94	25,592	2,405,648		-		-	2,405,648
〃	D 100	M	128	33,096	4,236,288		-		-	4,236,288
〃	D 125	M	49	47,306	2,317,994		-		-	2,317,994
〃	D 150	M	45	56,140	2,526,300		-		-	2,526,300
〃	D 200	M	2	88,424	176,848		-		-	176,848
〃	D 300	M	17	156,968	2,668,456		-		-	2,668,456
〃	D 350	M	27	205,604	5,551,308		-		-	5,551,308
〃	D 400	M	72	235,354	16,945,488		-		-	16,945,488
〃	D 450	M	40	246,480	9,859,200		-		-	9,859,200
〃	D 65	M	56	22,040	1,234,240		-		-	1,234,240
〃	D 100	M	122	38160	4,655,520		-		-	4,655,520
〃	D 200	M	75	141590	10,619,250		-		-	10,619,250
〃	D 300	M	28	210560	5,895,680		-		-	5,895,680
〃	D 350	M	71	255945	18,172,095		-		-	18,172,095
〃	D 450	M	41	371,925	15,248,925		-		-	15,248,925
부속자재	주자재의14.4%	식	1	129,662,763	18,627,760		-		-	18,627,760

(2) 보온 부속자재의 경우

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
관보온 (고무발포재) 13t	D 80	M	85	6,961	591,685	17,696	1,504,160		-	2,095,845
관보온 (고무발포재) 13t	D 100	M	3	7,616	22,848	21,242	63,726		-	86,574
관보온 (고무발포재) 19t	D 65	M	93	7,663	712,659	16,334	1,519,062		-	2,231,721
관보온 (고무발포재) 19t	D 100	M	94	9,939	934,266	21,242	1,996,748		-	2,931,014
관보온 (고무발포재) 19t	D 125	M	44	11,483	505,252	23,689	1,042,316		-	1,547,568
관보온 (고무발포재) 19t	D 200	M	69	16,127	1,112,763	30,901	2,132,169		-	3,244,932
관보온 (고무발포재) 19t	D 300	M	40	22,336	893,440	42,339	1,693,560		-	2,587,000
관보온 (고무발포재) 19t	D 350	M	88	24,710	2,174,480	48,047	4,228,136		-	6,402,616
관보온 (고무발포재) 19t	D 400	M	65	27,900	1,813,500	52,954	3,442,010		-	5,255,510
관보온 (고무발포재) 19t	D 450	M	72		-		-		-	-
관보온(PERLITE) 50t	D 100	M	128	13,216	1,691,648	35,653	4,563,584		-	6,255,232
관보온(PERLITE) 50t	D 150	M	40	16,760	670,400	39,199	1,567,960		-	2,238,360
밸브보온(고무발포) 13t	D 50	개소	2	6,146	12,292	43,929	87,858		-	100,150

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
밸브보온(고무발포) 19t	D 50	개소	8	7,753	62,024	43,929	351,432		-	413,456
밸브보온(PERLITE) 50t	D 50	개소	2	8,901	17,802	74,130	148,260		-	166,062
엘보보온 13t	D 80	개소	6	6,453	38,718	8,015	48,090		-	86,808
엘보보온 13t	D 100	개소	6	8,024	48,144	12,605	75,630		-	123,774
엘보보온 19t	D 65	개소	14	6,754	94,556	6,165	86,310		-	180,866
엘보보온 19t	D 100	개소	13	8,874	115,362	12,605	163,865		-	279,227
엘보보온 19t	D 125	개소	8	10,465	83,720	17,953	143,624		-	227,344
엘보보온 19t	D 200	개소	6	20,504	123,024	36,977	221,862		-	344,886
엘보보온 19t	D 300	개소	10	35,967	359,670	75,715	757,150		-	1,116,820
엘보보온 19t	D 350	개소	8	45,481	363,848	100,038	800,304		-	1,164,152
엘보보온 19t	D 400	개소	2	49,187	98,374	126,075	252,150		-	350,524
엘보보온 19t	D 450	개소	6	66,546	399,276	156,237	937,422		-	1,336,698
엘보보온 25t	D 150	개소	10	12,379	123,790	22,955	229,550		-	353,340
엘보보온 25t	D 300	개소	5	35,967	179,835	75,715	378,575		-	558,410
엘보보온 50t	D 100	M	10	12,330	123,300	21,308	213,080		-	336,380
엘보보온 50t	D 150	M	3	20,516	61,548	37,395	112,185		-	173,733

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
관보온 (고무발포재) 13t	D 80	M	85	6,961	591,685	17,696	1,504,160		-	2,095,845
관보온 (고무발포재) 13t	D 100	M	3	7,616	22,848	21,242	63,726		-	86,574
관보온 (고무발포재) 19t	D 65	M	93	7,663	712,659	16,334	1,519,062		-	2,231,721
관보온 (고무발포재) 19t	D 100	M	94	9,939	934,266	21,242	1,996,748		-	2,931,014
관보온 (고무발포재) 19t	D 125	M	44	11,483	505,252	23,689	1,042,316		-	1,547,568
관보온 (고무발포재) 19t	D 200	M	69	16,127	1,112,763	30,901	2,132,169		-	3,244,932
관보온 (고무발포재) 19t	D 300	M	40	22,336	893,440	42,339	1,693,560		-	2,587,000
관보온 (고무발포재) 19t	D 350	M	88	24,710	2,174,480	48,047	4,228,136		-	6,402,616
관보온 (고무발포재) 19t	D 400	M	65	27,900	1,813,500	52,954	3,442,010		-	5,255,510
관보온 (고무발포재) 19t	D 450	M	72		-		-		-	-
관보온(PERLITE) 50t	D 100	M	128	13,216	1,691,648	35,653	4,563,584		-	6,255,232
관보온(PERLITE) 50t	D 150	M	40	16,760	670,400	39,199	1,567,960		-	2,238,360
부속자재 보온		식	1	2,305,283/8,760,893= 0.26	2,305,283	5,007,347/17,622,427=0.25	5,007,347		-	7,312,630

(3) 철골 자재의 경우

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금액	단가	금액
RH 형강(SS400)	350*175*7*11	톤	18.018	412,000	7,423,416					7,423,416
“	350*350*12*19	톤	12.459	412,000	5,133,108					5,133,108
“	390*300*10*16	톤	25.370	412,000	10,452,440					10,452,440
“	400*200*8*13	톤	101.682	412,000	41,892,984					41,892,984
“	400*400*13*21	톤	34.516	412,000	14,220,592					14,220,592
“	450*200*9*14	톤	4.676	412,000	1,926,512					1,926,512
“	488*300*11*18	톤	52.747	412,000	21,731,764					21,731,764
“	500*200*10*16	톤	39.134	412,000	16,123,208					16,123,208
“	506*201*11*19	톤	99.150	412,000	40,849,800					40,849,800
“	582*300*12*17	톤	42.555	412,000	17,532,660					17,532,660
“	588*300*12*20	톤	68.012	412,000	28,020,944					28,020,944
“	594*302*14*23	톤	3.296	412,000	1,357,952					1,357,952
“	600*200*11*17	톤	4.537	412,000	1,869,244					1,869,244
“	606*201*12*20	톤	1.066	412,000	439,192					439,192
“	692*300*13*20	톤	7.993	412,000	3,293,116					3,293,116
“	700*300*13*24	톤	42.758	412,000	17,616,296					17,616,296
“	800*300*20*26	톤	23.348	412,000	9,619,376					9,619,376
“	900*300*16*28	톤	12.473	412,000	5,138,876					5,138,876
“	900*300*20*28	톤	6.985	412,000	2,877,820					2,877,820

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단가	금액	단가	금액
ㄷ 형강	125*65*6*8	톤	6.915	395,000	2,731,425					2,731,425
ㄷ 형강	150*75*6.5*10	톤	18.440	395,000	7,283,800					7,283,800
ㄷ 형강	200*70*7*10	톤	1.899	395,000	750,105					750,105
ㄷ 형강	200*80*7.5*11	톤	7.556	395,000	2,984,620					2,984,620
ㄷ 형강	250*90*8*13.5	톤	2.731	395,000	1,078,745					1,078,745
ㄴ 형강	40*40*5	톤	0.366	365,000	133,590					133,590
ㄴ 형강	65*65*6	톤	8.174	365,000	2,983,510					2,983,510
ㄴ 형강	75*75*6	톤	10.036	365,000	3,663,140					3,663,140
ㄴ 형강	90*90*7	톤	1.084	365,000	395,660					395,660
ㄴ 형강	100*100*7	톤	0.954	380,000	362,520					362,520
ㄴ 형강	100*100*8	톤	1.159	380,000	440,420					440,420
철 판(SS41)	T=6	KG	14	288	4,032					4,032
철 판(SS41)	T=7	KG	106	288	30,528					30,528
철 판(SS41)	T=8	KG	4,426	288	1,274,688					1,274,688
철 판(SS41)	T=9	KG	22,121	290	6,415,090					6,415,090
철 판(SS41)	T=10	KG	15,487	290	4,491,230					4,491,230
철 판(SS41)	T=11	KG	1,658	290	480,820					480,820
철 판(SS41)	T=12	KG	14,737	290	4,273,730					4,273,730
철 판(SS41)	T=13	KG	1,207	290	350,030					350,030
철 판(SS41)	T=14	KG	8,839	290	2,563,310					2,563,310
철 판(SS41)	T=15	KG	3,578	290	1,037,620					1,037,620

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단가	금 액	단가	금액	단가	금액
철 판(SS41)	T=16	KG	5,144	290	1,491,760					1,491,760
철 판(SS41)	T=17	KG	1,872	290	542,880					542,880
철 판(SS41)	T=18	KG	3,207	290	930,030					930,030
철 판(SS41)	T=20	KG	3,762	290	1,090,980					1,090,980
철 판(SS41)	T=24	KG	36	290	10,440					10,440
철 판(SS41)	T=25	KG	151	290	43,790					43,790
철 판(SS41)	T=30	KG	3,072	290	890,880					890,880
철 판(SS41)	T=35	KG	3,991	290	1,157,390					1,157,390
철 판(SS41)	T=40	KG	4,743	290	1,375,470					1,375,470
철 판(SS41)	T=45	KG	256	290	74,240					74,240
무 늬 강 판 (아연도)	T=4.5	톤	6.645	267,500	1,777,537					1,777,537
무 늬 강 판 (아연도)	T=6	톤	55.092	267,500	14,737,110					14,737,110
철골가공조립 (ROLL BEAM)	사무1000톤이상	톤	967.457	14,032	13,575,356	361,710	349,938,871			363,514,227
철골세우기	중층1000톤 이상	톤	967.457	177	171,239	37,192	35,981,660			36,152,899
고장력볼트	M16 L:100	EA	21	260	5,460					5,460
고장력볼트	M20 L:100	EA	7,857	426	3,347,082					3,347,082
고장력볼트	M22 L:100	EA	39,964	568	22,699,552					22,699,552
STUD BOLT	∅19 L:135	EA	13,086	294	3,847,284					3,847,284
STUD-BOLT설치	(앙카볼트 ∅19의 1/8적용)	EA	12,463			1,102	13,734,226			13,734,226
SPRING BOLT	M20	EA	529	474	250,746					250,746

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단가	금 액	단가	금 액	단가	금액
EXP.앙카	M16	EA	148	1,100	162,800					162,800
EXP.앙카	M20	EA	315	1,500	472,500					472,500
앙카볼트	∅19 L:580	EA	185	810	149,850					149,850
앙카볼트	∅19 L:600	EA	42	870	36,540					36,540
앙카볼트	∅19 L:900	EA	29	1,305	37,845					37,845
앙카볼트	∅22 L:620	EA	107	1,220	130,540					130,540
앙카볼트	∅22 L:950	EA	349	1,931	673,919					673,919
앙카볼트	∅28 L:1050	EA	8	2,596	20,768					20,768
앙카볼트설치	주기둥∅19-25	개소	678			16,908	11,463,624			11,463,624
앙카볼트설치	주기둥∅28이상	개소	8			22,054	176,432			176,432
철근(관급)	HD 22	톤	0.163
철근(관급)	HD 25	톤	1.857
철근(관급)	HD 35	톤	3.410
철근가공조립	보통	톤	5.272	12,437	65,567	394,375	2,079,145			2,144,712
강 관	∅ 216.5*8.0	톤	0.165	632,236	104,318					104,318
강 관	∅ 267.4*7.0	톤	0.322	646,116	208,049					208,049
그라우트몰탈		M3	1	126,500	126,500	75,472	75,472			201,972
방청페인트	철골2회 뿜칠	M2	11,889	923	10,973,547	1,323	15,729,147			26,702,694
내화페인트	T6.2MM	M2	18	33,350	600,300					600,300
철골내화피복(라코트)	습식30MM. 2시간	M2	178	12,000	2,136,000					2,136,000

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
철골내화피복(라코트)	습식20MM. 1시간	M2	9,671	8,000	77,368,000					77,368,000
우레탄페인트	내화피복없는 철골면	M2	5,030	7,288	36,658,640					36,658,640
DECK PLATE	T:1.2 DV-3 GI강판	M2	2,028	10,850	22,003,800					22,003,800
DECK PLATE	T:1.6 DV-3 GI강판	M2	3,663	12,850	47,069,550					47,069,550
데크프레이트설치		M2	5,691	222	1,263,402	7,410	42,170,310			43,433,712

<철골 부자재를 주 공사비(H형강)에 대한 비율로 환산>

공사명 품 명	단위	나노종합FAB센터(CUB)			국민은행 대전콜센터
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
H 형강	톤	52.615	23,445,686	100.00	3,049.23	1,534,727,140	100.00
Steel Plate	톤	5.278	2,179,026	9.29	559.519	263,505,430	17.17
고장력볼트	EA	138	1,646,539	7.02	45.257(톤)	44,351,860	2.89
앙카볼트	EA	356	426,461	1.82	1.177(톤)	666,250	0.04
그라우트몰탈	M3	0.399	456,652	1.95	2.25	3,375,000	0.22
ㄷ 형강	톤	-			-
Stud Bolt	EA	-			-
ㄴ 형강	톤	-			-

공사명 품 명	단위	국립생물자원관			대전 신계중학교
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
H 형강	톤	733.17	294,498,261	100.00	59.939	27,216,952	100.00
Steel Plate	톤	75.33	27,972,244	9.50	4.514	1,916,884	7.04
고장력볼트	EA	29,662	15,052,550	5.11	1,396	537,651	1.98
앙카볼트	EA	781	1,160,067	0.39	311	603,432	2.22
그라우트몰탈	M3	0.5	162,374	0.06	0.117	38,021	0.14
ㄷ 형강	톤	6.14	3,024,720	1.03	0.717	283,215	1.04
Stud Bolt	EA	26,502	15,424,164	5.24	-
ㄴ 형강	톤	0.243	83,988	0.03	0.291	127,182	0.47

공사명 품 명	단위	차세대연구기반동			핵융합실험동
		수 량	금 액(원)	비율(%)	수 량	금 액	비율(%)
H 형강	톤	6.41	3,717,800	100.00	818.466	337,207,992	100.00
Steel Plate	톤	0.945	584,143	15.71	98.407	28,528,938	8.46
고장력볼트	EA	614	213,624	5.75	47,842	26,052,094	7.73
앙카볼트	EA	128	201,696	5.43	720	1,049,462	0.31
그라우트몰탈	M3	0.059	19,160	0.52	1	201,972	0.06
ㄷ 형강	톤	0.055	29,700	0.80	37.541	14,828,695	4.40
Stud Bolt	EA	-			13,086	3,847,284	1.14
ㄴ 형강	톤	-			21.773	7,978,840	2.37

공사명 품 명	단위	전자현미경실험동			핵융합지원동
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
H 형강	톤	33.096	12,124,544	100.00	127.754	52,634,650	100.00
Steel Plate	톤	3.941	1,105,617	9.12	15.163	4,397,270	8.35
고장력볼트	EA	820	265,971	2.19	4,560	2,242,758	4.26
앙카볼트	EA	161	62,811	0.52	95	82,850	0.16
그라우트몰탈	M3	-			0.1	20,197	0.04
ㄷ 형강	톤	-			-
Stud Bolt	EA	1,957	178,081	1.47	1,764	518,616	0.99
ㄴ 형강	톤	0.337	97,944	0.81	1.029	375,585	0.71

공사명 품 명	평 균	비 고
H 형강	100.00
Steel Plate	10.58
고장력볼트	4.62
앙카볼트	1.36
그라우트몰탈	0.43
ㄷ 형강	1.82
Stud Bolt	2.21
ㄴ 형강	0.88

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
04 철골공사
RH 형강 (SS400)	각종 (818톤)	식	1		337,207,992					337,207,992
ㄷ 형강	주자재 금액 × 1.82%	식	1		6,137,185					6,137,185
ㄴ 형강	주자재 금액 × 0.88%	식	1		2,967,430					2,967,430
철 판 (SS41)	각종, 주자재 금액 × 10.58%	식	1		35,676,606					35,676,606
무 늬 강 판 (아연도)	T=4.5	톤	6.645	267,500	1,777,537					1,777,537
무 늬 강 판 (아연도)	T=6	톤	55.092	267,500	14,737,110					14,737,110
철골가공조립(ROLL BEAM)	사무1000톤이상	톤	967.457	14,032	13,575,356	361,710	349,938,871			363,514,227
방청페인트	철골2회 뿜칠	M2	11,889	923	10,973,547	1,323	15,729,147			26,702,694
내화페인트	T6.2MM	M2	18	33,350	600,300					600,300
철골내화피복 (라코트)	습식30MM. 2시간	M2	178	12,000	2,136,000					2,136,000
철골내화피복 (라코트)	습식20MM. 1시간	M2	9,671	8,000	77,368,000					77,368,000
우레탄페인트	내화피복없는 철골면	M2	5,030	7,288	36,658,640					36,658,640
DECK PLATE	T:1.2 DV-3 GI강판	M2	2,028	10,850	22,003,800					22,003,800
DECK PLATE	T:1.6 DV-3 GI강판	M2	3,663	12,850	47,069,550					47,069,550
데크플레이트설치		M2	5,691	222	1,263,402	7,410	42,170,310			43,433,712

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단가	금 액	단 가	금 액	단가	금액
철골세우기	중층1000톤 이상	톤	967.457	177	171,239	37,192	35,981,660			36,152,899
고장력볼트	각종, 주자재 금액 × 4.62%	식	1		15,579,009					15,579,009
EXP.앙카	M16	EA	148	1,100	162,800					162,800
EXP.앙카	M20	EA	315	1,500	472,500					472,500
앙카볼트	각종, 주자재 금액 × 1.36%	식	1		4,586,027					4,586,027
STUD-BOLT	각종, 주자재 금액 × 2.21%	식	1		7,452,297					7,452,297
STUD-BOLT설치	(앙카볼트∅19의 1/8적용)	EA	12,463			1,102	13,734,226			13,734,226
SPRING BOLT	M20	EA	529	474	250,746					250,746
앙카볼트설치	주기둥∅19-25	개소	678			16,908	11,463,624			11,463,624
앙카볼트설치	주기둥∅28이상	개소	8			22,054	176,432			176,432
철근(관급)	HD 22	톤	0.163
철근(관급)	HD 25	톤	1.857
철근(관급)	HD 35	톤	3.410
철근가공조립	보통	톤	5.272	12,437	65,567	394,375	2,079,145			2,144,712
강 관	∅ 216.5*8.0	톤	0.165	632,236	104,318					104,318
강 관	∅ 267.4*7.0	톤	0.322	646,116	208,049					208,049
그라우트몰탈	각종, 주자재 금액 × 0.43%	식	1		1,449,994					1,449,994

(4) 가설전기, 가설용수

- 가설전기, 가설용수 등의 비용을 건축공사비에 대한 비율로 환산하여 적용

공사명 품 명	단위	차세대 연구기반동			전자현미경 실험동
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
건축 직접공사비	식	1	3,088,165,724	100.00	1	2,446,581,905	100.00
가설전기	〃	1	7,560,000	0.24	1	6,351,072	0.26
가설용수	〃	1	2,560,000	0.08	1	2,150,736	0.09
양수기 사용료	HR	1,600	179,200	0.01	6월	108,864	0.004
공사명 품 명	단위	나노종합FAB센터			평균		비고
		수 량	금 액(원)	비율(%)
건축 직접공사비	식	1	8,349,219,364	100.00	100.00
가설전기	〃	1	1,591,692	0.02	0.24
가설용수	〃	1	746,454	0.01
양수기 사용료	HR	-

나) 일위대가화

(1) 배관재

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 304 (SCH 10)	D 50	M	98	11,940	1,170,120		-		-	1,170,120
〃	D 65	M	81	14,800	1,198,800		-		-	1,198,800
〃	D 150	M	81	36,990	2,996,190		-		-	2,996,190
STS 배관(옥내배관)	D 50	M	89	859	76,451	36,590	3,256,510		-	3,332,984
STS 배관(옥내배관)	D 65	M	167	1,091	182,197	47,427	7,920,309		-	8,102,538
STS 배관(옥내배관)	D 80	M	85	1,258	106,930	54,647	4,644,995		-	4,751,950
STS 배관(옥내배관)	D 100	M	225	1,632	367,200	72,512	16,315,200		-	16,682,346
STS 배관(옥내배관)	D 125	M	44	1,972	86,768	88,807	3,907,508		-	3,994,297
STS 배관(옥내배관)	D 150	M	126	2,435	306,810	111,191	14,010,066		-	14,316,904
STS 배관(옥내배관)	D 200	M	69	3,384	233,496	160,302	11,060,838		-	11,294,361
STS 배관(옥내배관)	D 300	M	179	5,387	964,273	268,030	47,977,370		-	48,941,709
STS 배관(옥내배관)	D 350	M	227	5,763	1,308,201	296,572	67,321,844		-	68,630,045
STS 배관(옥내배관)	D 400	M	65	6,500	422,500	350,806	22,802,390		-	23,224,867
STS 배관(옥내배관)	D 450	M	72	7,291	524,952	412,316	29,686,752		-	30,211,671

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
STS 304 (SCH 10)	D 350	M	153	135,690	20,760,570		-		-	20,760,570
〃	D 80	M	94	25,592	2,405,648		-		-	2,405,648
STS 316 (SCH 10)	D 65	M	47	21,784	1,023,848		-		-	1,023,848
〃	D 100	M	128	33,096	4,236,288		-		-	4,236,288
〃	D 125	M	49	47,306	2,317,994		-		-	2,317,994
〃	D 150	M	45	56,140	2,526,300		-		-	2,526,300
〃	D 200	M	2	88,424	176,848		-		-	176,848
〃	D 300	M	17	156,968	2,668,456		-		-	2,668,456
〃	D 350	M	27	205,604	5,551,308		-		-	5,551,308
〃	D 400	M	72	235,354	16,945,488		-		-	16,945,488
〃	D 450	M	40	246,480	9,859,200		-		-	9,859,200
STS 316 (SCH 10)	D 65	M	56	22,040	1,234,240		-		-	1,234,240
〃	D 100	M	122	38160	4,655,520		-		-	4,655,520
〃	D 200	M	75	141590	10,619,250		-		-	10,619,250
〃	D 300	M	28	210560	5,895,680		-		-	5,895,680
〃	D 350	M	71	255945	18,172,095		-		-	18,172,095
〃	D 450	M	41	371,925	15,248,925		-		-	15,248,925
STS 배관(옥내배관)	D 50	M	89	859	76,451	36,590	3,256,510		-	3,332,984
STS 배관(옥내배관)	D 65	M	167	1,091	182,197	47,427	7,920,309		-	8,102,538
STS 배관(옥내배관)	D 80	M	85	1,258	106,930	54,647	4,644,995		-	4,751,950

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
STS 배관(옥내배관)	D 100	M	225	1,632	367,200	72,512	16,315,200		-	16,682,346
STS 배관(옥내배관)	D 125	M	44	1,972	86,768	88,807	3,907,508		-	3,994,297
STS 배관(옥내배관)	D 150	M	126	2,435	306,810	111,191	14,010,066		-	14,316,904
STS 배관(옥내배관)	D 200	M	69	3,384	233,496	160,302	11,060,838		-	11,294,361
STS 배관(옥내배관)	D 300	M	179	5,387	964,273	268,030	47,977,370		-	48,941,709
STS 배관(옥내배관)	D 350	M	227	5,763	1,308,201	296,572	67,321,844		-	68,630,045
STS 배관(옥내배관)	D 400	M	65	6,500	422,500	350,806	22,802,390		-	23,224,867
STS 배관(옥내배관)	D 450	M	72	7,291	524,952	412,316	29,686,752		-	30,211,671
STS 강관 용접	D 65	개소	70	2,603	182,210		-		-	182,210
STS 강관 용접	D 80	개소	27	3,281	88,587		-		-	88,587
STS 강관 용접	D 100	개소	101	5,090	514,090		-		-	514,090
STS 강관 용접	D 125	개소	24	7,639	183,336		-		-	183,336
STS 강관 용접	D 150	개소	56	9,545	534,520		-		-	534,520
STS 강관 용접	D 200	개소	25	16,061	401,525		-		-	401,525
STS 강관 용접	D 300	개소	64	30,953	1,980,992		-		-	1,980,992
STS 강관 용접	D 350	개소	69	34,560	2,384,640		-		-	2,384,640
STS 강관 용접	D 400	개소	16	39,495	631,920		-		-	631,920
STS 강관 용접	D 450	개소	16	44,434	710,944		7,612,764		-	8,323,708

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
2.21) 공동구
2.21-1 배관설치공사
STS 배관(옥내배관)	D 50	M	89	859	76,451	36,590	3,256,510		-	3,332,984
STS 배관(옥내배관)	D 65	M	167	1,091	182,197	47,427	7,920,309		-	8,102,538
STS 배관(옥내배관)	D 80	M	85	1,258	106,930	54,647	4,644,995		-	4,751,950
STS 배관(옥내배관)	D 100	M	225	1,632	367,200	72,512	16,315,200		-	16,682,346
STS 배관(옥내배관)	D 125	M	44	1,972	86,768	88,807	3,907,508		-	3,994,297
STS 배관(옥내배관)	D 150	M	126	2,435	306,810	111,191	14,010,066		-	14,316,904
STS 배관(옥내배관)	D 200	M	69	3,384	233,496	160,302	11,060,838		-	11,294,361
STS 배관(옥내배관)	D 300	M	179	5,387	964,273	268,030	47,977,370		-	48,941,709
STS 배관(옥내배관)	D 350	M	227	5,763	1,308,201	296,572	67,321,844		-	68,630,045
STS 배관(옥내배관)	D 400	M	65	6,500	422,500	350,806	22,802,390		-	23,224,867
STS 배관(옥내배관)	D 450	M	72	7,291	524,952	412,316	29,686,752		-	30,211,671

(2) 덕트 기구 취부

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
사각디퓨져 (STL)	ND125	EA	191	8,500	1,623,500					1,623,500
사각디퓨져 (STL)	ND150	EA	161	8,500	1,368,500					1,368,500
사각디퓨져 (STL)	ND200	EA	1	8,500	8,500					8,500
원형디퓨져 (STL)	ND125	EA	44	9,500	418,000					418,000
원형디퓨져 (STL)	ND150	EA	72	9,500	684,000					684,000
노즐디퓨져 (STL)	ND150	EA	39	11,400	444,600					444,600
후렉시블호스 (보온)	D125	M	311	3,050	948,550					948,550
후렉시블호스 (보온)	D150	M	476	3,660	1,742,160					1,742,160
후렉시블호스 (무)	D125	M	60	1,350	81,000					81,000
후렉시블호스 (무)	D150	M	40	1,620	64,800					64,800
후렉시블호스 (무)	D200	M	1	2,160	2,160					2,160
STS BAND	D125	EA	494	320	158,080					158,080
STS BAND	D150	EA	685	330	226,050					226,050
STS BAND	D200	EA	2	390	780					780
노무비	덕트공	인	409.5			26,108	10,691,226			10,691,226

-변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
사각디퓨져 (STL)	ND125	EA	191	13,715	2,619,565	20,625	3,939,375			6,558,940
사각디퓨져 (STL)	ND150	EA	161	14,650	2,358,650	21,408	3,446,688			5,805,338
사각디퓨져 (STL)	ND200	EA	1	15,280	15,280	22,191	22,191			37,471
원형디퓨져 (STL)	ND125	EA	44	14,715	647,460	20,625	907,500			1,554,960
원형디퓨져 (STL)	ND150	EA	72	15,650	1,126,800	21,408	1,541,376			2,668,176
노즐디퓨져 (STL)	ND150	EA	39	17,550	684,450	21,408	834,912			1,519,362

(3) 합판거푸집, 철근 구조물 콘크리트 펌프차 타설

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금 액
03 철근콘크리트공사
레미콘 (관급)	25-240-18	M3	35,047
레미콘 (관급)	25-180-15	M3	354
레미콘 (관급)	25-180-18	M3	2,391
레미콘 (관급)	25-135-8	M3	2,578
	《레미콘計》		40,370
펌프카붐타설	철근 100 M3 이상	M3	15,109	509	7,690,481	7,318	110,567,662	2,776	41,942,584
펌프카붐타설	무근 100 M3 이상	M3	5,218	458	2,389,844	6,183	32,262,894	2,496	13,024,128
배관타설 (TEST CELL)	철근 100 M3이상	M3	19,591	509	9,971,819	20,374	399,147,034	2,776	54,384,616
합판거푸집	1회	M2	13,277	11,535	153,150,195	32,025	425,195,925
합판거푸집	3회	M2	7,475	5,299	39,610,025	15,059	112,566,025
합판거푸집	4회	M2	2,507	4,608	11,552,256	12,810	32,114,670
원형거푸집 (장비패드)	2회	M2	14	14,238	199,332	39,218	549,052
시스템거푸집	벽체 T=1500	M2	15,698	42,600	668,734,800

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금 액
시스템거푸집	슬라브. TEST CELL	M2	4,480	37,000	165,760,000
시스템거푸집	지하외벽 .T=700이상	M2	26,779	25,500	682,864,500
	《거푸집計》		70,230
철근(관급)	HD 10	톤	161.225
철근(관급)	HD 13	톤	323.943
철근(관급)	HD 16	톤	250.120
철근(관급)	HD 19	톤	264.411
철근(관급)	HD 22	톤	729.118
철근(관급)	HD 25	톤	796.524
철근(관급)	HD 29	톤	374.035
철근(관급)	HD 32	톤	655.607
철근(관급)	HD 35	톤	91.818
	《철근 計》		3,646.801
비자성철근	PCD 21	톤	8.950	4,186,000	37,464,700
에폭시코팅 (가공비)	D25	톤	53.155	239,200	12,714,676
철근가공조립	보통	톤	3,549.272	12,437	44,142,295	394,375	1,399,744,145
진동기손료	전기식	M3	34,700					18	624,600
스페이샤	철제	EA	210,690	21	4,424,490
철근기계적이음	HD 35 (건설자재)	EA	1,299	16,770	21,784,230
경량탄열 콘크리트	B.S.T	M3	444	180,520	80,150,880
합 계

- 변경 전

합판거푸집                                                        (m2 당)

품 명	규 격	단위	단 가	1회 사용 시		2회 사용 시		3회 사용 시		4회 사용 시
				수 량	금 액	수 량	금 액	수 량	금 액	수 량	금 액
합 판	12mm 내수	m2	5,610	0.7931	4,449.2
각 재		m3	313,009	0.02926	9,158.6
철 선	#8 (4mm)	Kg	530	0.29	153.7
못		〃	564	0.20	112.8
박 리 제		ℓ	700	0.19	133.0
재료비소계					14,007	재료비의 57%	7,983	46.1%	6,457	40.1%	5,616
형틀목공	제작, 조립	인	92,242	0.30	27,672.6
보통인부	철거 포함	〃	52,374	0.25	13,093.5
노무비소계					40,766	인건비의 60%	24,459	47.1%	19,200	40%	16,306
합 계					54,773		32,442		25,657		21,922

- 변경 전

철근구조물 콘크리트 펌프차 타설(슬럼프 8~12cm)                  (m3 당)

품 명	규 격	단위	단 가	붐 타 설
				50m3 미만		50~100m3		100m3 이상
				수 량	금 액	수 량	금 액	수 량	금 액
콘크리트펌프차	80m3/h	hr	18,409	0.075	1,380.6	0.05	920.4	0.0416	765.8
재료비소계					1,380		920		765
콘크리트펌프차	80m3/h	hr	16,252	0.075	1,218.9	0.05	812.6	0.0416	676.0
콘크리트공		인	88,153	0.07	6,170.7	0.07	6,170.7	0.07	6,170.7
보통인부		〃	52,374	0.05	2,618.7	0.05	2,618.7	0.05	2,618.7
노무비소계					10,008		9,602		9,465
무근구조물타설
콘크리트펌프차	80m3/h	hr	96,846	0.075	7,263.4	0.05	4,842.3	0.0416	4,028.7
기계경비소계					7,263		4,842		4,028
합 계					18,651		15,364		14,258

- 스페이서, 세퍼레이터 및 진동기 손료를 주 공사비에 대한 비율로 환산하여 적용

공사명 품 명	단위	나노종합FAB센터			국민은행 대전콜센터
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
거푸집	M2	23,631	426,777,594	100.00	17,985	496,442,870	100.00
스페이서, 세퍼레이터	EA	65,243	1,226,362	0.29	-
펌프카 붐타설(철근)	M3	7,734	89,358,636	100.00	14,093	140,933,000	100.00
진동기 손료	M3	7,734	1,979,904	0.22	-
공사명 품 명	단위	서울 농학교 언어진료센터			국립생물자원관
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
거푸집	M2	755	322,904,492	100.00	7,654	224,557,010	100.00
스페이서, 세퍼레이터	EA	30,556	733,983	0.23	36,060	1,277,277	0.57
펌프카 붐타설(철근)	M3	3,388	44,554,329	100.00	5,423	67,207,239	100.00
진동기 손료	M3	3,388	13,552	0.03	5,423	309,111	0.46
공사명 품 명	단위	대전 신계중학교			차세대연구기반동
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
거푸집	M2	87,036	1,798,752,099	100.00	15,090	307,626,906	100.00
스페이서, 세퍼레이터	EA	23,397	458,518	0.03	16,938	643,644	0.21
펌프카 붐타설(철근)	M3	15,257	208,044,452	100.00	4,452	60,654,048	100.00
진동기 손료	M3	-			4,452	2,266,068	3.74

공사명 품 명	단위	핵융합실험동			전자현미경실험동
		수 량	금 액(원)	비율(%)	수 량	금 액(원)	비율(%)
거푸집	M2	70,230	2,292,296,780	100.00	10,024	157,888,369	100.00
스페이서, 세퍼레이터	EA	210,690	4,424,490	0.19	10,537	421,480	0.27
펌프카 붐타설(철근)	M3	34,700	623,704,196	100.00	3,278	30,672,246	100.00
진동기 손료	M3	34,700	624,600	0.10	3,278	1,117,798	3.64
공사명 품 명	단위	핵융합지원동			평 균		비 고
		수 량	금 액(원)	비율(%)
거푸집	M2	16,412	328,882,296	100.00	100.00
스페이서, 세퍼레이터	EA	49,236	1,033,956	0.31	0.26
펌프카 붐타설(철근)	M3	4,182	44,341,746	100.00	100.00
진동기 손료	M3	4,182	75,276	0.17	1.48

- 변경 후

합판거푸집                                                       (m2 당)

품 명	규 격	단위	단 가	1회 사용시		2회 사용시		3회 사용시		4회 사용시
				수 량	금 액	수 량	금 액	수 량	금 액	수 량	금 액
합 판	12mm 내수	m2	5,610	0.7931	4,449.2
각 재		m3	313,009	0.02926	9,158.6
철 선	#8 (4mm)	Kg	530	0.29	153.7
못		〃	564	0.20	112.8
박 리 제		ℓ	700	0.19	133.0
재료비소계 (1차)					14,007	재료비의 57%	7,983	46.1%	6,457	40.1%	5,616
형틀목공	제작, 조립	인	92,242	0.30	27,672.6
보통인부	철거 포함	〃	52,374	0.25	13,093.5
노무비소계					40,766	인건비의 60%	24,459	47.1%	19,200	40%	16,306
계					54,773		32,442		25,657		21,922
스페이서, 세퍼레이터	(계) × 0.26%				142.4		84.4		66.7		57.0
재료비소계 (2차)					14,149		8,067		6,523		5,673
합 계 (재료비+ 노무비2차+ 기계경비)					54,915		32,526		25,724		21,979

- 변경 후

철근구조물 콘크리트 펌프차 타설(슬럼프 8~12cm)                   (m3 당)

품 명	규 격	단위	단 가	붐 타 설
				50m3 미만		50~100m3		100m3 이상
				수 량	금 액	수 량	금 액	수 량	금 액
콘크리트펌프차	80m3/h	hr	18,409	0.075	1,380.6	0.05	920.4	0.0416	765.8
재 료 비 소 계					1,380		920		765
콘크리트펌프차	80m3/h	hr	16,252	0.075	1,218.9	0.05	812.6	0.0416	676.0
콘 크 리 트 공		인	88,153	0.07	6,170.7	0.07	6,170.7	0.07	6,170.7
보 통 인 부		〃	52,374	0.05	2,618.7	0.05	2,618.7	0.05	2,618.7
노무비 소 계 (1차)					10,008		9,602		9,465
무근구조물타설
콘크리트펌프차	80m3/h	hr	96,846	0.075	7,263.4	0.05	4,842.3	0.0416	4,028.7
기계경비소계					7,263		4,842		4,028
계					18,651		15,364		14,258
진동기 손료	(계) × 1.48%				276.0		227.4		211.0
노무비 소계 (2차)					10,284		9,829		9,676
합 계 (재료비+노무비 2차+기계경비)					18,927		15,591		14.469

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금 액
03 철근콘크리트공사
레미콘 (관급)	25-240-18	M3	35,047
레미콘 (관급)	25-180-15	M3	354
레미콘 (관급)	25-180-18	M3	2,391
레미콘 (관급)	25-135-8	M3	2,578
	《레미콘計》		40,370
펌프카붐타설	철근 100 M3 이상	M3	15,109	509	7,690,481	7,318	110,567,662	2,794	42,214,546
펌프카붐타설	무근 100 M3 이상	M3	5,218	458	2,389,844	6,183	32,262,894	2,496	13,024,128
배관타설 (TEST CELL)	철근 100 M3이상	M3	19,591	509	9,971,819	20,374	399,147,034	2,794	54,737,254
합판거푸집	1회	M2	13,277	11,556	153,150,195	32,025	425,195,925
합판거푸집	3회	M2	7,475	5,320	39,610,025	15,059	112,566,025
합판거푸집	4회	M2	2,507	4,629	11,552,256	12,810	32,114,670
원형거푸집 (장비패드)	2회	M2	14	14,238	199,332	39,218	549,052
시스템거푸집	벽체 T=1500	M2	15,698	42,600	668,734,800

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금 액
시스템거푸집	슬라브. TEST CELL	M2	4,480	37,000	165,760,000
시스템거푸집	지하외벽 .T=700이상	M2	26,779	25,500	682,864,500
	《거푸집計》		70,230
철근(관급)	HD 10	톤	161.225
철근(관급)	HD 13	톤	323.943
철근(관급)	HD 16	톤	250.120
철근(관급)	HD 19	톤	264.411
철근(관급)	HD 22	톤	729.118
철근(관급)	HD 25	톤	796.524
철근(관급)	HD 29	톤	374.035
철근(관급)	HD 32	톤	655.607
철근(관급)	HD 35	톤	91.818
	《철근 計》		3,646.801
비자성철근	PCD 21	톤	8.950	4,186,000	37,464,700
에폭시코팅 (가공비)	D25	톤	53.155	239,200	12,714,676
철근가공조립	보통	톤	3,549.272	12,437	44,142,295	394,375	1,399,744,145
철근기계적이음	HD 35 (건설자재)	EA	1,299	16,770	21,784,230
경량탄열 콘크리트	B.S.T	M3	444	180,520	80,150,880
합 계

(4) 석공사 및 타일공사

- 변경 전(타일공사)  : 압착 및 밀착공법(바닥)

(㎡)

구 분	규 격	단위	단 가	바름두께 5mm		6mm		7mm
				수 량	금 액	수 량	금 액	수량	금액
시 멘 트		kg	77.2	3.57	275.6	4.28	330.4	5.00	386.0
백시멘트		〃	200	1.48	296.0	1.48	296.0	1.48	296.0
모 래		㎥	11,000	0.0062	68.2	0.0073	80.3	0.0081	89.1
공구손료	인건비의 3%	식		1	951.4	1	951.4	1	951.4
재료비소계					1,591		1,658		1,722
타 일 공		인	98,192	0.216	21,209.4	0.216	21,209.4	0.216	21,209.4
줄 눈 공		〃	79,875	0.024	1,917.0	0.024	1,917.0	0.024	1,917.0
보통인부	붙 임	〃	52,374	0.080	4,189.9	0.080	4,189.9	0.080	4,189.9
〃	청 소	〃	52,374	0.024	1,256.9	0,024	1,256.9	0,024	1,256.9
〃	소운반	〃	52,374	0.060	3,142.4	0.060	3,142.4	0.060	3,142.4
노무비소계					31,715		31,715		31,715
합 계					33,306		33,373		33,437

건축물 보양                                                (보양면적 ㎡당)

구 분	규 격	단위	단 가	석재면, 테라조면타일(바닥)
				수량	금액
가 마 니		매	4,000	-	-
톱 밥		ℓ	별도	30	-
재료비소계					-
보 통 인 부		인	52,374	0.002	104.7
노무비소계					104
합 계					104

- 변경 후(타일공사)  : 압착 및 밀착공법(바닥)

(㎡)

구 분	규 격	단위	단 가	바름두께 5mm		6mm		7mm
				수 량	금 액	수 량	금 액	수량	금액
시 멘 트		kg	77.2	3.57	275.6	4.28	330.4	5.00	386.0
백시멘트		〃	200	1.48	296.0	1.48	296.0	1.48	296.0
모 래		㎥	11,000	0.0062	68.2	0.0073	80.3	0.0081	89.1
공구손료	인건비의 3%	식		1	951.4	1	951.4	1	951.4
재료비소계					19,101		19,168		19,232
타 일 공		인	98,192	0.216	21,209.4	0.216	21,209.4	0.216	21,209.4
줄 눈 공		〃	79,875	0.024	1,917.0	0.024	1,917.0	0.024	1,917.0
보통인부	붙 임	〃	52,374	0.080	4,189.9	0.080	4,189.9	0.080	4,189.9
〃	청 소	〃	52,374	0.024	1,256.9	0,024	1,256.9	0,024	1,256.9
〃	소운반	〃	52,374	0.060	3,142.4	0.060	3,142.4	0.060	3,142.4
〃	보 양	〃	52,374	0.002	104.7	0.002	104.7	0.002	104.7
노무비소계					31,820		31,820		31,820
합 계					50,921		50,988		51,052

※ 타일 붙이기 및 보양 노무비 일위대가표 통합

- 변경 전(석공사)  : 화강석판(바닥)

(㎡)

구 분	규 격	단 위	단 가	바 닥
				수 량	금 액
석 재 판		㎡	40,900	1.1	11,990
모 르 터	1:3(바름두께40mm)	㎡	103,846	0,045	4,673.0
철 물	황동	kg	4,100		-
재료비소계					49,663
석 공		인	95,056	0,49	46,577.4
보통인부		〃	52,374	0,25	13,093.5
노무비소계					59,670
합 계					109,333

건축물 보양                                                (보양면적 ㎡당)

구 분	규 격	단위	단 가	석재면, 테라조면타일(바닥)
				수량	금액
가 마 니		매	4,000	-	-
톱 밥		ℓ	별도	30	-
재료비소계					-
보 통 인 부		인	52,374	0.002	104.7
노무비소계					104
합 계					104

-변경 후(석공사)  : 화강석판(바닥)

(㎡당)

구 분	규 격	단 위	단 가	바 닥
				수 량	금 액
석 재 판		㎡	40,900	1.1	44,990
모 르 터	1:3(바름두께40mm)	㎡	103,846	0,045	4,673.0
철 물	황동	kg	4,100		-
재료비소계					49,663
석 공		인	95,056	0,49	46,577.4
보통인부		〃	52,374	0,25	13,093.5
〃	보양	〃	52,374	0.002	104.7
노무비소계					59,775
합 계					109,438

※ 석재 붙이기 및 보양 노무비 일위대가표 통합

다) 단위 변경

(1) 덕트 부속

(가) Sound chamber

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
SOUND CHAMBER	3900x1800x850	EA	1	1,376,340	1,376,340					1,376,340
SOUND CHAMBER	2600x1500x850	EA	1	856,660	856,660					856,660
SOUND CHAMBER	2400x1400x900	EA	1	786,480	786,480					786,480
SOUND CHAMBER	3400x2100x850	EA	1	1,370,540	1,370,540					1,370,540
SOUND CHAMBER	1000x1200x800	EA	1	343,360	343,360					343,360
SOUND CHAMBER	1700x1200x1400	EA	1	707,600	707,600					707,600
SOUND CHAMBER	2500x1400x1400	EA	1	1,039,360	1,039,360					1,039,360

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
SOUND CHAMBER		cm2	648,034	10	6,480,340					6,480,340

(나) Damper 류

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
F.V.D W/FUSE	1500x450	EA	1	46,275	46,275					46,275
F.V.D W/FUSE	1000x600	EA	1	41,400	41,400					41,400
F.V.D W/FUSE	1000x450	EA	1	31,650	31,650					31,650
F.V.D W/FUSE	1000x550	EA	1	38,150	38,150					38,150
F.V.D W/FUSE	1100x550	EA	1	41,725	41,725					41,725
F.V.D W/FUSE	1400x550	EA	1	52,450	52,450					52,450
F.V.D W/FUSE	1700x550	EA	1	63,175	63,175					63,175
F.V.D W/FUSE	2200x550	EA	1	81,050	81,050					81,050
F.V.D W/FUSE	300x 200	EA	3	9,400	28,200					28,200
F.V.D W/FUSE	350x 175	EA	1	9,400	9,400					9,400
F.V.D W/FUSE	400x 175	EA	2	9,400	18,800					18,800
F.V.D W/FUSE	400x 200	EA	3	9,400	28,200					28,200
F.V.D W/FUSE	450x 175	EA	2	9,400	18,800					18,800
F.V.D W/FUSE	450x 200	EA	3	9,400	28,200					28,200
F.V.D W/FUSE	450x 250	EA	1	9,713	9,713					9,713

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
F.V.D W/FUSE	450x 400	EA	1	14,100	14,100					14,100
F.V.D W/FUSE	500x 175	EA	1	8,088	8,088					8,088
F.V.D W/FUSE	550x 150	EA	2	9,400	18,800					18,800
F.V.D W/FUSE	550x 350	EA	1	14,913	14,913					14,913
F.V.D W/FUSE	600x 175	EA	5	9,225	46,125					46,125
F.V.D W/FUSE	600x 400	EA	1	18,000	18,000					18,000
F.V.D W/FUSE	700x 400	EA	1	20,600	20,600					20,600
F.V.D W/FUSE	750x 800	EA	1	41,400	41,400					41,400
F.V.D W/FUSE	800x 400	EA	1	23,200	23,200					23,200
F.V.D W/FUSE	850x 450	EA	1	27,263	27,263					27,263
F.V.D W/FUSE	900x 500	EA	1	31,650	31,650					31,650
F.V.D W/FUSE	900x 900	EA	1	55,050	55,050					55,050
F.V.D W/FUSE	950x 500	EA	1	33,275	33,275					33,275
F.V.D W/FUSE	200x 200	EA	1	14,400	14,400					14,400
F.V.D W/FUSE	2200x550	EA		81,050						81,050
F.V.D W/FUSE	1550x550	EA		57,813						57,813
F.V.D W/FUSE	1400x550	EA		52,450						52,450

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
F.V.D W/FUSE	1200x450	EA		37,500						37,500
F.V.D W/FUSE	900x 900	EA		55,050						55,050
F.V.D W/FUSE	850x 450	EA		27,263						27,263
F.V.D W/FUSE	750x 800	EA		41,400						41,400
F . D W/FUSE	1000x1000	EA	1	67,400	67,400					67,400
F . D W/FUSE	1000x550	EA	1	38,150	38,150					38,150
F . D W/FUSE	1100x450	EA	2	34,575	69,150					69,1505
F . D W/FUSE	1400x550	EA	2	52,450	104,900					104,900
F . D W/FUSE	200x 150	EA	4	9,400	37,600					37,600
F . D W/FUSE	2300x1900	EA	2	286,450	572,900					572,900
F . D W/FUSE	300x 175	EA	1	9,400	9,400					9,400
F . D W/FUSE	350x 175	EA	1	9,400	9,400					9,400
F . D W/FUSE	400x 175	EA	1	9,400	9,400					9,400
F . D W/FUSE	400x 250	EA	1	9,400	9,400					9,400
F . D W/FUSE	450x 200	EA		8,250
F . D W/FUSE	500x 250	EA	1	10,525	10,525					10,525
F . D W/FUSE	600x 300	EA	2	14,100	28,200					28,200

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
F . D W/FUSE	650x 175	EA	1	9,794	9,794					9,794
F . D W/FUSE	650x 350	EA	4	17,188	68,752					68,752
F . D W/FUSE	700x 400	EA	1	20,600	20,600					20,600
F . D W/FUSE	800x 400	EA	2	23,200	46,400					46,400
F . D W/FUSE	850x 400	EA	2	24,500	49,000					49,000
F . D W/FUSE	900x 750	EA	2	46,275	92,550					92,550
F . D (STS 1.5t)	600x 350	EA	1	63,000	63,000					63,000
M.F.D (STL)	300x 200	EA	1	7,000	7,000					7,000
M.F.D (STL)	400x 200	EA	1	7,000	7,000					7,000
M.F.D (STL)	400x 300	EA	1	7,800	7,800					7,800
M.F.D (STL)	450x 200	EA	1	7,000	7,000					7,000
M.F.D (STL)	700x 400	EA	1	18,200	18,200					18,200
M.F.D (STL) W/모타	1100x500	EA	1	78,750	78,750					78,750
M.F.D (STL) W/모타	1100x450	EA	1	75,175	75,175					75,175
V . D (STL)	200x 100	EA	18	7,000	126,000					126,000
V . D (STL)	200x 150	EA	60	7,000	420,000					420,000
V . D (STL)	200x 200	EA	3	7,000	21,000					21,000

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
V . D (STL)	250x 150	EA	18	7,000	126,000					126,000
V . D (STL)	250x 200	EA	24	7,000	168,000					168,000
V . D (STL)	250x 250	EA	1	7,000	7,000					7,000
V . D (STL)	300x 150	EA	33	7,000	231,000					231,000
V . D (STL)	300x 200	EA	30	7,000	210,000					210,000
V . D (STL)	300x 250	EA	4	7,000	28,000					28,000
V . D (STL)	350x 150	EA	8	7,000	56,000					56,000
V . D (STL)	350x 200	EA	7	7,000	49,000					49,000
V . D (STL)	350x 250	EA	6	7,000	42,000					42,000
V . D (STL)	350x 300	EA		7,000
V . D (STL)	400x 150	EA	4	7,000	28,000					28,000
V . D (STL)	400x 200	EA	8	7,000	56,000					56,000
V . D (STL)	400x 250	EA	3	7,000	21,000					21,000
V . D (STL)	450x 200	EA	6	7,000	42,000					42,000
V . D (STL)	450x 250	EA	7	7,313	51,191					51,191
V . D (STL)	500x 250	EA	4	8,125	32,500					32,500
V . D (STL)	500x 300	EA	2	9,750	19,500					19,500

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
V . D (STL)	550x 250	EA	2	8,938	17,876					17,876
V . D (STL)	550x 300	EA	4	10,725	42,900					42,900
V . D (STL)	600x 300	EA	1	11,700	11,700					11,700
V . D (STL)	600x 350	EA	1	13,650	13,650					13,650
V . D (STL)	650x 350	EA	1	14,788	14,788					14,788
V . D (STL)	650x 400	EA	1	16,900	16,900					16,900
V . D (STL)	700x 350	EA	1	15,925	15,925					15,925
V . D (STL)	700x 400	EA	2	18,200	36,400					36,400
V . D (STL)	950x 450	EA	1	27,788	27,788					27,788
V . D (STL)	1100x450	EA	1	32,175	32,175					32,175
V . D (STS 1.5t)	600x 350	EA	2	63,000	126,000					126,000
V . D (STS)	200x 200	EA	1	12,000	12,000					12,000

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
V . D		cm2	512,729	10	5,127,290					5,127,290
FUSE		EA	73	8,500	620,500					620,500

(다) Register 류

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
GRILLE (AL)	1000x650	EA	2	58,500	117,000					117,000
GRILLE (AL)	1000x700	EA	3	63,000	189,000					189,000
GRILLE (AL)	600x 450	EA	1	24,300	24,300					24,300
GRILLE (AL)	650x 400	EA	4	23,400	93,600					93,600
REGISTER (AL)	1100x700	EA	8	115,500	924,000					924,000
REGISTER (AL)	1000x550	EA	12	82,500	990,000					990,000
REGISTER (AL)	200x 150	EA	29	15,000	435,000					435,000
REGISTER (AL)	250x 150	EA	15	15,000	225,000					225,000
REGISTER (AL)	250x 200	EA	6	15,000	90,000					90,000
REGISTER (AL)	250x 250	EA	14	15,000	210,000					210,000
REGISTER (AL)	250x 400	EA	6	15,000	90,000					90,000
REGISTER (AL)	300x 250	EA	1	15,000	15,000					15,000
REGISTER (AL)	350x 250	EA	4	15,000	60,000					60,000
REGISTER (AL)	350x 300	EA	2	15,750	31,500					31,500

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
REGISTER (AL)	400x 300	EA	4	18,000	72,000					72,000
REGISTER (AL)	450x 250	EA	10	16,875	168,750					168,750
REGISTER (AL)	500x 250	EA	7	18,750	131,250					131,250
REGISTER (AL)	600x 400	EA	3	36,000	108,000					108,000
REGISTER (AL)	650x 400	EA	1	39,000	39,000					39,000
REGISTER (AL)	700x 550	EA	2	57,750	115,500					115,500
REGISTER (AL)	800x 500	EA	10	60,000	600,000					600,000
LOUVER (AL)	550x 300	EA	8	24,750	198,000					198,000

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단 가	금 액
GRILLE (AL)		cm2	3,854	11	423,940					423,940
REGISTER (AL)		cm2	266,292	18	4,793,256					4,793,256
T.V		m	224	4,000	896,000					896,000

(2) 배관재의 단위를 중량으로

배관재를 규격별로 수량산출 한 후 중량으로 환산 (m × kg/m = kg) 하여 표기할 수는 있으나 획기적인 방법이 될 것 같다.  또한 내역서 만으로 공사의 성격을 알기에는 어려울 것 같다.

(3) 창호공사

- SD : 개소 ⟶ 면적(㎡)으로 수량산출

- AL, AG : 개소 ⟶ 중량(㎏)으로 수량 산출

- 변경 전

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
0112 창호공사
FSD-1	2600*3400	개소	1	645,320	645,320	0	0	0	0	645,320
FSD-2	2500*2400	개소	1	522,000	522,000	0	0	0	0	522,000
FSD-3	2400*3400	개소	1	734,400	734,400	0	0	0	0	734,400
FSD-4A	1800*2100	개소	2	275,940	551,880	0	0	0	0	551,880
FSD-4B	1800*2100	개소	1	340,200	340,200	0	0	0	0	340,200
FSD-5	2600*2400	개소	1	455,520	455,520	0	0	0	0	455,520
FSD-6	2400*2400	개소	1	420,480	420,480	0	0	0	0	420,480
FSD-7	1000*2100	개소	2	210,000	420,000	0	0	0	0	420,000
SD-1A	2200*2100	개소	1	337,260	337,260	0	0	0	0	337,260
SD-1B	2200*2100	개소	1	415,800	415,800	0	0	0	0	415,800
SD-2A	1800*2100	개소	1	275,940	275,940	0	0	0	0	275,940
SD-2B	1800*2100	개소	2	340,200	680,400	0	0	0	0	680,400
SD-3	1800*2100	개소	16	272,160	4,354,560	0	0	0	0	4,354,560
SD-4	1800*2000	개소	1	307,680	307,680	0	0	0	0	307,680
SD-5A	1000*2100	개소	1	210,000	210,000	0	0	0	0	210,000
SD-5B	1000*2100	개소	5	186,900	934,500	0	0	0	0	934,500
SD-5C	1000*2100	개소	3	186,900	560,700	0	0	0	0	560,700
SD-6	750*2100	개소	2	114,975	229,950	0	0	0	0	229,950
SD-7	750*1500	개소	2	79,875	159,750	0	0	0	0	159,750
SD-8	2300*2700	개소	1	465,750	465,750	0	0	0	0	465,750
SD-9	2400*2700	개소	1	583,200	583,200	0	0	0	0	583,200
SSD-1	6400*2600*3600	개소	1	4,571,850	4,571,850	0	0	0	0	4,571,850
자동문	양개	조	2	1,500,000	3,000,000	0	0	0	0	3,000,000
SSD-2	1100*2000	개소	1	210,180	210,180	0	0	0	0	210,180
SSD-3	5100*3600	개소	1	1,768,894	1,768,894	0	0	0	0	1,768,894

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
SSD-4	4300*3600	개소	1	1,213,571	1,213,571	0	0	0	0	1,213,571
SSD-5	1985*3600	개소	1	681,642	681,642	0	0	0	0	681,642
SSD-6	3100*3600	개소	1	793,130	793,130	0	0	0	0	793,130
ATD-1	940*2300	개소	2	1,500,000	3,000,000	0	0	0	0	3,000,000
SPD-1 (스틸차음방음문)	3000*3600	개소	1	11,820,000	11,820,000	0	0	0	0	11,820,000
SPD-2 (스틸차음방음문)	3100*3000	개소	1	10,180,000	10,180,000	0	0	0	0	10,180,000
SSF-1A	1800*2400	개소	1	320,100	320,100	0	0	0	0	320,100
SSF-1B	1800*2400	개소	1	425,040	425,040	0	0	0	0	425,040
SSW-1A	2300*3600	개소	1	878,891	878,891	0	0	0	0	878,891
SSW-1B	2350*3600	개소	1	889,686	889,686	0	0	0	0	889,686
GB-1	6850*2700	개소	1	647,490	647,490	0	0	0	0	647,490
GB-2	6850*1800	개소	1	586,470	586,470	0	0	0	0	586,470
CAW-1A (100MM SL)	6600*3000 (120.6KG) 불소코팅	개소	3	1,213,236	3,639,708	0	0	0	0	3,639,708
CAW-1B (100MM SL)	6550*3000 (120.2KG) 불소코팅	개소	1	1,209,212	1,209,212	0	0	0	0	1,209,212
CAW-1C (100MM SL)	6300*3000 (117.8KG) 불소코팅	개소	1	1,185,068	1,185,068	0	0	0	0	1,185,068
CAW-2A (100MM SL)	1750*3000 (35.3KG) 불소코팅	개소	1	355,118	355,118	0	0	0	0	355,118
CAW-2B (100MM SL)	1600*3000 (33.9KG) 불소코팅	개소	1	341,034	341,034	0	0	0	0	341,034
CAW-3A (100MM SL)	6600*900 (43.2KG) 불소코팅	개소	1	434,592	434,592	0	0	0	0	434,592
CAW-3B (100MM SL)	6600*1200 (57.6KG) 불소코팅	개소	1	579,456	579,456	0	0	0	0	579,456

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
CAW-4 (100MM SL)	2400*1200 (20.1KG) 불소코팅	개소	1	202,206	202,206	0	0	0	0	202,206
CAW-5 (100MM FIX)	2400*1200 (13.3KG) 불소코팅	개소	1	118,237	118,237	0	0	0	0	118,237
CAW-8 (100MM FIX+PJ)	2700*2100 (121.5KG) 불소코팅	개소	2	1,458,000	2,916,000	0	0	0	0	2,916,000
CAW-10 (100MM FIX)	3000*1200 (36.0KG) 불소코팅	개소	2	320,040	640,080	0	0	0	0	640,080
CAW-11 (100MM FIX)	1800*1800 (28.1KG) 불소코팅	개소	6	249,809	1,498,854	0	0	0	0	1,498,854
CAW-12A (100MM FIX)	3130*900 (29.5KG) 불소코팅	개소	1	262,255	262,255	0	0	0	0	262,255
CAW-12B (100MM FIX)	2495*900 (25.1KG) 불소코팅	개소	1	223,139	223,139	0	0	0	0	223,139
CAW-13A (100MM FIX)	1550*900 (18.6KG) 불소코팅	개소	2	165,354	330,708	0	0	0	0	330,708
CAW-13B (100MM FIX)	1250*900 (16.5KG) 불소코팅	개소	2	146,685	293,370	0	0	0	0	293,370
CAW-14A (100MM PJ)	4400*900 (124.8KG) 불소코팅	개소	1	1,497,600	1,497,600	0	0	0	0	1,497,600
CAW-14B (100MM PJ)	4150*900 (120.6KG) 불소코팅	개소	2	1,447,200	2,894,400	0	0	0	0	2,894,400
CAW-15 (100MM PJ)	4800*900 (135.9KG) 불소코팅	개소	1	1,630,800	1,630,800	0	0	0	0	1,630,800
CAW-17 (120MM FIX)	7800*3800 (225.8KG) 불소코팅	개소	1	2,007,362	2,007,362	0	0	0	0	2,007,362

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
CAW-18 (120MM FIX+PJ)	7800*3800 (337.7KG) 불소코팅	개소	3	4,052,400	12,157,200	0	0	0	0	12,157,200
CAW-19 (120MM FIX+PJ)	3550*3800 (161.4KG) 불소코팅	개소	2	1,936,800	3,873,600	0	0	0	0	3,873,600
CAW-20 (120MM FIX)	9440*3800 (277.5KG) 불소코팅	개소	1	2,466,975	2,466,975	0	0	0	0	2,466,975
CAW-21 (120MM FIX+PJ)	9440*3800 (419.7KG) 불소코팅	개소	1	5,036,400	5,036,400	0	0	0	0	5,036,400
CAW-22 (150MM FIX+PJ, 커턴월)	4200*13200(789.7KG) 불소코팅	개소	1	9,775,440	9,775,440	0	0	0	0	9,775,440
CAW-23 (150MM FIX+PJ, 커턴월)	4300*12000(740.1KG) 불소코팅	개소	1	9,154,760	9,154,760	0	0	0	0	9,154,760
AG-1A (100MM)	6600*900 (74.2KG) 불소코팅	개소	5	659,638	3,298,190	0	0	0	0	3,298,190
AG-1B (100MM)	6300*900 (71.1KG) 불소코팅	개소	1	632,079	632,079	0	0	0	0	632,079
AG-2 (100MM)	3300*900 (37.8KG) 불소코팅	개소	1	336,042	336,042	0	0	0	0	336,042
AG-4 (100MM)	2350*1600 (45.4KG) 불소코팅	개소	8	403,606	3,228,848	0	0	0	0	3,228,848
AG-5 (100MM)	1650*1600 (34.1KG) 불소코팅	개소	12	303,149	3,637,788	0	0	0	0	3,637,788
AG-6 (100MM)	2350*1600 (47.9KG) 불소코팅	개소	4	425,831	1,703,324	0	0	0	0	1,703,324
AG-7 (100MM)	3300*1000 (42.0KG) 불소코팅	개소	1	373,380	373,380	0	0	0	0	373,380

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
AG-8 (100MM)	500*200 (2.8KG) 불소코팅	개소	1	24,892	24,892	0	0	0	0	24,892
AG-9 (100MM)	3000*1600 (59.3KG) 불소코팅	개소	1	527,177	527,177	0	0	0	0	527,177
강화유리문	투명 12 0 9 2 25	개	4	140,000	560,000	0	0	0	0	560,000
강화유리문	투명 12 0 9 2 5	개	2	180,000	360,000	0	0	0	0	360,000
강화유리문	투명 12 1 0 2 25	개	2	160,000	320,000	0	0	0	0	320,000
강화유리문	컬러 12 1 086 2 1	개	1	170,000	170,000	0	0	0	0	170,000
강화유리문	컬러 12 1 175 2 1	개	2	190,000	380,000	0	0	0	0	380,000
후로아힌지설치		개소	11	47,325	520,575	10,852	119,372	0	0	639,947
도아체크달기 (강재)	방화용	개소	18	39,211	705,798	7,060	127,080	0	0	832,878
도아체크달기 (강재)	일반용	개소	34	18,211	619,174	7,060	240,040	0	0	859,214
도아록설치	철문용	개소	47	9,026	424,222	898	42,206	0	0	466,428
도아록설치	공정	개소	32	4,126	132,032	898	28,736	0	0	160,768
철제정첩	4“	개	50	1,500	75,000	0	0	0	0	75,000
피벗힌지	140Kg이하 (K1400)	조	65	16,000	1,040,000	0	0	0	0	1,040,000
AL방충망 (미서기,후레임포함)	불소코팅 시공도	M2	61	15,900	969,900	0	0	0	0	969,900
< 계 >

AW창호(개소⟶중량)

품 명	규 격	단 위	수 량	계
CAW - 1A	120.6Kg	EA	3	361.8
CAW - 1B	120.2Kg	EA	1	120.2
CAW - 1C	117.8Kg	EA	1	117.8
CAW - 2A	35.3Kg	EA	1	35.3
CAW - 2B	33.9Kg	EA	1	33.9
CAW - 3A	43.2Kg	EA	1	43.2
CAW - 3B	57.6Kg	EA	1	57.6
CAW - 4	20.1Kg	EA	1	20.1
CAW - 5	13.3Kg	EA	1	13.3
CAW - 8	121.5Kg	EA	2	243
CAW - 10	36Kg	EA	2	72
CAW - 11	28.1Kg	EA	6	168.6
CAW - 12A	29.5Kg	EA	1	29.5
CAW - 12B	25.1Kg	EA	1	25.1
CAW - 13A	18.6Kg	EA	2	37.2
CAW - 13B	16.5Kg	EA	2	33
CAW - 14A	124.8Kg	EA	1	124.8
CAW - 14B	120.6Kg	EA	2	241.2
CAW - 15	135.9Kg	EA	1	135.9
CAW - 17	225.8Kg	EA	1	225.8
CAW - 18	337.7Kg	EA	3	1013.1
CAW - 19	161.4Kg	EA	2	322.8
CAW - 20	277.5Kg	EA	1	277.5
CAW - 21	419.7Kg	EA	1	419.7
CAW - 22	789.7Kg	EA	1	789.7
CAW - 23	740.1Kg	EA	1	740.1
계				5,702
AG - 1A	74.2Kg	EA	5	371
AG - 1B	71.1Kg	EA	1	71.1
AG - 2	37.8Kg	EA	1	37.8
AG - 4	45.4Kg	EA	8	363.2
AG - 5	34.1Kg	EA	12	409.2
AG - 6	47.9Kg	EA	4	191.6
AG - 7	42Kg	EA	1	42
AG - 8	2.8Kg	EA	1	2.8
AG - 9	59.3Kg	EA	1	59.3
계				1,548

- 변경 후

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
0112 창호공사
SD	각종(47개소)	㎡	172	79,100	13,605,200	0	0	0	0	13,605,200
SSD-1	6400*2600*3600	개소	1	4,571,850	4,571,850	0	0	0	0	4,571,850
자동문	양개	조	2	1,500,000	3,000,000	0	0	0	0	3,000,000
SSD-2	1100*2000	개소	1	210,180	210,180	0	0	0	0	210,180
SSD-3	5100*3600	개소	1	1,768,894	1,768,894	0	0	0	0	1,768,894
SSD-6	3100*3600	개소	1	793,130	793,130	0	0	0	0	793,130
ATD-1	940*2300	개소	2	1,500,000	3,000,000	0	0	0	0	3,000,000
SPD-1 (스틸차음방음문)	3000*3600	개소	1	11,820,000	11,820,000	0	0	0	0	11,820,000
SPD-2 (스틸차음방음문)	3100*3000	개소	1	10,180,000	10,180,000	0	0	0	0	10,180,000
SSF-1A	1800*2400	개소	1	320,100	320,100	0	0	0	0	320,100
SSF-1B	1800*2400	개소	1	425,040	425,040	0	0	0	0	425,040
SSW-1A	2300*3600	개소	1	878,891	878,891	0	0	0	0	878,891
SSW-1B	2350*3600	개소	1	889,686	889,686	0	0	0	0	889,686
GB-1	6850*2700	개소	1	647,490	647,490	0	0	0	0	647,490
GB-2	6850*1800	개소	1	586,470	586,470	0	0	0	0	586,470
CAW		KG	5,702	22,132	126,196,664	0	0	0	0	126,196,664
AG		KG	1,548	8,549	13,233,852	0	0	0	0	13,233,852

품 명	규 격	단위	수량	재 료 비		노 무 비		경 비		계
				단 가	금 액	단 가	금 액	단가	금액
강화유리문	투명 12 0 9 2 25	개	4	140,000	560,000	0	0	0	0	560,000
강화유리문	투명 12 0 9 2 5	개	2	180,000	360,000	0	0	0	0	360,000
강화유리문	투명 12 1 0 2 25	개	2	160,000	320,000	0	0	0	0	320,000
강화유리문	컬러 12 1 086 2 1	개	1	170,000	170,000	0	0	0	0	170,000
강화유리문	컬러 12 1 175 2 1	개	2	190,000	380,000	0	0	0	0	380,000
후로아힌지설치		개소	11	47,325	520,575	10,852	119,372	0	0	639,947
도아체크달기 (강재)	방화용	개소	18	39,211	705,798	7,060	127,080	0	0	832,878
도아체크달기 (강재)	일반용	개소	34	18,211	619,174	7,060	240,040	0	0	859,214
도아록설치	철문용	개소	47	9,026	424,222	898	42,206	0	0	466,428
도아록설치	공정	개소	32	4,126	132,032	898	28,736	0	0	160,768
철제정첩	4“	개	50	1,500	75,000	0	0	0	0	75,000
피벗힌지	140Kg이하 (K1400)	조	65	16,000	1,040,000	0	0	0	0	1,040,000
AL방충망 (미서기,후레임포함)	불소코팅 시공도	M2	61	15,900	969,900	0	0	0	0	969,900
< 계 >

# 부록3

기계설비공사 관이음부속 및 지지물 부자재비율
구 분	00대학병원		00도로출입국		00초.중등학교		00실험동		00전자현미경		00우체국
공정별	관재질	부자재비율 (%)	관재질	부자재비율 (%)	관재질	부자재비율 (%)	관재질	부자재비율 (%)	관재질	부자재비율 (%)	관재질	부자재비율 (%)
1.장비설치
2.기계실배관	STS	54.9	STS	44.4	STS	34.2	STS	52.4	STS	54.5	STS	65.2
3.공조난방	STS	47.7	STS	28.6	STS	45.4			CU	47.8	STS	58.5
4.위생배관	CU	58.6	CU	40.3	CU	32.5			CU	35.2	STS	45.8
5.위생기구설치
6.오배수공사
7.닥트공사
8.보온공사
9.자동제어
10.소화장비
11.옥내소화	ST	37.9	ST	64.5	ST	12.2			ST	28.5	ST	54.3
12.스프링쿨러
13.배연설비
14.특수소화
15.연도
16.가스설비
17.주방기구
18.실험실배관							STS	65.2
19.우수배관
20.중온수배관
21.특수설비
23.정화조
24.TAB
계		49.8		44.5		31.1		58.8		41.5		60

#첨부4

기계설비공사 공정별 상세 간소화율
구 분	00대학병원			00도로출입국			00초․중등 학교			00실험동			00전자현미경			00우체국
공정별	변경전	변경후	간소화율 (%)	변경전	변경후	간소화율 (%)	변경전	변경후	간소화율 (%)	변경전	변경후	간소화율 (%)	변경전	변경후	간소화율 (%)	변경전	변경후	간소화율 (%)
1.장비설치	379	340	10	58	48	17	79	74	6	45	38	16	35	29	17	320	268	16
2.기계실배관	620	314	49	228	65	72	320	94	71	250	77	69	110	48	56	629	220	65
3.공조난방	672	282	58	260	55	79	472	107	77				98	42	57	684	285	58
4.위생배관	477	185	61	158	63	60	227	114	50				65	30	54	479	268	44
5.위생기구설치	11	11	0	3	3	0	4	4	0				6	6	0	10	10	0
6.오배수공사	677	190	72	170	48	72	277	63	77				102	45	56	680	327	52
7.닥트공사	850	204	76	145	52	64	210	86	59				45	21	53	754	385	49
8.보온공사	150	60	60	75	24	68	111	52	53				58	23	60	245	93	62
9.자동제어	340	142	58	86	35	59							65	44	32	320	154	52
10.소화장비	15	15	0	5	5	0							4	4	0	14	14	0
11.옥내소화	359	72	80	65	26	60							46	24	48	328	112	66
12.스프링쿨러	75	45	40	60	24	60										68	22	68
13.배연설비	86	30	65													65	24	63
14.특수소화
15.연도	165	59	64	54	12	77	65	13	80							150	38	75
16.가스설비	377	189	50	35	14	60	277	87	69
17.주방기구	12	12	0				4	4	0
18.실험실배관										150	65	57
19.우수배관																43	20	53
20.중온수배관
21.특수설비										411	225	45
23.정화조
24.TAB	85	85	0													80	80	0
계	5,350	2,235	58	1,402	450	68	2,046	698	66	856	405	53	634	316	51	4,869	2,320	52

#부록5 프로젝트별 표준화 내역서 작성(○○대학병원) - CD로 제출

#부록6 시뮬레이션 자료(변경 전, 변경 후) - CD로 제출

#부록7 건축공사 내역서 표준서식 ․동해설 번역서 - CD로 제출

#부록8 공공건축공사내역서 표준서식(설비공사편)․동해설 번역서 - CD로 제출

□ 연구 참여자 명단

소 속	성 명
조달청	건축과장 안호협, 사무관 이보영, 서상락
	설비과장 한성부, 사무관 김중곤, 오원택
(사)한국구매조달학회	원장 추욱호, 과장 이원희
연구자	유성연, 이제묘, 박준택, 류윤수
전문가 자문단	수요기관 : 서울시(최중선 팀장, 신기채 팀장), 교육부(이연생 사무관), 한국전력 (정진철 과장), 한국수자원공사( 이재선 과장), 한국건설기술연구원(이유섭 수석 연구원) 설계자 : 정림건축(김환기 이사), (주)구성E& E(박수영 부사장) 적산업체 : (주)현대적산ENG (정동철 대표), (주)경원건축(김기원 이사), (주)대신적산(장세윤 소장) 시공사 : LG건설(주)(한명훈 부장, 하정환 부장, 장성규 과장), 대우건설(주)(김홍성 소장, 백인수 차장), (주)정림기연( 현원준 이사), (주)광장설비(황갑주 대표) 협회 : 대한건설협회(최재균 부장), 대한설비건설협회(황영환 부장)